(kicad_symbol_lib (version 20210619) (generator kicad_symbol_editor)
  (symbol "New_Library:NE555" (in_bom yes) (on_board yes)
    (property "Reference" "U?" (id 0) (at 0 13.9996 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "NE555" (id 1) (at 0 11.2245 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/ne555.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "timer" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Precision Timers, DIP-8/SOIC-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TSSOP*3x3mm*P0.65mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "NE555_0_0"
      (pin power_in line (at -3.175 -10.16 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "NE555_0_1"
      (rectangle (start -8.89 -7.62) (end 8.89 7.62)
        (stroke (width 0.254)) (fill (type background))
      )
      (rectangle (start -8.89 -7.62) (end 8.89 7.62)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "NE555_1_1"
      (pin input line (at -12.7 5.08 0) (length 3.81)
        (name "TR" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 3.81)
        (name "Q" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at 5.08 10.16 270) (length 3.81)
        (name "R" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 3.81 -11.43 90) (length 3.81)
        (name "CV" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 3.81)
        (name "THR" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 0 0) (length 3.81)
        (name "DIS" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
