<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="45.085" y2="0" width="0" layer="20"/>
<wire x1="45.085" y1="0" x2="45.085" y2="32.385" width="0" layer="20"/>
<wire x1="45.085" y1="32.385" x2="0" y2="32.385" width="0" layer="20"/>
<wire x1="0" y1="32.385" x2="0" y2="0" width="0" layer="20"/>
<text>Touch</text>
<text>ACT</text>
<text>On</text>
<text>Low</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>sjm4306</text>
<text>VacPen v1.0</text>
<text>010422</text>
<text>JLCJLCJLCJLC</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="140CLH-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, High temperature 140 CLH&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3">
<description>&lt;h3&gt;Plated Through Hole - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_LOCK">
<description>&lt;h3&gt;Plated Through Hole - Locking Footprint&lt;/h3&gt;
Holes are staggered by 0.005" from center to hold pins while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
<description>SOT23-3</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-003</description>
</package>
</packages>
</library>
<library name="SparkFun-IC-Microcontroller">
<description>&lt;h3&gt;SparkFun Microcontrollers&lt;/h3&gt;
This library contains microcontrollers.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO14">
<description>SOIC, 0.15 inch width</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MELF-MLL41">
<description>&lt;b&gt;DIODE&lt;/b&gt;&lt;p&gt;
Package DO-213AB = http://www.diotec.com/pdf/sm4001.pdf</description>
</package>
</packages>
</library>
<library name="sjm4306_LOGO">
<packages>
<package name="SJM4306_LOGO_MEDIUM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="adafruit" package="C0603" value="0.1uF">
<attribute name="VALUE"/>
</element>
<element name="ICSP" library="SparkFun-Connectors" package="2X3" value="ICSP">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-09701"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="600mA/40V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="R1" library="adafruit" package="M0805" value="10K">
<attribute name="VALUE"/>
</element>
<element name="IC1" library="linear" package="TO252" value="7805DT">
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="140CLH-0810" value="100uF">
<attribute name="VALUE"/>
</element>
<element name="BATTERY" library="SparkFun-Connectors" package="1X02_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PUMP" library="SparkFun-Connectors" package="1X02_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="M0805" value="1K">
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT23-3" value="600mA/40V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="LED1" library="adafruit" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="M0805" value="1K">
<attribute name="VALUE"/>
</element>
<element name="SWITCH" library="SparkFun-Connectors" package="1X02_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-IC-Microcontroller" package="SO14" value="ATTINY84">
<attribute name="PROD_ID" value="IC-11285"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="M0805" value="1K">
<attribute name="VALUE"/>
</element>
<element name="R5" library="adafruit" package="M0805" value="10K">
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="M0805" value="10K">
<attribute name="VALUE"/>
</element>
<element name="Q3" library="SparkFun-DiscreteSemi" package="SOT23-3" value="600mA/40V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="VALVE" library="SparkFun-Connectors" package="1X02_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="adafruit" package="M0805" value="1K">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="adafruit" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R8" library="adafruit" package="M0805" value="1K">
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="MELF-MLL41" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="diode" package="MELF-MLL41" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="adafruit" package="C0603" value="0.1uF">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="sjm4306_LOGO" package="SJM4306_LOGO_MEDIUM" value=""/>
<element name="U$3" library="sjm4306_LOGO" package="SJM4306_LOGO_MEDIUM" value=""/>
<element name="PSWITCH" library="SparkFun-Connectors" package="1X02_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="ICSP" pad="6"/>
<contactref element="C1" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="BATTERY" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="C2" pad="-"/>
<contactref element="LED1" pad="K"/>
<contactref element="SWITCH" pad="2"/>
<contactref element="U$1" pad="14"/>
<contactref element="LED2" pad="K"/>
<contactref element="R6" pad="1"/>
<contactref element="Q3" pad="2"/>
<contactref element="LED3" pad="K"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="ICSP" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="PUMP" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="U$1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="VALVE" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="RST">
<contactref element="ICSP" pad="5"/>
<contactref element="U$1" pad="4"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="ICSP" pad="4"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="MISO">
<contactref element="ICSP" pad="1"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="SCK">
<contactref element="ICSP" pad="3"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="N$1">
<contactref element="PUMP" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="Q2" pad="3"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="Q1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="V_BATT">
<contactref element="C2" pad="+"/>
<contactref element="IC1" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="PSWITCH" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="LED">
<contactref element="R3" pad="1"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="SW">
<contactref element="SWITCH" pad="1"/>
<contactref element="U$1" pad="10"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="VB">
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="TOUCH">
<contactref element="U$1" pad="12"/>
</signal>
<signal name="PUMP">
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="11"/>
</signal>
<signal name="N$5">
<contactref element="VALVE" pad="2"/>
<contactref element="Q3" pad="3"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$7">
<contactref element="Q3" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="VALVE">
<contactref element="R7" pad="1"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="R8" pad="2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="LED1">
<contactref element="R4" pad="1"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="LED2">
<contactref element="R8" pad="1"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="N$8">
<contactref element="PSWITCH" pad="1"/>
<contactref element="BATTERY" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
