<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="30" y1="5" x2="30" y2="23.25" width="0.127" layer="20"/>
<wire x1="28" y1="25.25" x2="2.25" y2="25.25" width="0.127" layer="20"/>
<wire x1="2.25" y1="25.25" x2="0.25" y2="23.25" width="0.127" layer="20"/>
<wire x1="0.25" y1="23.25" x2="0.25" y2="5" width="0.127" layer="20"/>
<hole x="2.75" y="22.75" drill="2.3"/>
<text>BACK</text>
<text>mdeeds</text>
<text>2022</text>
<text>IN</text>
<text>VCC</text>
<text>OUT</text>
<text>GND</text>
<wire x1="2.25" y1="3" x2="28" y2="3" width="0.127" layer="20"/>
<wire x1="28" y1="3" x2="30" y2="5" width="0.127" layer="20"/>
<wire x1="28" y1="25.25" x2="30" y2="23.25" width="0.127" layer="20"/>
<wire x1="2.25" y1="3" x2="0.25" y2="5" width="0.127" layer="20"/>
<hole x="27.5" y="5.5" drill="2.3"/>
<text>NEO-SEG-14</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>14</text>
</plain>
<libraries>
<library name="SK6812B4020">
<packages>
<package name="SK6812B4020">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_SMD_RA_FEMALE">
<description>&lt;h3&gt;SMD - 4 Pin Right-Angle Female Header&lt;/h3&gt;
Silk outline shows header location. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="SK6812B4020" package="SK6812B4020" value="SK6812B4020"/>
<element name="U$2" library="SK6812B4020" package="SK6812B4020" value="SK6812B4020"/>
<element name="U$3" library="SK6812B4020" package="SK6812B4020" value="SK6812B4020"/>
<element name="U$4" library="SK6812B4020" package="SK6812B4020" value="SK6812B4020"/>
<element name="U$5" library="SK6812B4020" package="SK6812B4020" value="SK6812B4020"/>
<element name="U$6" library="SK6812B4020" package="SK6812B4020" value="SK6812B4020"/>
<element name="U$7" library="SK6812B4020" package="SK6812B4020" value="SK6812B4020"/>
<element name="U$8" library="SK6812B4020" package="SK6812B4020" value="SK6812B4020"/>
<element name="U$9" library="SK6812B4020" package="SK6812B4020" value="SK6812B4020"/>
<element name="U$10" library="SK6812B4020" package="SK6812B4020" value="SK6812B4020"/>
<element name="U$11" library="SK6812B4020" package="SK6812B4020" value="SK6812B4020"/>
<element name="U$12" library="SK6812B4020" package="SK6812B4020" value="SK6812B4020"/>
<element name="U$13" library="SK6812B4020" package="SK6812B4020" value="SK6812B4020"/>
<element name="U$14" library="SK6812B4020" package="SK6812B4020" value="SK6812B4020"/>
<element name="J2" library="SparkFun-Connectors" package="1X04_SMD_RA_FEMALE" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-12382"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="3.3V">
<contactref element="U$1" pad="P$3"/>
<contactref element="U$2" pad="P$3"/>
<contactref element="U$3" pad="P$3"/>
<contactref element="U$4" pad="P$3"/>
<contactref element="U$5" pad="P$3"/>
<contactref element="U$6" pad="P$3"/>
<contactref element="U$7" pad="P$3"/>
<contactref element="U$8" pad="P$3"/>
<contactref element="U$9" pad="P$3"/>
<contactref element="U$10" pad="P$3"/>
<contactref element="U$11" pad="P$3"/>
<contactref element="U$12" pad="P$3"/>
<contactref element="U$13" pad="P$3"/>
<contactref element="U$14" pad="P$3"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="P$5"/>
<contactref element="U$2" pad="P$5"/>
<contactref element="U$3" pad="P$5"/>
<contactref element="U$4" pad="P$5"/>
<contactref element="U$5" pad="P$5"/>
<contactref element="U$6" pad="P$5"/>
<contactref element="U$7" pad="P$5"/>
<contactref element="U$8" pad="P$5"/>
<contactref element="U$9" pad="P$5"/>
<contactref element="U$10" pad="P$5"/>
<contactref element="U$11" pad="P$5"/>
<contactref element="U$12" pad="P$5"/>
<contactref element="U$13" pad="P$5"/>
<contactref element="U$14" pad="P$5"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="DIN">
<contactref element="U$1" pad="P$2"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="P$4"/>
<contactref element="U$2" pad="P$2"/>
</signal>
<signal name="N$4">
<contactref element="U$2" pad="P$4"/>
<contactref element="U$3" pad="P$2"/>
</signal>
<signal name="N$5">
<contactref element="U$3" pad="P$4"/>
<contactref element="U$4" pad="P$2"/>
</signal>
<signal name="N$6">
<contactref element="U$4" pad="P$4"/>
<contactref element="U$5" pad="P$2"/>
</signal>
<signal name="N$7">
<contactref element="U$5" pad="P$4"/>
<contactref element="U$6" pad="P$2"/>
</signal>
<signal name="N$8">
<contactref element="U$6" pad="P$4"/>
<contactref element="U$7" pad="P$2"/>
</signal>
<signal name="DOUT">
<contactref element="U$14" pad="P$4"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$8" pad="P$4"/>
<contactref element="U$9" pad="P$2"/>
</signal>
<signal name="N$2">
<contactref element="U$9" pad="P$4"/>
<contactref element="U$10" pad="P$2"/>
</signal>
<signal name="N$9">
<contactref element="U$10" pad="P$4"/>
<contactref element="U$11" pad="P$2"/>
</signal>
<signal name="N$10">
<contactref element="U$11" pad="P$4"/>
<contactref element="U$12" pad="P$2"/>
</signal>
<signal name="N$11">
<contactref element="U$12" pad="P$4"/>
<contactref element="U$13" pad="P$2"/>
</signal>
<signal name="N$12">
<contactref element="U$13" pad="P$4"/>
<contactref element="U$14" pad="P$2"/>
</signal>
<signal name="N$13">
<contactref element="U$7" pad="P$4"/>
<contactref element="U$8" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
