<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<wire x1="4.75" y1="4.5" x2="4.75" y2="36.25" width="0.0762" layer="20"/>
<wire x1="5.75" y1="37.25" x2="23.75" y2="37.25" width="0.0762" layer="20"/>
<wire x1="24.75" y1="36.25" x2="24.75" y2="4.5" width="0.0762" layer="20"/>
<wire x1="20.75" y1="0.5" x2="8.75" y2="0.5" width="0.0762" layer="20"/>
<wire x1="8.75" y1="0.5" x2="4.75" y2="4.5" width="0.0762" layer="20"/>
<wire x1="20.75" y1="0.5" x2="24.75" y2="4.5" width="0.0762" layer="20"/>
<text>mdeeds</text>
<text>v1 2021</text>
<wire x1="5.75" y1="37.25" x2="4.75" y2="36.25" width="0.0762" layer="20"/>
<wire x1="23.75" y1="37.25" x2="24.75" y2="36.25" width="0.0762" layer="20"/>
</plain>
<libraries>
<library name="AMS1117-3.3">
<packages>
<package name="SOT229P700X180-4N">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
<description>&lt;B&gt;LED 0603 SMT&lt;/B&gt;&lt;p&gt;
0603, surface mount.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.075inch &lt;/li&gt;
&lt;li&gt;Area: 0.06" x 0.03"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED - BLUE&lt;/li&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_SMD_4.6X2.8MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 4.6 x 2.8mm&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.ck-components.com/media/1479/kmr2.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="1-1734028-1">
<packages>
<package name="TE_1-1734028-1">
</package>
</packages>
</library>
<library name="SamacSys_Parts">
<description>&lt;b&gt;https://componentsearchengine.com&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="ESP32S2WROVERM22S2H3216PH3Q0">
<description>&lt;b&gt;ESP32-S2-WROVER(M22S2H3216PH3Q0)-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="TL9320AF400QG">
<packages>
<package name="TL9320AF400QG">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U3" library="AMS1117-3.3" package="SOT229P700X180-4N" value="AMS1117-3.3">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" LDO Voltage Regulators 800MA LDO LINEAR REG "/>
<attribute name="MF" value="AMD"/>
<attribute name="MP" value="AMS1117-3.3"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-0603" value="RED">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-00819"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0603" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11015"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0603" value="22uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11015"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11015"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED-0603" value="BLUE">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-08575"/>
<attribute name="VALUE"/>
</element>
<element name="RESET" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_4.6X2.8MM" value="MOMENTARY-SWITCH-SPST-SMD-4.6X2.8MM">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-13065"/>
</element>
<element name="BOOT" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_4.6X2.8MM" value="MOMENTARY-SWITCH-SPST-SMD-4.6X2.8MM">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-13065"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="1-1734028-1" package="TE_1-1734028-1" value="1-1734028-1">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="CENTERLINE_PITCH" value="2 mm[.078 in]"/>
<attribute name="COMMENT" value="1-1734028-1"/>
<attribute name="DESCRIPTION" value=" Conn USB 2.0 Type A PL 4 POS Solder RA SMD 4 Terminal 1 Port T/R "/>
<attribute name="MF" value="TE Connectivity"/>
<attribute name="MP" value="1-1734028-1"/>
<attribute name="NUMBER_OF_POSITIONS" value="4"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="PRODUCT_TYPE" value="Connector"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/1-1734028-1/?ref=eda"/>
</element>
<element name="IC1" library="SamacSys_Parts" package="ESP32S2WROVERM22S2H3216PH3Q0" value="ESP32-S2-WROVER_M22S2H3216PH3Q">
<attribute name="DESCRIPTION" value="WiFi Modules (802.11) Module ESP32-S2 WROVER PCB ANT"/>
<attribute name="HEIGHT" value="3.45mm"/>
<attribute name="MANUFACTURER_NAME" value="Espressif Systems"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ESP32-S2-WROVER(M22S2H3216PH3Q0)"/>
<attribute name="MOUSER_PART_NUMBER" value="356-ESP32S2WRV3216PH"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Espressif-Systems/ESP32-S2-WROVERM22S2H3216PH3Q0?qs=vHuUswq2%252BswhBPbltcIS8Q%3D%3D"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="TL9320AF400QG" package="TL9320AF400QG" value="TL9320AF400QG"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C3" pad="2"/>
<contactref element="U3" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="BOOT" pad="4"/>
<contactref element="BOOT" pad="3"/>
<contactref element="RESET" pad="4"/>
<contactref element="RESET" pad="3"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="J2" pad="4"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="26"/>
<contactref element="IC1" pad="51"/>
<contactref element="IC1" pad="42"/>
<contactref element="IC1" pad="43"/>
<contactref element="IC1" pad="44"/>
<contactref element="IC1" pad="45"/>
<contactref element="IC1" pad="46"/>
<contactref element="IC1" pad="47"/>
<contactref element="IC1" pad="48"/>
<contactref element="IC1" pad="49"/>
<contactref element="IC1" pad="50"/>
<contactref element="C7" pad="2"/>
<contactref element="U$1" pad="P$2"/>
</signal>
<signal name="5V">
<contactref element="U3" pad="3"/>
<contactref element="C3" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="ESP_EN">
<contactref element="RESET" pad="1"/>
<contactref element="RESET" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="IC1" pad="41"/>
<contactref element="R6" pad="2"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="U3" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="2"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="USB_D+">
<contactref element="J2" pad="3"/>
<contactref element="IC1" pad="23"/>
</signal>
<signal name="USB_D-">
<contactref element="J2" pad="2"/>
<contactref element="IC1" pad="22"/>
</signal>
<signal name="LED1">
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="24"/>
</signal>
<signal name="IO0">
<contactref element="BOOT" pad="1"/>
<contactref element="BOOT" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="SHIELD">
<contactref element="J2" pad="S1"/>
<contactref element="J2" pad="S2"/>
</signal>
<signal name="ESP_RX">
<contactref element="IC1" pad="38"/>
</signal>
<signal name="ESP_TX">
<contactref element="IC1" pad="37"/>
</signal>
<signal name="N$3">
<contactref element="R5" pad="2"/>
<contactref element="IC1" pad="21"/>
</signal>
<signal name="IO1">
<contactref element="IC1" pad="4"/>
</signal>
<signal name="IO2">
<contactref element="IC1" pad="5"/>
</signal>
<signal name="IO3">
<contactref element="IC1" pad="6"/>
</signal>
<signal name="IO4">
<contactref element="IC1" pad="7"/>
</signal>
<signal name="IO5">
<contactref element="IC1" pad="8"/>
</signal>
<signal name="IO6">
<contactref element="IC1" pad="9"/>
</signal>
<signal name="IO7">
<contactref element="IC1" pad="10"/>
</signal>
<signal name="IO8">
<contactref element="IC1" pad="11"/>
</signal>
<signal name="IO9">
<contactref element="IC1" pad="12"/>
</signal>
<signal name="IO10">
<contactref element="IC1" pad="13"/>
</signal>
<signal name="IO11">
<contactref element="IC1" pad="14"/>
</signal>
<signal name="IO12">
<contactref element="IC1" pad="15"/>
</signal>
<signal name="IO13">
<contactref element="IC1" pad="16"/>
</signal>
<signal name="IO14">
<contactref element="IC1" pad="17"/>
</signal>
<signal name="IO15">
<contactref element="IC1" pad="18"/>
</signal>
<signal name="IO16">
<contactref element="IC1" pad="19"/>
</signal>
<signal name="IO17">
<contactref element="IC1" pad="20"/>
</signal>
<signal name="IO18">
<contactref element="IC1" pad="27"/>
</signal>
<signal name="IO19">
<contactref element="IC1" pad="28"/>
</signal>
<signal name="IO20">
<contactref element="IC1" pad="29"/>
</signal>
<signal name="LED2">
<contactref element="IC1" pad="34"/>
</signal>
<signal name="BTN1">
<contactref element="IC1" pad="35"/>
<contactref element="U$1" pad="P$1"/>
</signal>
<signal name="BTN2">
<contactref element="IC1" pad="36"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
