<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="3.5" y1="0" x2="56.5" y2="0" width="0" layer="20"/>
<wire x1="60" y1="3.5" x2="60" y2="76.5" width="0" layer="20"/>
<wire x1="56.5" y1="80" x2="3.5" y2="80" width="0" layer="20"/>
<wire x1="0" y1="76.5" x2="0" y2="3.5" width="0" layer="20"/>
<wire x1="3.5" y1="52.5" x2="16.5" y2="52.5" width="0.1524" layer="20"/>
<wire x1="16.5" y1="52.5" x2="16.5" y2="55" width="0.1524" layer="20"/>
<wire x1="16.5" y1="55" x2="3.5" y2="55" width="0.1524" layer="20"/>
<wire x1="3.5" y1="55" x2="3.5" y2="52.5" width="0.1524" layer="20"/>
<wire x1="23.5" y1="52.5" x2="36.5" y2="52.5" width="0.1524" layer="20"/>
<wire x1="36.5" y1="52.5" x2="36.5" y2="55" width="0.1524" layer="20"/>
<wire x1="36.5" y1="55" x2="23.5" y2="55" width="0.1524" layer="20"/>
<wire x1="23.5" y1="55" x2="23.5" y2="52.5" width="0.1524" layer="20"/>
<wire x1="43.5" y1="52.5" x2="56.5" y2="52.5" width="0.1524" layer="20"/>
<wire x1="56.5" y1="52.5" x2="56.5" y2="55" width="0.1524" layer="20"/>
<wire x1="56.5" y1="55" x2="43.5" y2="55" width="0.1524" layer="20"/>
<wire x1="43.5" y1="55" x2="43.5" y2="52.5" width="0.1524" layer="20"/>
<wire x1="3.5" y1="34" x2="16.5" y2="34" width="0.1524" layer="20"/>
<wire x1="16.5" y1="34" x2="16.5" y2="36.5" width="0.1524" layer="20"/>
<wire x1="16.5" y1="36.5" x2="3.5" y2="36.5" width="0.1524" layer="20"/>
<wire x1="3.5" y1="36.5" x2="3.5" y2="34" width="0.1524" layer="20"/>
<wire x1="23.5" y1="34" x2="36.5" y2="34" width="0.1524" layer="20"/>
<wire x1="36.5" y1="34" x2="36.5" y2="36.5" width="0.1524" layer="20"/>
<wire x1="36.5" y1="36.5" x2="23.5" y2="36.5" width="0.1524" layer="20"/>
<wire x1="23.5" y1="36.5" x2="23.5" y2="34" width="0.1524" layer="20"/>
<wire x1="43.5" y1="34" x2="56.5" y2="34" width="0.1524" layer="20"/>
<wire x1="56.5" y1="34" x2="56.5" y2="36.5" width="0.1524" layer="20"/>
<wire x1="56.5" y1="36.5" x2="43.5" y2="36.5" width="0.1524" layer="20"/>
<wire x1="43.5" y1="36.5" x2="43.5" y2="34" width="0.1524" layer="20"/>
<wire x1="3.5" y1="15.5" x2="16.5" y2="15.5" width="0.1524" layer="20"/>
<wire x1="16.5" y1="15.5" x2="16.5" y2="18" width="0.1524" layer="20"/>
<wire x1="16.5" y1="18" x2="3.5" y2="18" width="0.1524" layer="20"/>
<wire x1="3.5" y1="18" x2="3.5" y2="15.5" width="0.1524" layer="20"/>
<wire x1="23.5" y1="15.5" x2="36.5" y2="15.5" width="0.1524" layer="20"/>
<wire x1="36.5" y1="15.5" x2="36.5" y2="18" width="0.1524" layer="20"/>
<wire x1="36.5" y1="18" x2="23.5" y2="18" width="0.1524" layer="20"/>
<wire x1="23.5" y1="18" x2="23.5" y2="15.5" width="0.1524" layer="20"/>
<wire x1="43.5" y1="15.5" x2="56.5" y2="15.5" width="0.1524" layer="20"/>
<wire x1="56.5" y1="15.5" x2="56.5" y2="18" width="0.1524" layer="20"/>
<wire x1="56.5" y1="18" x2="43.5" y2="18" width="0.1524" layer="20"/>
<wire x1="43.5" y1="18" x2="43.5" y2="15.5" width="0.1524" layer="20"/>
<hole x="20" y="20.5" drill="3.2"/>
<hole x="40" y="20.5" drill="3.2"/>
<hole x="40" y="49" drill="3.2"/>
<hole x="20" y="49" drill="3.2"/>
<wire x1="60" y1="3.5" x2="56.5" y2="0" width="0.0762" layer="20" curve="-90"/>
<wire x1="3.5" y1="0" x2="0" y2="3.5" width="0.0762" layer="20" curve="-90"/>
<wire x1="56.5" y1="80" x2="60" y2="76.5" width="0.1524" layer="20" curve="-90"/>
<wire x1="0" y1="76.5" x2="3.5" y2="80" width="0.1524" layer="20" curve="-90"/>
<text>CREE-BOARD</text>
<text>v1</text>
<text>mdeeds</text>
<text>2022</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
</plain>
<libraries>
<library name="TAJA106K016SNJ">
<packages>
<package name="CAPMP3216X180N">
<description>&lt;b&gt;TANTALUM CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
<description>&lt;B&gt;LED 0603 SMT&lt;/B&gt;&lt;p&gt;
0603, surface mount.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.075inch &lt;/li&gt;
&lt;li&gt;Area: 0.06" x 0.03"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED - BLUE&lt;/li&gt;</description>
</package>
</packages>
</library>
<library name="694106301002">
<packages>
<package name="694106301002">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled (6.4)</description>
</package>
</packages>
</library>
<library name="USB-B-S-X-X-TH">
<packages>
<package name="SAMTEC_USB-B-S-X-X-TH">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_SMD_6.0X3.5MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 6.0 x 3.5 mm&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/1101.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="ESP32-C3-WROOM-02-H4">
<packages>
<package name="MODULE_ESP32-C3-WROOM-02-H4">
</package>
</packages>
</library>
<library name="AMS1117-3.3">
<packages>
<package name="SOT229P700X180-4N">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="DMN2005K-7">
<packages>
<package name="SOT95P240X120-3N">
</package>
</packages>
</library>
<library name="switch_bandw">
<packages>
<package name="SWITCH_BANDW">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M_COPPER">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Medium - Top Copper&lt;/h3&gt;
&lt;p&gt;Exposed copper logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="TAJA106K016SNJ" package="CAPMP3216X180N" value="TAJA106K016SNJ">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" 10 µF Molded Tantalum Capacitors 16 V 1206 (3216 Metric) 3Ohm "/>
<attribute name="MF" value="AVX"/>
<attribute name="MP" value="TAJA106K016SNJ"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="1206 AVX"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/TAJA106K016SNJ/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="TAJA106K016SNJ" package="CAPMP3216X180N" value="TAJA106K016SNJ">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" 10 µF Molded Tantalum Capacitors 16 V 1206 (3216 Metric) 3Ohm "/>
<attribute name="MF" value="AVX"/>
<attribute name="MP" value="TAJA106K016SNJ"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="1206 AVX"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/TAJA106K016SNJ/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0603" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11015"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11015"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0603" value="1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11015"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED-0603" value="RED">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-00819"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="694106301002" package="694106301002" value="694106301002">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" Power Barrel Connector Jack 2.10mm ID (0.083), 5.50mm OD (0.217) Through Hole, Right Angle "/>
<attribute name="MF" value="Wurth Elektronik"/>
<attribute name="MP" value="694106301002"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/694106301002/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="USB-B-S-X-X-TH" package="SAMTEC_USB-B-S-X-X-TH" value="USB-B-S-X-X-TH">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" USB-B Series USB 2.0 Interface, Type B "/>
<attribute name="MF" value="Samtec"/>
<attribute name="MP" value="USB-B-S-S-B-TH-TR"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/USB-B-S-S-B-TH-TR/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="S3" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_6.0X3.5MM" value="MOMENTARY-SWITCH-SPST-SMD-6.0X3.5MM">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-00815"/>
<attribute name="SF_SKU" value="COM-08229"/>
</element>
<element name="S4" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_6.0X3.5MM" value="MOMENTARY-SWITCH-SPST-SMD-6.0X3.5MM">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-00815"/>
<attribute name="SF_SKU" value="COM-08229"/>
</element>
<element name="U1" library="ESP32-C3-WROOM-02-H4" package="MODULE_ESP32-C3-WROOM-02-H4" value="ESP32-C3-WROOM-02-H4">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" WiFi Modules (802.11) (Engineering Samples) SMD module, ESP32-C3, 4MB SPI flash, PCB antenna, -40 C +105 C "/>
<attribute name="MF" value="Espressif Systems"/>
<attribute name="MP" value="ESP32-C3-WROOM-02-H4"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="VFQFN-32 Espressif Systems"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/ESP32-C3-WROOM-02-H4/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="AMS1117-3.3" package="SOT229P700X180-4N" value="AMS1117-3.3">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" LDO Voltage Regulators 800MA LDO LINEAR REG "/>
<attribute name="MF" value="AMD"/>
<attribute name="MP" value="AMS1117-3.3"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-0603" value="RED">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-00819"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="J12" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q10" library="DMN2005K-7" package="SOT95P240X120-3N" value="DMN2005K-7">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" N-Channel 20 V 300mA (Ta) 350mW (Ta) Surface Mount SOT-23-3 "/>
<attribute name="MF" value="Diodes Inc."/>
<attribute name="MP" value="DMN2005K-7"/>
<attribute name="PACKAGE" value="SOT-23 Diodes Inc."/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/DMN2005K-7/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="CREE_LED" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="SparkFun-Resistors" package="AXIAL-0.3" value="1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-12182"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="TAJA106K016SNJ" package="CAPMP3216X180N" value="TAJA106K016SNJ">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" 10 µF Molded Tantalum Capacitors 16 V 1206 (3216 Metric) 3Ohm "/>
<attribute name="MF" value="AVX"/>
<attribute name="MP" value="TAJA106K016SNJ"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="1206 AVX"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/TAJA106K016SNJ/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="switch_bandw" package="SWITCH_BANDW" value="SWITCH_BANDW"/>
<element name="Q1" library="DMN2005K-7" package="SOT95P240X120-3N" value="DMN2005K-7">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" N-Channel 20 V 300mA (Ta) 350mW (Ta) Surface Mount SOT-23-3 "/>
<attribute name="MF" value="Diodes Inc."/>
<attribute name="MP" value="DMN2005K-7"/>
<attribute name="PACKAGE" value="SOT-23 Diodes Inc."/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/DMN2005K-7/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="CREE_LED1" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="switch_bandw" package="SWITCH_BANDW" value="SWITCH_BANDW"/>
<element name="Q2" library="DMN2005K-7" package="SOT95P240X120-3N" value="DMN2005K-7">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" N-Channel 20 V 300mA (Ta) 350mW (Ta) Surface Mount SOT-23-3 "/>
<attribute name="MF" value="Diodes Inc."/>
<attribute name="MP" value="DMN2005K-7"/>
<attribute name="PACKAGE" value="SOT-23 Diodes Inc."/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/DMN2005K-7/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="CREE_LED2" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="switch_bandw" package="SWITCH_BANDW" value="SWITCH_BANDW"/>
<element name="Q3" library="DMN2005K-7" package="SOT95P240X120-3N" value="DMN2005K-7">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" N-Channel 20 V 300mA (Ta) 350mW (Ta) Surface Mount SOT-23-3 "/>
<attribute name="MF" value="Diodes Inc."/>
<attribute name="MP" value="DMN2005K-7"/>
<attribute name="PACKAGE" value="SOT-23 Diodes Inc."/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/DMN2005K-7/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="CREE_LED3" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="switch_bandw" package="SWITCH_BANDW" value="SWITCH_BANDW"/>
<element name="Q4" library="DMN2005K-7" package="SOT95P240X120-3N" value="DMN2005K-7">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" N-Channel 20 V 300mA (Ta) 350mW (Ta) Surface Mount SOT-23-3 "/>
<attribute name="MF" value="Diodes Inc."/>
<attribute name="MP" value="DMN2005K-7"/>
<attribute name="PACKAGE" value="SOT-23 Diodes Inc."/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/DMN2005K-7/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="CREE_LED4" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="U$5" library="switch_bandw" package="SWITCH_BANDW" value="SWITCH_BANDW"/>
<element name="Q5" library="DMN2005K-7" package="SOT95P240X120-3N" value="DMN2005K-7">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" N-Channel 20 V 300mA (Ta) 350mW (Ta) Surface Mount SOT-23-3 "/>
<attribute name="MF" value="Diodes Inc."/>
<attribute name="MP" value="DMN2005K-7"/>
<attribute name="PACKAGE" value="SOT-23 Diodes Inc."/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/DMN2005K-7/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="CREE_LED5" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="U$6" library="switch_bandw" package="SWITCH_BANDW" value="SWITCH_BANDW"/>
<element name="Q6" library="DMN2005K-7" package="SOT95P240X120-3N" value="DMN2005K-7">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" N-Channel 20 V 300mA (Ta) 350mW (Ta) Surface Mount SOT-23-3 "/>
<attribute name="MF" value="Diodes Inc."/>
<attribute name="MP" value="DMN2005K-7"/>
<attribute name="PACKAGE" value="SOT-23 Diodes Inc."/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/DMN2005K-7/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="CREE_LED6" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="U$7" library="switch_bandw" package="SWITCH_BANDW" value="SWITCH_BANDW"/>
<element name="Q7" library="DMN2005K-7" package="SOT95P240X120-3N" value="DMN2005K-7">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" N-Channel 20 V 300mA (Ta) 350mW (Ta) Surface Mount SOT-23-3 "/>
<attribute name="MF" value="Diodes Inc."/>
<attribute name="MP" value="DMN2005K-7"/>
<attribute name="PACKAGE" value="SOT-23 Diodes Inc."/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/DMN2005K-7/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="CREE_LED7" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="U$8" library="switch_bandw" package="SWITCH_BANDW" value="SWITCH_BANDW"/>
<element name="Q8" library="DMN2005K-7" package="SOT95P240X120-3N" value="DMN2005K-7">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" N-Channel 20 V 300mA (Ta) 350mW (Ta) Surface Mount SOT-23-3 "/>
<attribute name="MF" value="Diodes Inc."/>
<attribute name="MP" value="DMN2005K-7"/>
<attribute name="PACKAGE" value="SOT-23 Diodes Inc."/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/DMN2005K-7/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="CREE_LED8" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="U$9" library="switch_bandw" package="SWITCH_BANDW" value="SWITCH_BANDW"/>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M_COPPER" value="OSHW-LOGOM-COPPER"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="R25" pad="P$2"/>
<contactref element="CREE_LED" pad="2"/>
<contactref element="CREE_LED1" pad="2"/>
<contactref element="CREE_LED2" pad="2"/>
<contactref element="CREE_LED3" pad="2"/>
<contactref element="CREE_LED4" pad="2"/>
<contactref element="CREE_LED5" pad="2"/>
<contactref element="CREE_LED6" pad="2"/>
<contactref element="CREE_LED7" pad="2"/>
<contactref element="CREE_LED8" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="U3" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="3"/>
<contactref element="R2" pad="2"/>
<contactref element="J4" pad="4"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U1" pad="9"/>
<contactref element="U1" pad="19"/>
<contactref element="U1" pad="20"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="22"/>
<contactref element="U1" pad="23"/>
<contactref element="U1" pad="24"/>
<contactref element="U1" pad="25"/>
<contactref element="U1" pad="26"/>
<contactref element="U1" pad="27"/>
<contactref element="U1" pad="28"/>
<contactref element="U1" pad="29"/>
<contactref element="U1" pad="30"/>
<contactref element="U1" pad="31"/>
<contactref element="U1" pad="32"/>
<contactref element="U1" pad="33"/>
<contactref element="U1" pad="34"/>
<contactref element="U1" pad="35"/>
<contactref element="U1" pad="36"/>
<contactref element="U1" pad="37"/>
<contactref element="U1" pad="38"/>
<contactref element="U1" pad="39"/>
<contactref element="C5" pad="2"/>
<contactref element="S4" pad="2"/>
<contactref element="S3" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="J12" pad="1"/>
<contactref element="Q10" pad="2"/>
<contactref element="R26" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="Q3" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="Q4" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="Q5" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="Q6" pad="2"/>
<contactref element="R12" pad="1"/>
<contactref element="Q7" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="Q8" pad="2"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="U3" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="J12" pad="3"/>
<contactref element="C6" pad="1"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="U$2" pad="P$1"/>
<contactref element="U$3" pad="P$1"/>
<contactref element="U$4" pad="P$1"/>
<contactref element="U$5" pad="P$1"/>
<contactref element="U$6" pad="P$1"/>
<contactref element="U$7" pad="P$1"/>
<contactref element="U$8" pad="P$1"/>
<contactref element="U$9" pad="P$1"/>
</signal>
<signal name="VIN">
<contactref element="C1" pad="1"/>
<contactref element="U3" pad="3"/>
<contactref element="J1" pad="1"/>
<contactref element="R25" pad="P$1"/>
</signal>
<signal name="ESP_EN">
<contactref element="U1" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="S3" pad="1"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="USB_D-">
<contactref element="J4" pad="2"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="USB_D+">
<contactref element="J4" pad="3"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="N$1">
<contactref element="D2" pad="C"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="IO9">
<contactref element="U1" pad="8"/>
<contactref element="R4" pad="1"/>
<contactref element="S4" pad="1"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="IO8">
<contactref element="U1" pad="7"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="IO10">
<contactref element="U1" pad="10"/>
<contactref element="U$8" pad="P$4"/>
<contactref element="R13" pad="2"/>
<contactref element="Q7" pad="1"/>
</signal>
<signal name="IO0">
<contactref element="U1" pad="18"/>
<contactref element="R26" pad="2"/>
<contactref element="Q10" pad="1"/>
<contactref element="U$1" pad="P$4"/>
</signal>
<signal name="IO2">
<contactref element="U1" pad="16"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="IO3">
<contactref element="U1" pad="15"/>
<contactref element="U$3" pad="P$4"/>
<contactref element="R8" pad="2"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="IO4">
<contactref element="U1" pad="3"/>
<contactref element="U$4" pad="P$4"/>
<contactref element="R9" pad="2"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="IO5">
<contactref element="U1" pad="4"/>
<contactref element="U$5" pad="P$4"/>
<contactref element="R10" pad="2"/>
<contactref element="Q4" pad="1"/>
</signal>
<signal name="IO6">
<contactref element="U1" pad="5"/>
<contactref element="U$6" pad="P$4"/>
<contactref element="R11" pad="2"/>
<contactref element="Q5" pad="1"/>
</signal>
<signal name="IO7">
<contactref element="U1" pad="6"/>
<contactref element="U$7" pad="P$4"/>
<contactref element="R12" pad="2"/>
<contactref element="Q6" pad="1"/>
</signal>
<signal name="IO1">
<contactref element="U1" pad="17"/>
<contactref element="U$2" pad="P$4"/>
<contactref element="R6" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="D1" pad="C"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="IO21">
<contactref element="U1" pad="12"/>
<contactref element="J12" pad="2"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="IO20">
<contactref element="U1" pad="11"/>
<contactref element="U$9" pad="P$4"/>
<contactref element="R14" pad="2"/>
<contactref element="Q8" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="CREE_LED" pad="1"/>
<contactref element="Q10" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="CREE_LED1" pad="1"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="CREE_LED2" pad="1"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="CREE_LED3" pad="1"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="CREE_LED4" pad="1"/>
<contactref element="Q4" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="CREE_LED5" pad="1"/>
<contactref element="Q5" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="CREE_LED6" pad="1"/>
<contactref element="Q6" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="CREE_LED7" pad="1"/>
<contactref element="Q7" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="CREE_LED8" pad="1"/>
<contactref element="Q8" pad="3"/>
</signal>
<signal name="USB_VCC">
<contactref element="J4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
