Altium Designer Pick and Place Locations
K:\Work\ELLO LC\LC1\electronics\project outputs\Pick Place for ELLO_LC1_PCB.txt

========================================================================================================================
File Design Information:

Date:       27/01/23
Time:       20:26
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment          Layer       Footprint                       Center-X(mm) Center-Y(mm) Rotation Description                                           
C6         1u               BottomLayer CIH_0603                        59.2500      -46.3500     180      Capacitor                                             
C5         1u               BottomLayer CIH_0603                        56.2500      -46.3500     180      Capacitor                                             
C4         1u               BottomLayer CIH_0603                        53.2500      -46.3500     180      Capacitor                                             
C3         1u               BottomLayer CIH_0603                        50.2500      -46.3500     180      Capacitor                                             
C2         1u               BottomLayer CIH_0603                        47.2500      -46.3500     180      Capacitor                                             
C1         1u               BottomLayer CIH_0603                        44.2500      -46.3500     180      Capacitor                                             
DSP1       "EA DOGM204N-A"  TopLayer    DOGM204N-A_(in-PCB)             72.2500      -22.6000     180      "Ultra-thin FSTN 20x4 characters display"             
SW1        EVQ-PUJ02K       BottomLayer EVQPUx02K                       31.2500      -3.0000      0        "Switch, Momentary, Normal Open"                      
U1         PIC18F47Q83-I/PT TopLayer    QFP80P1200X1200X120-44_(IN-PCB) 24.0000      -37.0000     270      "Flash Microcontrollers with nanoWatt XLP Technology" 
