<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<text>Please focus on the direction of battery,
if you reversely connecting the battery, 
the charging circuit will be damaged,
so please pay attention to it when
you mounting the battery.</text>
<text>LIGHT</text>
<text>USB
POWER
Charger
module</text>
<text>+5V</text>
<text>GND</text>
<text>+BAT</text>
<text>GND</text>
<text>GND</text>
<text>+inUSB</text>
<text>USB-C</text>
<text>POWER</text>
<wire x1="8.255" y1="5.08" x2="100.965" y2="5.08" width="0" layer="20"/>
<wire x1="100.965" y1="5.08" x2="103.505" y2="7.62" width="0" layer="20" curve="90"/>
<wire x1="103.505" y1="7.62" x2="103.505" y2="87.63" width="0" layer="20"/>
<wire x1="103.505" y1="87.63" x2="100.965" y2="90.17" width="0" layer="20" curve="90"/>
<wire x1="100.965" y1="90.17" x2="8.255" y2="90.17" width="0" layer="20"/>
<wire x1="8.255" y1="90.17" x2="5.715" y2="87.63" width="0" layer="20" curve="90"/>
<wire x1="5.715" y1="87.63" x2="5.715" y2="7.62" width="0" layer="20"/>
<wire x1="5.715" y1="7.62" x2="8.255" y2="5.08" width="0" layer="20" curve="90"/>
<circle x="51.435" y="63.5" radius="22.89525" width="0.002540625" layer="20"/>
<text>FAN</text>
<text>GND</text>
<text>GND</text>
<text>+BAT</text>
<text>+BAT</text>
<text>GND</text>
<text>+5V</text>
<text>+5V</text>
<text>GND</text>
</plain>
<libraries>
<library name="microbuilder">
<packages>
<package name="USB_C_CUSB31-CFM2AX-01-X">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3">
<description>&lt;h3&gt;Plated Through Hole - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - Long Pads without Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Batteries">
<description>&lt;h3&gt;SparkFun Batteries&lt;/h3&gt;
This library contains battery clips, connectors, and appropriately sized silk outlines for LiPo batteries. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="18650_HOLDER_SINGLE_THROUGH-HOLE">
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-A-S-NOSILK-FEMALE">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH-SIDEEZ">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP20SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J9" library="SparkFun-Connectors" package="2X3" value="FEMALE 2x3">
<attribute name="PROD_ID" value="CONN-11566"/>
</element>
<element name="BT3" library="Batteries" package="18650_HOLDER_SINGLE_THROUGH-HOLE" value=""/>
<element name="USB-C_POWER_ONLY" library="microbuilder" package="USB_C_CUSB31-CFM2AX-01-X" value="">
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X06_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X02_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="USBIN1" library="SparkFun" package="USB-A-S-NOSILK-FEMALE" value="USB-A-SMD"/>
<element name="J3" library="SparkFun-Connectors" package="1X02_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="2X3" value="FEMALE 2x3">
<attribute name="PROD_ID" value="CONN-11566"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X02_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="S5" library="SparkFun-Electromechanical" package="TACTILE-PTH-SIDEEZ" value="SWITCH-MOMENTARY-2SIDE_EZ"/>
<element name="PWRON" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X02_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$4">
</signal>
<signal name="N$164">
</signal>
<signal name="VCC1">
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$9">
</signal>
<signal name="N$10">
</signal>
<signal name="N$11">
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="N$14">
</signal>
<signal name="N$15">
</signal>
<signal name="N$56">
</signal>
<signal name="N$19">
</signal>
<signal name="N$20">
</signal>
<signal name="VBUS">
<contactref element="USB-C_POWER_ONLY" pad="A4B9"/>
<contactref element="USB-C_POWER_ONLY" pad="B4A9"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="GND">
<contactref element="USB-C_POWER_ONLY" pad="B1A12"/>
<contactref element="USB-C_POWER_ONLY" pad="A1B12"/>
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="5"/>
<contactref element="USBIN1" pad="GND"/>
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="1"/>
<contactref element="J5" pad="2"/>
<contactref element="S5" pad="2"/>
<contactref element="J6" pad="1"/>
<contactref element="BT3" pad="CON(-)"/>
</signal>
<signal name="+5V">
<contactref element="J1" pad="1"/>
<contactref element="USBIN1" pad="VBUS"/>
<contactref element="J3" pad="2"/>
<contactref element="J6" pad="2"/>
<contactref element="J4" pad="4"/>
<contactref element="J4" pad="2"/>
<contactref element="J4" pad="3"/>
<contactref element="J4" pad="1"/>
<contactref element="J9" pad="4"/>
<contactref element="J9" pad="2"/>
<contactref element="J9" pad="3"/>
<contactref element="J9" pad="1"/>
</signal>
<signal name="N$16">
</signal>
<signal name="N$17">
</signal>
<signal name="N$18">
</signal>
<signal name="N$5">
</signal>
<signal name="N$7">
<contactref element="J9" pad="5"/>
<contactref element="J9" pad="6"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="J4" pad="5"/>
<contactref element="J4" pad="6"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="BAT">
<contactref element="J1" pad="3"/>
<contactref element="BT3" pad="CON(+)"/>
</signal>
<signal name="N$6">
<contactref element="PWRON" pad="TP"/>
<contactref element="S5" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
