<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<text>(Bobricius)</text>
<text>GND</text>
<text>MOSI</text>
<text>MISO</text>
<text>SCK</text>
<text>CS</text>
<text>My DIY
Long
uCard</text>
<text>VCC</text>
<text>Name:</text>
<text>XTSD0xG</text>
<text>JLCJLCJLCJLC</text>
<wire x1="15.4305" y1="1.2065" x2="15.4305" y2="5.7785" width="0" layer="20"/>
<wire x1="15.4305" y1="5.7785" x2="16.5735" y2="6.7945" width="0" layer="20"/>
<wire x1="16.5735" y1="6.7945" x2="16.5735" y2="8.3185" width="0" layer="20"/>
<wire x1="16.5735" y1="8.3185" x2="16.0655" y2="8.3185" width="0" layer="20"/>
<wire x1="16.0655" y1="8.3185" x2="16.0655" y2="9.8425" width="0" layer="20"/>
<wire x1="16.0655" y1="9.8425" x2="16.5735" y2="10.3505" width="0" layer="20"/>
<wire x1="5.7785" y1="1.2065" x2="6.2865" y2="0.6985" width="0" layer="20" curve="90"/>
<wire x1="6.2865" y1="0.6985" x2="14.9225" y2="0.6985" width="0" layer="20"/>
<wire x1="14.9225" y1="0.6985" x2="15.4305" y2="1.2065" width="0" layer="20" curve="90"/>
<wire x1="5.7785" y1="1.2065" x2="5.7785" y2="15.494" width="0" layer="20"/>
<wire x1="5.7785" y1="15.494" x2="4.7625" y2="16.51" width="0" layer="20" curve="90"/>
<wire x1="4.7625" y1="16.51" x2="-1.27" y2="16.51" width="0" layer="20"/>
<wire x1="-1.27" y1="16.51" x2="-1.905" y2="17.145" width="0" layer="20" curve="-90"/>
<wire x1="-1.905" y1="17.145" x2="-1.905" y2="35.56" width="0" layer="20"/>
<wire x1="16.5735" y1="10.3505" x2="16.5735" y2="35.306" width="0" layer="20"/>
<wire x1="16.5735" y1="35.306" x2="14.605" y2="37.1475" width="0" layer="20" curve="101.345967"/>
<wire x1="14.605" y1="37.1475" x2="-0.3175" y2="37.1475" width="0" layer="20"/>
<wire x1="-0.3175" y1="37.1475" x2="-1.905" y2="35.56" width="0" layer="20" curve="90"/>
<text>BOBRICIUS</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="MICRO-SDCARD">
</package>
</packages>
</library>
<library name="microbuilder">
<packages>
<package name="LGA8_8X6">
<description>&lt;b&gt;Small Outline IC - 150mil Wide&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rc-master-smd">
<packages>
<package name="C0603">
<description>&lt;b&gt;SMD CHIP CAP&lt;/b&gt; - 0603</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun" package="MICRO-SDCARD" value="MICRO-SDCARD"/>
<element name="C1" library="rc-master-smd" package="C0603" value="100n"/>
<element name="U2" library="microbuilder" package="LGA8_8X6" value="XTSD"/>
<element name="J1" library="SparkFun-Connectors" package="1X06_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="GND"/>
<contactref element="C1" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="VCC"/>
<contactref element="C1" pad="1"/>
<contactref element="U2" pad="8"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="DAT0"/>
<contactref element="U2" pad="6"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="CMD"/>
<contactref element="U2" pad="5"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="CLK"/>
<contactref element="U2" pad="3"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="CS">
<contactref element="U1" pad="CD/DAT3"/>
<contactref element="U2" pad="2"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
