<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="1.5" y1="0.25" x2="25.5" y2="0.25" width="0" layer="20"/>
<wire x1="25.5" y1="0.25" x2="25.5" y2="17.25" width="0" layer="20"/>
<wire x1="25.5" y1="17.25" x2="1.5" y2="17.25" width="0" layer="20"/>
<wire x1="1.5" y1="17.25" x2="1.5" y2="0.25" width="0" layer="20"/>
<text>mdeeds
2023</text>
<text>cups</text>
<text>v1</text>
<text>12v</text>
<text>BATT</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA3216">
<description>Generic EIA 3216 (1206) polarized tantalum capacitor</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - Long Pads with Locking Footprint&lt;/h3&gt;
Pins are staggered by 0.005" from center to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SI7463DP">
<packages>
<package name="TRANS_SI7463DP">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="LTC4416EMS_PBF">
<packages>
<package name="MSOP-10_MS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00811"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X02_LOCK_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SI7463DP" package="TRANS_SI7463DP" value="SI7463DP">
<attribute name="AVAILABILITY" value="Not in stock"/>
<attribute name="DESCRIPTION" value=" P-Channel 40 V 11A (Ta) 1.9W (Ta) Surface Mount PowerPAK® SO-8 "/>
<attribute name="MF" value="Vishay"/>
<attribute name="MP" value="SI7463DP"/>
<attribute name="PACKAGE" value="SO-8 Vishay"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="Q2" library="SI7463DP" package="TRANS_SI7463DP" value="SI7463DP">
<attribute name="AVAILABILITY" value="Not in stock"/>
<attribute name="DESCRIPTION" value=" P-Channel 40 V 11A (Ta) 1.9W (Ta) Surface Mount PowerPAK® SO-8 "/>
<attribute name="MF" value="Vishay"/>
<attribute name="MP" value="SI7463DP"/>
<attribute name="PACKAGE" value="SO-8 Vishay"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="Q3" library="SI7463DP" package="TRANS_SI7463DP" value="SI7463DP">
<attribute name="AVAILABILITY" value="Not in stock"/>
<attribute name="DESCRIPTION" value=" P-Channel 40 V 11A (Ta) 1.9W (Ta) Surface Mount PowerPAK® SO-8 "/>
<attribute name="MF" value="Vishay"/>
<attribute name="MP" value="SI7463DP"/>
<attribute name="PACKAGE" value="SO-8 Vishay"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="Q4" library="SI7463DP" package="TRANS_SI7463DP" value="SI7463DP">
<attribute name="AVAILABILITY" value="Not in stock"/>
<attribute name="DESCRIPTION" value=" P-Channel 40 V 11A (Ta) 1.9W (Ta) Surface Mount PowerPAK® SO-8 "/>
<attribute name="MF" value="Vishay"/>
<attribute name="MP" value="SI7463DP"/>
<attribute name="PACKAGE" value="SO-8 Vishay"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603" value="2.2k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="LTC4416EMS_PBF" package="MSOP-10_MS" value="LTC4416EMS#PBF">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" OR Controller Source Selector Switch P-Channel 2:1 10-MSOP "/>
<attribute name="MF" value="Analog Devices"/>
<attribute name="MP" value="LTC4416EMS#PBF"/>
<attribute name="PACKAGE" value="MSOP-10 Analog Devices"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search?q=LTC4416EMS#PBF&amp;ref=eda"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X02_LOCK_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X02_LOCK_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="Q1" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="Q2" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="Q3" pad="1"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q3" pad="3"/>
<contactref element="Q4" pad="1"/>
<contactref element="Q4" pad="2"/>
<contactref element="Q4" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="Q3" pad="4"/>
<contactref element="Q4" pad="4"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="10"/>
<contactref element="Q1" pad="4"/>
<contactref element="Q2" pad="4"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="-"/>
<contactref element="J1" pad="2"/>
<contactref element="U1" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="12V">
<contactref element="Q1" pad="5"/>
<contactref element="Q1" pad="6"/>
<contactref element="Q1" pad="7"/>
<contactref element="Q1" pad="8"/>
<contactref element="Q1" pad="9"/>
<contactref element="U1" pad="9"/>
<contactref element="R1" pad="2"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="V_BATT">
<contactref element="U1" pad="7"/>
<contactref element="Q3" pad="5"/>
<contactref element="Q3" pad="6"/>
<contactref element="Q3" pad="7"/>
<contactref element="Q3" pad="8"/>
<contactref element="Q3" pad="9"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="8"/>
<contactref element="Q4" pad="5"/>
<contactref element="Q4" pad="6"/>
<contactref element="Q4" pad="7"/>
<contactref element="Q4" pad="8"/>
<contactref element="Q4" pad="9"/>
<contactref element="Q2" pad="5"/>
<contactref element="Q2" pad="6"/>
<contactref element="Q2" pad="7"/>
<contactref element="Q2" pad="8"/>
<contactref element="Q2" pad="9"/>
<contactref element="C1" pad="+"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
