(kicad_sch (version 20230121) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Connector:Conn_01x01_Pin" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at 0 2.54 0))
      (property "Value" "Conn_01x01_Pin" (at 0 -2.54 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_locked" "" (at 0 0 0))
      (property "ki_keywords" "connector" (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x01, script generated" (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (at 0 0 0))
      (symbol "Conn_01x01_Pin_1_1"
        (polyline
          (pts
            (xy 1.27 0)
            (xy 0.8636 0)
          )
          (fill (type none))
        )
        (rectangle (start 0.8636 0.127) (end 0 -0.127)
          (fill (type outline))
        )
        (pin passive line (at 5.08 0 180) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
      )
    )
    (symbol "Connector:Conn_01x02_Pin" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at 0 2.54 0))
      (property "Value" "Conn_01x02_Pin" (at 0 -5.08 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_locked" "" (at 0 0 0))
      (property "ki_keywords" "connector" (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x02, script generated" (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (at 0 0 0))
      (symbol "Conn_01x02_Pin_1_1"
        (polyline
          (pts
            (xy 1.27 -2.54)
            (xy 0.8636 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy 0.8636 0)
          )
          (fill (type none))
        )
        (rectangle (start 0.8636 -2.413) (end 0 -2.667)
          (fill (type outline))
        )
        (rectangle (start 0.8636 0.127) (end 0 -0.127)
          (fill (type outline))
        )
        (pin passive line (at 5.08 0 180) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 5.08 -2.54 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (at 0.635 2.54 0))
      (property "Value" "C" (at 0.635 -2.54 0))
      (property "Footprint" "" (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (at 0 0 0))
      (property "ki_fp_filters" "C_*" (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:LED" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (at 0 2.54 0))
      (property "Value" "LED" (at 0 -2.54 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "LED diode" (at 0 0 0))
      (property "ki_description" "Light emitting diode" (at 0 0 0))
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (at 0 0 0))
      (symbol "LED_0_1"
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy -1.27 0)
            (xy 1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.048 -0.762)
            (xy -4.572 -2.286)
            (xy -3.81 -2.286)
            (xy -4.572 -2.286)
            (xy -4.572 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 -0.762)
            (xy -3.302 -2.286)
            (xy -2.54 -2.286)
            (xy -3.302 -2.286)
            (xy -3.302 -1.524)
          )
          (fill (type none))
        )
      )
      (symbol "LED_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (at 2.032 0 90))
      (property "Value" "R" (at 0 0 90))
      (property "Footprint" "" (at -1.778 0 90))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "R res resistor" (at 0 0 0))
      (property "ki_description" "Resistor" (at 0 0 0))
      (property "ki_fp_filters" "R_*" (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "easyeda2kicad:2001SMT-2P_C132500" (in_bom yes) (on_board yes)
      (property "Reference" "CN" (at 0 11.43 0))
      (property "Value" "2001SMT-2P_C132500" (at 0 -11.43 0))
      (property "Footprint" "easyeda2kicad:CONN-SMD_2001SMT-2P-WT" (at 0 -13.97 0))
      (property "Datasheet" "https://lcsc.com/product-detail/PH-Connectors_Shenzhen-Cancome-2001series-socket-1-2P-2mm_C132500.html" (at 0 -16.51 0))
      (property "LCSC Part" "C132500" (at 0 -19.05 0))
      (symbol "2001SMT-2P_C132500_0_1"
        (rectangle (start -3.81 3.81) (end 6.35 -3.81)
          (fill (type background))
        )
        (circle (center -2.54 2.54) (radius 0.38)
          (fill (type none))
        )
        (pin unspecified line (at -6.35 1.27 0) (length 2.54)
          (name "1")
          (number "1")
        )
        (pin unspecified line (at -6.35 -1.27 0) (length 2.54)
          (name "2")
          (number "2")
        )
        (pin unspecified line (at 3.81 -6.35 90) (length 2.54)
          (name "3")
          (number "3")
        )
        (pin unspecified line (at 3.81 6.35 270) (length 2.54)
          (name "4")
          (number "4")
        )
      )
    )
    (symbol "easyeda2kicad:AO3401A_C347476" (in_bom yes) (on_board yes)
      (property "Reference" "Q" (at 0 10.16 0))
      (property "Value" "AO3401A_C347476" (at 0 -10.16 0))
      (property "Footprint" "easyeda2kicad:SOT-23_L2.9-W1.3-P1.90-LS2.4-BR" (at 0 -12.7 0))
      (property "Datasheet" "https://lcsc.com/product-detail/Others_Youtai-Semiconductor-Co-Ltd-AO3401A-4-1A_C347476.html" (at 0 -15.24 0))
      (property "LCSC Part" "C347476" (at 0 -17.78 0))
      (symbol "AO3401A_C347476_0_1"
        (polyline
          (pts
            (xy -3.05 2.29)
            (xy -3.05 -2.29)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -2.29)
            (xy -2.54 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -0.51)
            (xy -2.54 0.51)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 1.27)
            (xy -2.54 2.29)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -1.78)
            (xy -2.54 -1.78)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.78)
            (xy -2.54 1.78)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 0)
            (xy 0 0)
            (xy 0 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -2.54)
            (xy 2.54 -2.54)
            (xy 2.54 -0.51)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy -1.52 0.51)
            (xy -1.52 -0.51)
            (xy 0 0)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 1.78)
            (xy 0 2.54)
            (xy 2.54 2.54)
            (xy 2.54 0.76)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -0.51)
            (xy 3.3 0.76)
            (xy 1.78 0.76)
            (xy 2.54 -0.51)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy 3.3 -0.51)
            (xy 3.05 -0.51)
            (xy 2.03 -0.51)
            (xy 1.78 -0.51)
          )
          (fill (type none))
        )
        (pin unspecified line (at -5.08 0 0) (length 2.032)
          (name "G")
          (number "1")
        )
        (pin unspecified line (at 0 -5.08 90) (length 2.54)
          (name "S")
          (number "2")
        )
        (pin unspecified line (at 0 5.08 270) (length 2.54)
          (name "D")
          (number "3")
        )
      )
    )
    (symbol "easyeda2kicad:CA45-B-16V-22UF-M" (in_bom yes) (on_board yes)
      (property "Reference" "C" (at 0 5.08 0))
      (property "Value" "CA45-B-16V-22UF-M" (at 0 -5.08 0))
      (property "Footprint" "easyeda2kicad:CAP-SMD_L3.5-W2.8-R-RD" (at 0 -7.62 0))
      (property "Datasheet" "https://lcsc.com/product-detail/Tantalum-Capacitors_22uF-226-20-16V_C140371.html" (at 0 -10.16 0))
      (property "LCSC Part" "C140371" (at 0 -12.7 0))
      (symbol "CA45-B-16V-22UF-M_0_1"
        (polyline
          (pts
            (xy -0.51 -2.03)
            (xy -0.51 2.03)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.51 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.51 -2.03)
            (xy 0.51 2.03)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy 0.51 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.03 -1.52)
            (xy 2.03 -0.51)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -1.02)
            (xy 1.52 -1.02)
          )
          (fill (type none))
        )
        (pin input line (at 3.81 0 180) (length 2.54)
          (name "1")
          (number "1")
        )
        (pin input line (at -3.81 0 0) (length 2.54)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "easyeda2kicad:CN3063" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 8.89 0))
      (property "Value" "CN3063" (at 0 -13.97 0))
      (property "Footprint" "easyeda2kicad:SOIC-8_L4.9-W3.9-P1.27-LS6.0-BL-EP3.3-1" (at 0 -16.51 0))
      (property "Datasheet" "https://lcsc.com/product-detail/PMIC-AC-DC-Converters_CN3063_C28078.html" (at 0 -19.05 0))
      (property "LCSC Part" "C28078" (at 0 -21.59 0))
      (symbol "CN3063_0_1"
        (rectangle (start -8.89 6.35) (end 8.89 -6.35)
          (fill (type background))
        )
        (circle (center -7.62 5.08) (radius 0.38)
          (fill (type none))
        )
        (pin unspecified line (at -11.43 3.81 0) (length 2.54)
          (name "TEMP")
          (number "1")
        )
        (pin unspecified line (at -11.43 1.27 0) (length 2.54)
          (name "ISET")
          (number "2")
        )
        (pin unspecified line (at -11.43 -1.27 0) (length 2.54)
          (name "GND")
          (number "3")
        )
        (pin unspecified line (at -11.43 -3.81 0) (length 2.54)
          (name "VIN")
          (number "4")
        )
        (pin unspecified line (at 11.43 -3.81 180) (length 2.54)
          (name "BAT")
          (number "5")
        )
        (pin unspecified line (at 11.43 -1.27 180) (length 2.54)
          (name "DONE")
          (number "6")
        )
        (pin unspecified line (at 11.43 1.27 180) (length 2.54)
          (name "CHRG")
          (number "7")
        )
        (pin unspecified line (at 11.43 3.81 180) (length 2.54)
          (name "FB")
          (number "8")
        )
        (pin unspecified line (at 0 -8.89 90) (length 2.54)
          (name "EP")
          (number "9")
        )
      )
    )
    (symbol "easyeda2kicad:DB301V-5.0-2P" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 5.08 0))
      (property "Value" "DB301V-5.0-2P" (at 0 -7.62 0))
      (property "Footprint" "easyeda2kicad:CONN-TH_2P-P5.00_L7.6-W10.0" (at 0 -10.16 0))
      (property "Datasheet" "https://lcsc.com/product-detail/Screw-terminal_DIBO-DB301V-5-0-2P_C395882.html" (at 0 -12.7 0))
      (property "LCSC Part" "C395882" (at 0 -15.24 0))
      (symbol "DB301V-5.0-2P_0_1"
        (rectangle (start -2.54 2.54) (end 2.54 -5.08)
          (fill (type background))
        )
        (circle (center -1.27 1.27) (radius 0.38)
          (fill (type none))
        )
        (pin unspecified line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1")
        )
        (pin unspecified line (at -5.08 -2.54 0) (length 2.54)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "easyeda2kicad:PSPNAQ4030-1R5M" (in_bom yes) (on_board yes)
      (property "Reference" "L" (at 0 5.08 0))
      (property "Value" "PSPNAQ4030-1R5M" (at 0 -5.08 0))
      (property "Footprint" "easyeda2kicad:IND-SMD_L4.0-W4.0" (at 0 -7.62 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "LCSC Part" "C436670" (at 0 -10.16 0))
      (symbol "PSPNAQ4030-1R5M_0_1"
        (arc (start -2.03 0.01) (mid -3.055 1.013) (end -4.06 -0.01)
          (fill (type none))
        )
        (arc (start 0 0.01) (mid -1.025 1.013) (end -2.03 -0.01)
          (fill (type none))
        )
        (arc (start 2.03 0.01) (mid 1.005 1.013) (end 0 -0.01)
          (fill (type none))
        )
        (arc (start 4.06 0.01) (mid 3.035 1.013) (end 2.03 -0.01)
          (fill (type none))
        )
        (pin unspecified line (at -5.08 0 0) (length 1.016)
          (name "1")
          (number "1")
        )
        (pin unspecified line (at 5.08 0 180) (length 1.016)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "easyeda2kicad:SS14" (in_bom yes) (on_board yes)
      (property "Reference" "D" (at 0 5.08 0))
      (property "Value" "SS14" (at 0 -5.08 0))
      (property "Footprint" "easyeda2kicad:SMA_L4.2-W2.6-LS5.3-RD" (at 0 -7.62 0))
      (property "Datasheet" "https://lcsc.com/product-detail/Schottky-Barrier-Diodes-SBD_SS14_C2480.html" (at 0 -10.16 0))
      (property "LCSC Part" "C2480" (at 0 -12.7 0))
      (symbol "SS14_0_1"
        (polyline
          (pts
            (xy 1.27 1.52)
            (xy -1.27 0)
            (xy 1.27 -1.78)
            (xy 1.27 1.52)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -2.03 1.52)
            (xy -2.03 1.78)
            (xy -1.52 1.78)
            (xy -1.52 -2.03)
            (xy -1.02 -2.03)
            (xy -1.02 -1.78)
          )
          (fill (type none))
        )
        (pin unspecified line (at -5.08 0 0) (length 3.81)
          (name "K")
          (number "1")
        )
        (pin unspecified line (at 5.08 0 180) (length 3.81)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "easyeda2kicad:TPS63020DSJR" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 15.24 0))
      (property "Value" "TPS63020DSJR" (at 0 -17.78 0))
      (property "Footprint" "easyeda2kicad:VSON-14_L4.0-W3.0-P0.50-BL-EP_TI_DSJ" (at 0 -20.32 0))
      (property "Datasheet" "https://lcsc.com/product-detail/DC-DC-Converters_TI_TPS63020DSJR_TPS63020DSJR_C15483.html" (at 0 -22.86 0))
      (property "LCSC Part" "C15483" (at 0 -25.4 0))
      (symbol "TPS63020DSJR_0_1"
        (rectangle (start -10.16 12.7) (end 10.16 -7.62)
          (fill (type background))
        )
        (pin unspecified line (at -15.24 10.16 0) (length 5.08)
          (name "VINA")
          (number "1")
        )
        (pin unspecified line (at 15.24 0 180) (length 5.08)
          (name "VIN")
          (number "10")
        )
        (pin unspecified line (at 15.24 2.54 180) (length 5.08)
          (name "VIN")
          (number "11")
        )
        (pin unspecified line (at 15.24 5.08 180) (length 5.08)
          (name "EN")
          (number "12")
        )
        (pin unspecified line (at 15.24 7.62 180) (length 5.08)
          (name "PS/SYNC")
          (number "13")
        )
        (pin unspecified line (at 15.24 10.16 180) (length 5.08)
          (name "PG")
          (number "14")
        )
        (pin unspecified line (at 0 -12.7 90) (length 5.08)
          (name "PGND")
          (number "15")
        )
        (pin unspecified line (at -15.24 7.62 0) (length 5.08)
          (name "GND")
          (number "2")
        )
        (pin unspecified line (at -15.24 5.08 0) (length 5.08)
          (name "FB")
          (number "3")
        )
        (pin unspecified line (at -15.24 2.54 0) (length 5.08)
          (name "VOUT")
          (number "4")
        )
        (pin unspecified line (at -15.24 0 0) (length 5.08)
          (name "VOUT")
          (number "5")
        )
        (pin unspecified line (at -15.24 -2.54 0) (length 5.08)
          (name "L2")
          (number "6")
        )
        (pin unspecified line (at -15.24 -5.08 0) (length 5.08)
          (name "L2")
          (number "7")
        )
        (pin unspecified line (at 15.24 -5.08 180) (length 5.08)
          (name "L1")
          (number "8")
        )
        (pin unspecified line (at 15.24 -2.54 180) (length 5.08)
          (name "L1")
          (number "9")
        )
      )
    )
    (symbol "easyeda2kicad:TYPE-C-31-M-12" (in_bom yes) (on_board yes)
      (property "Reference" "USBC" (at 0 26.67 0))
      (property "Value" "TYPE-C-31-M-12" (at 0 -26.67 0))
      (property "Footprint" "easyeda2kicad:USB-C_SMD-TYPE-C-31-M-12" (at 0 -29.21 0))
      (property "Datasheet" "https://lcsc.com/product-detail/USB-Type-C_Korean-Hroparts-Elec-TYPE-C-31-M-12_C165948.html" (at 0 -31.75 0))
      (property "LCSC Part" "C165948" (at 0 -34.29 0))
      (symbol "TYPE-C-31-M-12_0_1"
        (rectangle (start -8.89 16.51) (end 8.89 -16.51)
          (fill (type background))
        )
        (circle (center -7.62 15.24) (radius 0.38)
          (fill (type none))
        )
        (pin unspecified line (at -1.27 -21.59 90) (length 5.08)
          (name "SH")
          (number "0")
        )
        (pin unspecified line (at -1.27 21.59 270) (length 5.08)
          (name "SH")
          (number "0")
        )
        (pin unspecified line (at 1.27 -21.59 90) (length 5.08)
          (name "SH")
          (number "0")
        )
        (pin unspecified line (at 1.27 21.59 270) (length 5.08)
          (name "SH")
          (number "0")
        )
        (pin unspecified line (at 11.43 -13.97 180) (length 2.54)
          (name "GND")
          (number "A1")
        )
        (pin unspecified line (at 11.43 13.97 180) (length 2.54)
          (name "GND")
          (number "A12")
        )
        (pin unspecified line (at 11.43 -6.35 180) (length 2.54)
          (name "VBUS")
          (number "A4")
        )
        (pin unspecified line (at 11.43 -3.81 180) (length 2.54)
          (name "CC1")
          (number "A5")
        )
        (pin unspecified line (at 11.43 -1.27 180) (length 2.54)
          (name "DP1")
          (number "A6")
        )
        (pin unspecified line (at 11.43 1.27 180) (length 2.54)
          (name "DN1")
          (number "A7")
        )
        (pin unspecified line (at 11.43 3.81 180) (length 2.54)
          (name "SBU1")
          (number "A8")
        )
        (pin unspecified line (at 11.43 6.35 180) (length 2.54)
          (name "VBUS")
          (number "A9")
        )
        (pin unspecified line (at -11.43 13.97 0) (length 2.54)
          (name "GND")
          (number "B1")
        )
        (pin unspecified line (at -11.43 -13.97 0) (length 2.54)
          (name "GND")
          (number "B12")
        )
        (pin unspecified line (at -11.43 6.35 0) (length 2.54)
          (name "VBUS")
          (number "B4")
        )
        (pin unspecified line (at -11.43 3.81 0) (length 2.54)
          (name "CC2")
          (number "B5")
        )
        (pin unspecified line (at -11.43 1.27 0) (length 2.54)
          (name "DP2")
          (number "B6")
        )
        (pin unspecified line (at -11.43 -1.27 0) (length 2.54)
          (name "DN2")
          (number "B7")
        )
        (pin unspecified line (at -11.43 -3.81 0) (length 2.54)
          (name "SBU2")
          (number "B8")
        )
        (pin unspecified line (at -11.43 -6.35 0) (length 2.54)
          (name "VBUS")
          (number "B9")
        )
      )
    )
    (symbol "power:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -3.81 0))
      (property "Value" "+5V" (at 0 3.556 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (at 0 0 0))
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -6.35 0))
      (property "Value" "GND" (at 0 -3.81 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 50.8 76.2) (diameter 0) (color 0 0 0 0))
  (junction (at 49.53 29.21) (diameter 0) (color 0 0 0 0))
  (junction (at 105.41 113.03) (diameter 0) (color 0 0 0 0))
  (junction (at 123.19 31.75) (diameter 0) (color 0 0 0 0))
  (junction (at 180.34 58.42) (diameter 0) (color 0 0 0 0))
  (junction (at 48.26 76.2) (diameter 0) (color 0 0 0 0))
  (junction (at 123.19 50.8) (diameter 0) (color 0 0 0 0))
  (junction (at 54.61 133.35) (diameter 0) (color 0 0 0 0))
  (junction (at 22.86 45.72) (diameter 0) (color 0 0 0 0))
  (junction (at 55.88 125.73) (diameter 0) (color 0 0 0 0))
  (junction (at 30.48 125.73) (diameter 0) (color 0 0 0 0))
  (junction (at 105.41 123.19) (diameter 0) (color 0 0 0 0))
  (junction (at 129.54 113.03) (diameter 0) (color 0 0 0 0))
  (junction (at 177.8 114.3) (diameter 0) (color 0 0 0 0))
  (junction (at 123.19 25.4) (diameter 0) (color 0 0 0 0))
  (junction (at 49.53 76.2) (diameter 0) (color 0 0 0 0))
  (junction (at 135.89 50.8) (diameter 0) (color 0 0 0 0))
  (junction (at 175.26 30.48) (diameter 0) (color 0 0 0 0))
  (junction (at 93.98 127) (diameter 0) (color 0 0 0 0))
  (junction (at 93.98 133.35) (diameter 0) (color 0 0 0 0))
  (junction (at 74.93 45.72) (diameter 0) (color 0 0 0 0))
  (junction (at 40.64 125.73) (diameter 0) (color 0 0 0 0))
  (junction (at 139.7 113.03) (diameter 0) (color 0 0 0 0))
  (junction (at 119.38 113.03) (diameter 0) (color 0 0 0 0))
  (no_connect (at 264.16 34.29))
  (no_connect (at 38.1 48.26))
  (no_connect (at 149.86 45.72))
  (no_connect (at 264.16 21.59))
  (no_connect (at 38.1 53.34))
  (no_connect (at 60.96 55.88))
  (no_connect (at 38.1 55.88))
  (no_connect (at 60.96 53.34))
  (no_connect (at 60.96 48.26))
  (no_connect (at 60.96 50.8))
  (no_connect (at 38.1 50.8))
  (wire (pts (xy 30.48 137.16) (xy 30.48 140.97)))
  (wire (pts (xy 114.3 31.75) (xy 114.3 45.72)))
  (wire (pts (xy 123.19 25.4) (xy 123.19 31.75)))
  (wire (pts (xy 132.08 64.77) (xy 132.08 68.58)))
  (wire (pts (xy 123.19 21.59) (xy 123.19 25.4)))
  (wire (pts (xy 252.73 48.26) (xy 252.73 45.72)))
  (wire (pts (xy 54.61 154.94) (xy 69.85 154.94)))
  (wire (pts (xy 223.52 104.14) (xy 223.52 102.87)))
  (wire (pts (xy 74.93 58.42) (xy 74.93 45.72)))
  (wire (pts (xy 180.34 71.12) (xy 180.34 73.66)))
  (wire (pts (xy 106.68 50.8) (xy 109.22 50.8)))
  (wire (pts (xy 219.71 109.22) (xy 219.71 106.68)))
  (wire (pts (xy 80.01 154.94) (xy 93.98 154.94)))
  (wire (pts (xy 119.38 113.03) (xy 119.38 114.3)))
  (wire (pts (xy 129.54 121.92) (xy 129.54 124.46)))
  (wire (pts (xy 180.34 58.42) (xy 184.15 58.42)))
  (wire (pts (xy 177.8 110.49) (xy 177.8 114.3)))
  (wire (pts (xy 123.19 31.75) (xy 123.19 33.02)))
  (wire (pts (xy 170.18 53.34) (xy 161.29 53.34)))
  (wire (pts (xy 170.18 40.64) (xy 170.18 53.34)))
  (wire (pts (xy 119.38 113.03) (xy 129.54 113.03)))
  (wire (pts (xy 139.7 113.03) (xy 139.7 114.3)))
  (wire (pts (xy 93.98 128.27) (xy 90.17 128.27)))
  (wire (pts (xy 38.1 45.72) (xy 22.86 45.72)))
  (wire (pts (xy 90.17 118.11) (xy 95.25 118.11)))
  (wire (pts (xy 223.52 102.87) (xy 227.33 102.87)))
  (wire (pts (xy 180.34 58.42) (xy 180.34 63.5)))
  (wire (pts (xy 209.55 26.67) (xy 214.63 26.67)))
  (wire (pts (xy 137.16 58.42) (xy 138.43 58.42)))
  (wire (pts (xy 132.08 55.88) (xy 132.08 57.15)))
  (wire (pts (xy 177.8 124.46) (xy 177.8 129.54)))
  (wire (pts (xy 40.64 137.16) (xy 40.64 140.97)))
  (wire (pts (xy 57.15 118.11) (xy 59.69 118.11)))
  (wire (pts (xy 50.8 76.2) (xy 62.23 76.2)))
  (wire (pts (xy 49.53 29.21) (xy 50.8 29.21)))
  (wire (pts (xy 161.29 58.42) (xy 180.34 58.42)))
  (wire (pts (xy 254 43.18) (xy 257.81 43.18)))
  (wire (pts (xy 36.83 38.1) (xy 38.1 38.1)))
  (wire (pts (xy 104.14 38.1) (xy 104.14 41.91)))
  (wire (pts (xy 105.41 132.08) (xy 105.41 135.89)))
  (wire (pts (xy 62.23 66.04) (xy 60.96 66.04)))
  (wire (pts (xy 54.61 133.35) (xy 54.61 154.94)))
  (wire (pts (xy 90.17 123.19) (xy 105.41 123.19)))
  (wire (pts (xy 55.88 125.73) (xy 40.64 125.73)))
  (wire (pts (xy 93.98 127) (xy 95.25 127)))
  (wire (pts (xy 161.29 55.88) (xy 180.34 55.88)))
  (wire (pts (xy 36.83 66.04) (xy 36.83 76.2)))
  (wire (pts (xy 180.34 55.88) (xy 180.34 40.64)))
  (wire (pts (xy 119.38 50.8) (xy 123.19 50.8)))
  (wire (pts (xy 90.17 130.81) (xy 93.98 130.81)))
  (wire (pts (xy 22.86 58.42) (xy 38.1 58.42)))
  (wire (pts (xy 57.15 123.19) (xy 59.69 123.19)))
  (wire (pts (xy 105.41 113.03) (xy 105.41 114.3)))
  (wire (pts (xy 74.93 140.97) (xy 74.93 143.51)))
  (wire (pts (xy 139.7 113.03) (xy 149.86 113.03)))
  (wire (pts (xy 149.86 113.03) (xy 149.86 114.3)))
  (wire (pts (xy 30.48 125.73) (xy 40.64 125.73)))
  (wire (pts (xy 59.69 125.73) (xy 55.88 125.73)))
  (wire (pts (xy 105.41 123.19) (xy 105.41 124.46)))
  (wire (pts (xy 248.92 29.21) (xy 254 29.21)))
  (wire (pts (xy 50.8 29.21) (xy 50.8 30.48)))
  (wire (pts (xy 57.15 120.65) (xy 59.69 120.65)))
  (wire (pts (xy 129.54 113.03) (xy 129.54 114.3)))
  (wire (pts (xy 214.63 26.67) (xy 214.63 29.21)))
  (wire (pts (xy 74.93 45.72) (xy 74.93 41.91)))
  (wire (pts (xy 60.96 38.1) (xy 63.5 38.1)))
  (wire (pts (xy 50.8 76.2) (xy 50.8 73.66)))
  (wire (pts (xy 177.8 100.33) (xy 177.8 102.87)))
  (wire (pts (xy 90.17 125.73) (xy 93.98 125.73)))
  (wire (pts (xy 93.98 154.94) (xy 93.98 133.35)))
  (wire (pts (xy 144.78 153.67) (xy 144.78 156.21)))
  (wire (pts (xy 49.53 26.67) (xy 49.53 29.21)))
  (wire (pts (xy 55.88 128.27) (xy 55.88 125.73)))
  (wire (pts (xy 219.71 106.68) (xy 227.33 106.68)))
  (wire (pts (xy 218.44 104.14) (xy 223.52 104.14)))
  (wire (pts (xy 119.38 121.92) (xy 119.38 124.46)))
  (wire (pts (xy 149.86 121.92) (xy 149.86 125.73)))
  (wire (pts (xy 123.19 50.8) (xy 135.89 50.8)))
  (wire (pts (xy 48.26 73.66) (xy 48.26 76.2)))
  (wire (pts (xy 139.7 121.92) (xy 139.7 124.46)))
  (wire (pts (xy 177.8 114.3) (xy 177.8 116.84)))
  (wire (pts (xy 105.41 121.92) (xy 105.41 123.19)))
  (wire (pts (xy 60.96 58.42) (xy 74.93 58.42)))
  (wire (pts (xy 132.08 53.34) (xy 138.43 53.34)))
  (wire (pts (xy 48.26 30.48) (xy 48.26 29.21)))
  (wire (pts (xy 129.54 113.03) (xy 139.7 113.03)))
  (wire (pts (xy 175.26 19.05) (xy 175.26 21.59)))
  (wire (pts (xy 175.26 30.48) (xy 180.34 30.48)))
  (wire (pts (xy 161.29 50.8) (xy 162.56 50.8)))
  (wire (pts (xy 40.64 125.73) (xy 40.64 129.54)))
  (wire (pts (xy 248.92 31.75) (xy 248.92 29.21)))
  (wire (pts (xy 175.26 30.48) (xy 170.18 30.48)))
  (wire (pts (xy 180.34 30.48) (xy 180.34 33.02)))
  (wire (pts (xy 30.48 125.73) (xy 30.48 129.54)))
  (wire (pts (xy 59.69 128.27) (xy 55.88 128.27)))
  (wire (pts (xy 123.19 50.8) (xy 123.19 58.42)))
  (wire (pts (xy 104.14 25.4) (xy 123.19 25.4)))
  (wire (pts (xy 54.61 133.35) (xy 59.69 133.35)))
  (wire (pts (xy 48.26 76.2) (xy 49.53 76.2)))
  (wire (pts (xy 27.94 125.73) (xy 30.48 125.73)))
  (wire (pts (xy 250.19 26.67) (xy 254 26.67)))
  (wire (pts (xy 93.98 127) (xy 93.98 128.27)))
  (wire (pts (xy 135.89 43.18) (xy 135.89 50.8)))
  (wire (pts (xy 49.53 76.2) (xy 50.8 76.2)))
  (wire (pts (xy 49.53 76.2) (xy 49.53 80.01)))
  (wire (pts (xy 252.73 45.72) (xy 257.81 45.72)))
  (wire (pts (xy 93.98 133.35) (xy 90.17 133.35)))
  (wire (pts (xy 22.86 45.72) (xy 22.86 58.42)))
  (wire (pts (xy 54.61 130.81) (xy 54.61 133.35)))
  (wire (pts (xy 123.19 66.04) (xy 123.19 68.58)))
  (wire (pts (xy 138.43 55.88) (xy 132.08 55.88)))
  (wire (pts (xy 62.23 76.2) (xy 62.23 66.04)))
  (wire (pts (xy 135.89 50.8) (xy 138.43 50.8)))
  (wire (pts (xy 114.3 31.75) (xy 123.19 31.75)))
  (wire (pts (xy 209.55 24.13) (xy 215.9 24.13)))
  (wire (pts (xy 104.14 30.48) (xy 104.14 25.4)))
  (wire (pts (xy 93.98 130.81) (xy 93.98 133.35)))
  (wire (pts (xy 36.83 76.2) (xy 48.26 76.2)))
  (wire (pts (xy 59.69 130.81) (xy 54.61 130.81)))
  (wire (pts (xy 22.86 45.72) (xy 22.86 43.18)))
  (wire (pts (xy 105.41 111.76) (xy 105.41 113.03)))
  (wire (pts (xy 38.1 66.04) (xy 36.83 66.04)))
  (wire (pts (xy 170.18 30.48) (xy 170.18 33.02)))
  (wire (pts (xy 177.8 114.3) (xy 180.34 114.3)))
  (wire (pts (xy 144.78 143.51) (xy 144.78 146.05)))
  (wire (pts (xy 137.16 58.42) (xy 137.16 68.58)))
  (wire (pts (xy 48.26 29.21) (xy 49.53 29.21)))
  (wire (pts (xy 90.17 120.65) (xy 95.25 120.65)))
  (wire (pts (xy 105.41 113.03) (xy 119.38 113.03)))
  (wire (pts (xy 123.19 43.18) (xy 123.19 50.8)))
  (wire (pts (xy 60.96 45.72) (xy 74.93 45.72)))
  (wire (pts (xy 93.98 125.73) (xy 93.98 127)))
  (wire (pts (xy 175.26 29.21) (xy 175.26 30.48)))
  (rectangle (start 208.28 144.78) (end 281.94 163.83)
    (fill (type none))
  )
  (rectangle (start 13.97 91.44) (end 157.48 165.1)
    (fill (type none))
  )
  (rectangle (start 201.93 91.44) (end 248.92 118.11)
    (fill (type none))
  )
  (rectangle (start 158.75 91.44) (end 200.66 137.16)
    (fill (type none))
  )
  (rectangle (start 12.7 12.7) (end 87.63 87.63)
    (fill (type none))
  )
  (rectangle (start 194.31 12.7) (end 236.22 41.91)
    (fill (type none))
  )
  (rectangle (start 88.9 12.7) (end 193.04 87.63)
    (fill (type none))
  )
  (rectangle (start 237.49 12.7) (end 284.48 57.15)
    (fill (type none))
  )
  (rectangle (start 177.8 26.67) (end 177.8 26.67)
    (fill (type none))
  )
  (text "Solar Buck Boost" (at 187.96 190.5 0))
  (text "Power Regulator" (at 16.51 96.52 0))
  (text "Battery Charger Manager" (at 91.44 17.78 0))
  (text "Regulated Output" (at 203.2 95.25 0))
  (text "Developed By: Juan Flores Muñoz (jfm92)" (at 177.8 171.45 0))
  (text "USB Charger Input" (at 15.24 17.78 0))
  (text "Power Saving \nMode Selector" (at 160.02 96.52 0))
  (text "- Join R7 to disable power saving mode.\n- Join R8 to enable power saving mode.\n- Not join both!\n- R2 is a resistor to limit battery charging to 500mAh"
    (at 213.36 160.02 0)
  )
  (text "Information!" (at 213.36 148.59 0))
  (text "1.02" (at 269.24 194.31 0))
  (text "Battery Connector" (at 238.76 16.51 0))
  (text "1.5uH" (at 81.28 152.4 0))
  (text "Solar Panel Input" (at 195.58 16.51 0))
  (global_label "GND" (shape input) (at 36.83 38.1 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 29.9743 38.1 0))
  )
  (global_label "VBat" (shape input) (at 162.56 50.8 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 169.7785 50.8 0))
  )
  (global_label "VOut" (shape input) (at 95.25 127 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 102.529 127 0))
  )
  (global_label "GND" (shape input) (at 49.53 26.67 90) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 49.53 19.8143 90))
  )
  (global_label "PS" (shape input) (at 180.34 114.3 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 185.8047 114.3 0))
  )
  (global_label "VINA" (shape input) (at 177.8 100.33 90) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 177.8 93.2323 90))
  )
  (global_label "VBat" (shape input) (at 27.94 125.73 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 20.7215 125.73 0))
  )
  (global_label "VINA" (shape input) (at 95.25 118.11 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 102.3477 118.11 0))
  )
  (global_label "GND" (shape input) (at 132.08 53.34 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 125.2243 53.34 0))
  )
  (global_label "VINA" (shape input) (at 144.78 143.51 90) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 144.78 136.4123 90))
  )
  (global_label "VBat" (shape input) (at 254 43.18 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 246.7815 43.18 0))
  )
  (global_label "VCCSolar" (shape input) (at 106.68 50.8 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 95.1073 50.8 0))
  )
  (global_label "GND" (shape input) (at 95.25 120.65 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 102.1057 120.65 0))
  )
  (global_label "VBat" (shape input) (at 250.19 26.67 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 242.9715 26.67 0))
  )
  (global_label "VCCSolar" (shape input) (at 215.9 24.13 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 227.4727 24.13 0))
  )
  (global_label "GND" (shape input) (at 63.5 38.1 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 70.3557 38.1 0))
  )
  (global_label "VIN" (shape input) (at 135.89 43.18 90) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 135.89 37.1709 90))
  )
  (global_label "VBat" (shape input) (at 184.15 58.42 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 191.3685 58.42 0))
  )
  (global_label "VOut" (shape input) (at 218.44 104.14 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 211.161 104.14 0))
  )
  (global_label "PG" (shape input) (at 57.15 118.11 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 51.6248 118.11 0))
  )
  (global_label "PG" (shape input) (at 149.86 125.73 270) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 149.86 131.2552 90))
  )
  (global_label "VIN" (shape input) (at 175.26 19.05 90) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 175.26 13.0409 90))
  )
  (global_label "VINA" (shape input) (at 57.15 123.19 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 50.0523 123.19 0))
  )
  (global_label "PS" (shape input) (at 57.15 120.65 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 51.6853 120.65 0))
  )
  (global_label "VOut" (shape input) (at 105.41 111.76 90) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 105.41 104.481 90))
  )
  (symbol (lib_id "easyeda2kicad:TYPE-C-31-M-12") (at 49.53 52.07 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "USBC1" (at 19.05 26.67 0))
    (property "Value" "TYPE-C-31-M-12" (at 19.05 29.21 0))
    (property "Footprint" "easyeda2kicad:USB-C_SMD-TYPE-C-31-M-12" (at 49.53 81.28 0))
    (property "Datasheet" "https://lcsc.com/product-detail/USB-Type-C_Korean-Hroparts-Elec-TYPE-C-31-M-12_C165948.html" (at 49.53 83.82 0))
    (property "LCSC Part" "C165948" (at 49.53 86.36 0))
    (pin "0")
    (pin "0")
    (pin "0")
    (pin "0")
    (pin "A1")
    (pin "A12")
    (pin "A4")
    (pin "A5")
    (pin "A6")
    (pin "A7")
    (pin "A8")
    (pin "A9")
    (pin "B1")
    (pin "B12")
    (pin "B4")
    (pin "B5")
    (pin "B6")
    (pin "B7")
    (pin "B8")
    (pin "B9")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "USBC1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 248.92 31.75 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR011" (at 248.92 38.1 0))
    (property "Value" "GND" (at 248.92 36.83 0))
    (property "Footprint" "" (at 248.92 31.75 0))
    (property "Datasheet" "" (at 248.92 31.75 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "#PWR011") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:LED") (at 180.34 36.83 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D3" (at 184.15 37.1475 90))
    (property "Value" "LED" (at 184.15 39.6875 90))
    (property "Footprint" "LED_SMD:LED_0805_2012Metric" (at 180.34 36.83 0))
    (property "Datasheet" "~" (at 180.34 36.83 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "D3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 132.08 68.58 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR07" (at 132.08 74.93 0))
    (property "Value" "GND" (at 132.08 73.66 0))
    (property "Footprint" "" (at 132.08 68.58 0))
    (property "Datasheet" "" (at 132.08 68.58 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "#PWR07") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "easyeda2kicad:AO3401A_C347476") (at 114.3 50.8 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "Q1" (at 114.3 55.88 90))
    (property "Value" "AO3401A_C347476" (at 101.6 55.88 90))
    (property "Footprint" "easyeda2kicad:SOT-23_L2.9-W1.3-P1.90-LS2.4-BR" (at 127 50.8 0))
    (property "Datasheet" "https://lcsc.com/product-detail/Others_Youtai-Semiconductor-Co-Ltd-AO3401A-4-1A_C347476.html" (at 129.54 50.8 0))
    (property "LCSC Part" "C347476" (at 132.08 50.8 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "Q1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 30.48 140.97 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR019" (at 30.48 147.32 0))
    (property "Value" "GND" (at 30.48 146.05 0))
    (property "Footprint" "" (at 30.48 140.97 0))
    (property "Datasheet" "" (at 30.48 140.97 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "#PWR019") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 144.78 156.21 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR021" (at 144.78 162.56 0))
    (property "Value" "GND" (at 144.78 161.29 0))
    (property "Footprint" "" (at 144.78 156.21 0))
    (property "Datasheet" "" (at 144.78 156.21 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "#PWR021") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector:Conn_01x01_Pin") (at 232.41 106.68 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "J3" (at 231.775 101.6 0))
    (property "Value" "Conn_01x01_Pin" (at 231.775 104.14 0))
    (property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (at 232.41 106.68 0))
    (property "Datasheet" "~" (at 232.41 106.68 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "J3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 175.26 25.4 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R3" (at 177.8 24.13 0))
    (property "Value" "1K" (at 177.8 26.67 0))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (at 173.482 25.4 90))
    (property "Datasheet" "~" (at 175.26 25.4 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "R3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "easyeda2kicad:CA45-B-16V-22UF-M") (at 123.19 62.23 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C1" (at 116.84 62.23 90))
    (property "Value" "CA45-B-16V-22UF-M" (at 99.06 67.31 90))
    (property "Footprint" "easyeda2kicad:CAP-SMD_L3.5-W2.8-R-RD" (at 130.81 62.23 0))
    (property "Datasheet" "https://lcsc.com/product-detail/Tantalum-Capacitors_22uF-226-20-16V_C140371.html" (at 133.35 62.23 0))
    (property "LCSC Part" "C140371" (at 135.89 62.23 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "C1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 74.93 143.51 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR013" (at 74.93 149.86 0))
    (property "Value" "GND" (at 74.93 148.59 0))
    (property "Footprint" "" (at 74.93 143.51 0))
    (property "Datasheet" "" (at 74.93 143.51 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "#PWR013") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "easyeda2kicad:TPS63020DSJR") (at 74.93 128.27 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "U3" (at 74.93 110.49 0))
    (property "Value" "TPS63020DSJR" (at 74.93 113.03 0))
    (property "Footprint" "easyeda2kicad:VSON-14_L4.0-W3.0-P0.50-BL-EP_TI_DSJ" (at 74.93 148.59 0))
    (property "Datasheet" "https://lcsc.com/product-detail/DC-DC-Converters_TI_TPS63020DSJR_TPS63020DSJR_C15483.html" (at 74.93 151.13 0))
    (property "LCSC Part" "C15483" (at 74.93 153.67 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "U3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 180.34 73.66 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR08" (at 180.34 80.01 0))
    (property "Value" "GND" (at 180.34 78.74 0))
    (property "Footprint" "" (at 180.34 73.66 0))
    (property "Datasheet" "" (at 180.34 73.66 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "#PWR08") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 129.54 124.46 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR016" (at 129.54 130.81 0))
    (property "Value" "GND" (at 129.54 129.54 0))
    (property "Footprint" "" (at 129.54 124.46 0))
    (property "Datasheet" "" (at 129.54 124.46 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "#PWR016") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 40.64 140.97 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR020" (at 40.64 147.32 0))
    (property "Value" "GND" (at 40.64 146.05 0))
    (property "Footprint" "" (at 40.64 140.97 0))
    (property "Datasheet" "" (at 40.64 140.97 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "#PWR020") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "easyeda2kicad:CN3063") (at 149.86 54.61 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "U1" (at 149.86 66.04 0))
    (property "Value" "CN3063" (at 149.86 63.5 0))
    (property "Footprint" "easyeda2kicad:SOIC-8_L4.9-W3.9-P1.27-LS6.0-BL-EP3.3-1" (at 149.86 38.1 0))
    (property "Datasheet" "https://lcsc.com/product-detail/PMIC-AC-DC-Converters_CN3063_C28078.html" (at 149.86 35.56 0))
    (property "LCSC Part" "C28078" (at 149.86 33.02 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "U1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 177.8 120.65 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R8" (at 180.34 119.38 0))
    (property "Value" "0" (at 180.34 121.92 0))
    (property "Footprint" "Resistor_SMD:R_0402_1005Metric" (at 176.022 120.65 90))
    (property "Datasheet" "~" (at 177.8 120.65 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "R8") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 139.7 118.11 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C8" (at 143.51 116.84 0))
    (property "Value" "22uF" (at 143.51 121.92 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (at 140.6652 121.92 0))
    (property "Datasheet" "~" (at 139.7 118.11 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "C8") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 214.63 29.21 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR010" (at 214.63 35.56 0))
    (property "Value" "GND" (at 214.63 34.29 0))
    (property "Footprint" "" (at 214.63 29.21 0))
    (property "Datasheet" "" (at 214.63 29.21 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "#PWR010") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 105.41 128.27 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R5" (at 107.95 127 0))
    (property "Value" "180K" (at 107.95 129.54 0))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (at 103.632 128.27 90))
    (property "Datasheet" "~" (at 105.41 128.27 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "R5") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 252.73 48.26 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR012" (at 252.73 54.61 0))
    (property "Value" "GND" (at 252.73 53.34 0))
    (property "Footprint" "" (at 252.73 48.26 0))
    (property "Datasheet" "" (at 252.73 48.26 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "#PWR012") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 129.54 118.11 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C7" (at 133.35 116.84 0))
    (property "Value" "22uF" (at 133.35 121.92 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (at 130.5052 121.92 0))
    (property "Datasheet" "~" (at 129.54 118.11 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "C7") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 123.19 68.58 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR06" (at 123.19 74.93 0))
    (property "Value" "GND" (at 123.19 73.66 0))
    (property "Footprint" "" (at 123.19 68.58 0))
    (property "Datasheet" "" (at 123.19 68.58 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "#PWR06") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 144.78 149.86 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "C5" (at 148.59 148.59 0))
    (property "Value" "100nF" (at 148.59 151.13 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (at 145.7452 153.67 0))
    (property "Datasheet" "~" (at 144.78 149.86 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "C5") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 219.71 109.22 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR018" (at 219.71 115.57 0))
    (property "Value" "GND" (at 219.71 114.3 0))
    (property "Footprint" "" (at 219.71 109.22 0))
    (property "Datasheet" "" (at 219.71 109.22 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "#PWR018") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "easyeda2kicad:SS14") (at 123.19 38.1 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D1" (at 127 37.21 90))
    (property "Value" "SS14" (at 127 39.75 90))
    (property "Footprint" "easyeda2kicad:SMA_L4.2-W2.6-LS5.3-RD" (at 130.81 38.1 0))
    (property "Datasheet" "https://lcsc.com/product-detail/Schottky-Barrier-Diodes-SBD_SS14_C2480.html" (at 133.35 38.1 0))
    (property "LCSC Part" "C2480" (at 135.89 38.1 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "D1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 123.19 21.59 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR05" (at 123.19 25.4 0))
    (property "Value" "+5V" (at 123.19 16.51 0))
    (property "Footprint" "" (at 123.19 21.59 0))
    (property "Datasheet" "" (at 123.19 21.59 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "#PWR05") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 139.7 124.46 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR017" (at 139.7 130.81 0))
    (property "Value" "GND" (at 139.7 129.54 0))
    (property "Footprint" "" (at 139.7 124.46 0))
    (property "Datasheet" "" (at 139.7 124.46 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "#PWR017") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector:Conn_01x02_Pin") (at 262.89 43.18 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J1" (at 264.16 45.72 0))
    (property "Value" "Conn_01x02_Pin" (at 264.16 43.18 0))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (at 262.89 43.18 0))
    (property "Datasheet" "~" (at 262.89 43.18 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "J1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 132.08 60.96 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R2" (at 125.73 66.04 0))
    (property "Value" "3.6K" (at 125.73 68.58 0))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (at 130.302 60.96 90))
    (property "Datasheet" "~" (at 132.08 60.96 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "R2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 74.93 41.91 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR02" (at 74.93 45.72 0))
    (property "Value" "+5V" (at 74.93 36.83 0))
    (property "Footprint" "" (at 74.93 41.91 0))
    (property "Datasheet" "" (at 74.93 41.91 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "#PWR02") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector:Conn_01x01_Pin") (at 232.41 102.87 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "J2" (at 231.775 97.79 0))
    (property "Value" "Conn_01x01_Pin" (at 231.775 100.33 0))
    (property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (at 232.41 102.87 0))
    (property "Datasheet" "~" (at 232.41 102.87 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "J2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "easyeda2kicad:2001SMT-2P_C132500") (at 260.35 27.94 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "CN1" (at 267.97 34.29 0))
    (property "Value" "2001SMT-2P_C132500" (at 256.54 38.1 0))
    (property "Footprint" "easyeda2kicad:CONN-SMD_2001SMT-2P-WT" (at 260.35 41.91 0))
    (property "Datasheet" "https://lcsc.com/product-detail/PH-Connectors_Shenzhen-Cancome-2001series-socket-1-2P-2mm_C132500.html" (at 260.35 44.45 0))
    (property "LCSC Part" "C132500" (at 260.35 46.99 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "CN1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 105.41 135.89 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR014" (at 105.41 142.24 0))
    (property "Value" "GND" (at 105.41 140.97 0))
    (property "Footprint" "" (at 105.41 135.89 0))
    (property "Datasheet" "" (at 105.41 135.89 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "#PWR014") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "easyeda2kicad:DB301V-5.0-2P") (at 204.47 24.13 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "H1" (at 204.47 34.29 0))
    (property "Value" "DB301V-5.0-2P" (at 204.47 31.75 0))
    (property "Footprint" "easyeda2kicad:CONN-TH_2P-P5.00_L7.6-W10.0" (at 204.47 34.29 0))
    (property "Datasheet" "https://lcsc.com/product-detail/Screw-terminal_DIBO-DB301V-5-0-2P_C395882.html" (at 204.47 36.83 0))
    (property "LCSC Part" "C395882" (at 204.47 39.37 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "H1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 49.53 80.01 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR01" (at 49.53 86.36 0))
    (property "Value" "GND" (at 49.53 85.09 0))
    (property "Footprint" "" (at 49.53 80.01 0))
    (property "Datasheet" "" (at 49.53 80.01 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "#PWR01") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 180.34 67.31 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "C2" (at 184.15 66.04 0))
    (property "Value" "4.7uF" (at 184.15 68.58 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (at 181.3052 71.12 0))
    (property "Datasheet" "~" (at 180.34 67.31 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "C2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:LED") (at 170.18 36.83 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D2" (at 173.99 37.1475 90))
    (property "Value" "LED" (at 173.99 39.6875 90))
    (property "Footprint" "LED_SMD:LED_0805_2012Metric" (at 170.18 36.83 0))
    (property "Datasheet" "~" (at 170.18 36.83 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "D2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 104.14 41.91 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR04" (at 104.14 48.26 0))
    (property "Value" "GND" (at 104.14 46.99 0))
    (property "Footprint" "" (at 104.14 41.91 0))
    (property "Datasheet" "" (at 104.14 41.91 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "#PWR04") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 149.86 118.11 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R6" (at 152.4 116.84 0))
    (property "Value" "1M" (at 152.4 119.38 0))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (at 148.082 118.11 90))
    (property "Datasheet" "~" (at 149.86 118.11 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "R6") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "easyeda2kicad:PSPNAQ4030-1R5M") (at 74.93 154.94 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "L1" (at 74.93 157.48 0))
    (property "Value" "PSPNAQ4030-1R5M" (at 74.93 160.02 0))
    (property "Footprint" "easyeda2kicad:IND-SMD_L4.0-W4.0" (at 74.93 162.56 0))
    (property "Datasheet" "" (at 74.93 154.94 0))
    (property "LCSC Part" "C436670" (at 74.93 165.1 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "L1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 177.8 106.68 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R7" (at 180.34 105.41 0))
    (property "Value" "0" (at 180.34 107.95 0))
    (property "Footprint" "Resistor_SMD:R_0402_1005Metric" (at 176.022 106.68 90))
    (property "Datasheet" "~" (at 177.8 106.68 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "R7") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 119.38 124.46 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR015" (at 119.38 130.81 0))
    (property "Value" "GND" (at 119.38 129.54 0))
    (property "Footprint" "" (at 119.38 124.46 0))
    (property "Datasheet" "" (at 119.38 124.46 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "#PWR015") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 40.64 133.35 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C4" (at 44.45 132.08 0))
    (property "Value" "10uF" (at 44.45 137.16 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (at 41.6052 137.16 0))
    (property "Datasheet" "~" (at 40.64 133.35 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "C4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 30.48 133.35 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C3" (at 34.29 132.08 0))
    (property "Value" "10uF" (at 33.02 137.16 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (at 31.4452 137.16 0))
    (property "Datasheet" "~" (at 30.48 133.35 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "C3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 104.14 34.29 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R1" (at 106.68 33.02 0))
    (property "Value" "1K" (at 106.68 35.56 0))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (at 102.362 34.29 90))
    (property "Datasheet" "~" (at 104.14 34.29 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "R1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 137.16 68.58 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR023" (at 137.16 74.93 0))
    (property "Value" "GND" (at 137.16 73.66 0))
    (property "Footprint" "" (at 137.16 68.58 0))
    (property "Datasheet" "" (at 137.16 68.58 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "#PWR023") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 105.41 118.11 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R4" (at 107.95 116.84 0))
    (property "Value" "1M" (at 107.95 119.38 0))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (at 103.632 118.11 90))
    (property "Datasheet" "~" (at 105.41 118.11 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "R4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 22.86 43.18 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR03" (at 22.86 46.99 0))
    (property "Value" "+5V" (at 22.86 38.1 0))
    (property "Footprint" "" (at 22.86 43.18 0))
    (property "Datasheet" "" (at 22.86 43.18 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "#PWR03") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 177.8 129.54 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR022" (at 177.8 135.89 0))
    (property "Value" "GND" (at 177.8 134.62 0))
    (property "Footprint" "" (at 177.8 129.54 0))
    (property "Datasheet" "" (at 177.8 129.54 0))
    (pin "1")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "#PWR022") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 119.38 118.11 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C6" (at 123.19 116.84 0))
    (property "Value" "22uF" (at 121.92 121.92 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (at 120.3452 121.92 0))
    (property "Datasheet" "~" (at 119.38 118.11 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Solar-Buck-Boost"
        (path
          (reference "C6") (unit 1)
        )
      )
    )
  )
  (sheet_instances
    (path (page "1"))
  )
)
