(kicad_sch (version 20230121) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Connector:Conn_01x02_Pin" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at 0 2.54 0))
      (property "Value" "Conn_01x02_Pin" (at 0 -5.08 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_locked" "" (at 0 0 0))
      (property "ki_keywords" "connector" (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x02, script generated" (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (at 0 0 0))
      (symbol "Conn_01x02_Pin_1_1"
        (polyline
          (pts
            (xy 1.27 -2.54)
            (xy 0.8636 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy 0.8636 0)
          )
          (fill (type none))
        )
        (rectangle (start 0.8636 -2.413) (end 0 -2.667)
          (fill (type outline))
        )
        (rectangle (start 0.8636 0.127) (end 0 -0.127)
          (fill (type outline))
        )
        (pin passive line (at 5.08 0 180) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 5.08 -2.54 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
      )
    )
    (symbol "Device:C_Polarized" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (at 0.635 2.54 0))
      (property "Value" "C_Polarized" (at 0.635 -2.54 0))
      (property "Footprint" "" (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (at 0 0 0))
      (property "ki_description" "Polarized capacitor" (at 0 0 0))
      (property "ki_fp_filters" "CP_*" (at 0 0 0))
      (symbol "C_Polarized_0_1"
        (rectangle (start -2.286 0.508) (end 2.286 1.016)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 2.286)
            (xy -0.762 2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 2.794)
            (xy -1.27 1.778)
          )
          (fill (type none))
        )
        (rectangle (start 2.286 -0.508) (end -2.286 -1.016)
          (fill (type outline))
        )
      )
      (symbol "C_Polarized_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:C_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (at 0.254 1.778 0))
      (property "Value" "C_Small" (at 0.254 -2.032 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "capacitor cap" (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor, small symbol" (at 0 0 0))
      (property "ki_fp_filters" "C_*" (at 0 0 0))
      (symbol "C_Small_0_1"
        (polyline
          (pts
            (xy -1.524 -0.508)
            (xy 1.524 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.524 0.508)
            (xy 1.524 0.508)
          )
          (fill (type none))
        )
      )
      (symbol "C_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 2.032)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 2.032)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:D_Schottky" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (at 0 2.54 0))
      (property "Value" "D_Schottky" (at 0 -2.54 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "diode Schottky" (at 0 0 0))
      (property "ki_description" "Schottky diode" (at 0 0 0))
      (property "ki_fp_filters" "TO-???* *_Diode_* *SingleDiode* D_*" (at 0 0 0))
      (symbol "D_Schottky_0_1"
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 -1.27)
            (xy -1.27 0)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 0.635)
            (xy -1.905 1.27)
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 -0.635)
          )
          (fill (type none))
        )
      )
      (symbol "D_Schottky_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:LED_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (at -1.27 3.175 0))
      (property "Value" "LED_Small" (at -4.445 -2.54 0))
      (property "Footprint" "" (at 0 0 90))
      (property "Datasheet" "~" (at 0 0 90))
      (property "ki_keywords" "LED diode light-emitting-diode" (at 0 0 0))
      (property "ki_description" "Light emitting diode, small symbol" (at 0 0 0))
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (at 0 0 0))
      (symbol "LED_Small_0_1"
        (polyline
          (pts
            (xy -0.762 -1.016)
            (xy -0.762 1.016)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 0)
            (xy -0.762 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 -1.016)
            (xy -0.762 0)
            (xy 0.762 1.016)
            (xy 0.762 -1.016)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0.762)
            (xy -0.508 1.27)
            (xy -0.254 1.27)
            (xy -0.508 1.27)
            (xy -0.508 1.016)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.508 1.27)
            (xy 0 1.778)
            (xy 0.254 1.778)
            (xy 0 1.778)
            (xy 0 1.524)
          )
          (fill (type none))
        )
      )
      (symbol "LED_Small_1_1"
        (pin passive line (at -2.54 0 0) (length 1.778)
          (name "K")
          (number "1")
        )
        (pin passive line (at 2.54 0 180) (length 1.778)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:R_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "R" (at 0.762 0.508 0))
      (property "Value" "R_Small" (at 0.762 -1.016 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "R resistor" (at 0 0 0))
      (property "ki_description" "Resistor, small symbol" (at 0 0 0))
      (property "ki_fp_filters" "R_*" (at 0 0 0))
      (symbol "R_Small_0_1"
        (rectangle (start -0.762 1.778) (end 0.762 -1.778)
          (fill (type none))
        )
      )
      (symbol "R_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 0.762)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 0.762)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "GND_1" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -6.35 0))
      (property "Value" "GND_1" (at 0 -3.81 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (at 0 0 0))
      (symbol "GND_1_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
    (symbol "Transistor_FET:DMP3013SFV" (pin_names hide) (in_bom yes) (on_board yes)
      (property "Reference" "Q" (at 5.08 1.905 0))
      (property "Value" "DMP3013SFV" (at 5.08 0 0))
      (property "Footprint" "Package_SON:Diodes_PowerDI3333-8" (at 5.08 -1.905 0))
      (property "Datasheet" "https://www.diodes.com/assets/Datasheets/DMP3013SFV.pdf" (at 0 0 90))
      (property "ki_keywords" "P-Channel MOSFET" (at 0 0 0))
      (property "ki_description" "-12A Id, -30V Vds, P-Channel Power MOSFET, 9.5mOhm Ron, 33.7nC Qg (typ), PowerDI3333-8" (at 0 0 0))
      (property "ki_fp_filters" "Diodes*PowerDI3333*" (at 0 0 0))
      (symbol "DMP3013SFV_0_1"
        (polyline
          (pts
            (xy 0.254 0)
            (xy -2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.254 1.905)
            (xy 0.254 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 -1.27)
            (xy 0.762 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 0.508)
            (xy 0.762 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 2.286)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 2.54)
            (xy 2.54 1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -2.54)
            (xy 2.54 0)
            (xy 0.762 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 1.778)
            (xy 3.302 1.778)
            (xy 3.302 -1.778)
            (xy 0.762 -1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.286 0)
            (xy 1.27 0.381)
            (xy 1.27 -0.381)
            (xy 2.286 0)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 2.794 -0.508)
            (xy 2.921 -0.381)
            (xy 3.683 -0.381)
            (xy 3.81 -0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.302 -0.381)
            (xy 2.921 0.254)
            (xy 3.683 0.254)
            (xy 3.302 -0.381)
          )
          (fill (type none))
        )
        (circle (center 1.651 0) (radius 2.794)
          (fill (type none))
        )
        (circle (center 2.54 -1.778) (radius 0.254)
          (fill (type outline))
        )
        (circle (center 2.54 1.778) (radius 0.254)
          (fill (type outline))
        )
      )
      (symbol "DMP3013SFV_1_1"
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "S")
          (number "1")
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54) hide
          (name "S")
          (number "2")
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54) hide
          (name "S")
          (number "3")
        )
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "G")
          (number "4")
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "D")
          (number "5")
        )
      )
    )
    (symbol "aib:LTC4418IUF#TRPBF" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (at -10.16 18.542 0))
      (property "Value" "LTC4418IUF#TRPBF" (at -10.16 -20.32 0))
      (property "Footprint" "aib:QFN50P400X400X80-21N" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "MF" "Analog Devices" (at 0 0 0))
      (property "MAXIMUM_PACKAGE_HEIGHT" "0.8mm" (at 0 0 0))
      (property "Package" "QFN -20 Analog Devices" (at 0 0 0))
      (property "Price" "None" (at 0 0 0))
      (property "Check_prices" "https://www.snapeda.com/parts/LTC4418IUF%23TRPBF/Analog+Devices/view-part/?ref=eda" (at 0 0 0))
      (property "STANDARD" "IPC7351B" (at 0 0 0))
      (property "PARTREV" "A" (at 0 0 0))
      (property "SnapEDA_Link" "https://www.snapeda.com/parts/LTC4418IUF%23TRPBF/Analog+Devices/view-part/?ref=snap" (at 0 0 0))
      (property "MP" "LTC4418IUF#TRPBF" (at 0 0 0))
      (property "Purchase-URL" "https://pricing.snapeda.com/search?q=LTC4418IUF#TRPBF&ref=eda" (at 0 0 0))
      (property "Description" "\nDual Channel Prioritized PowerPath Controller\n" (at 0 0 0))
      (property "Availability" "In Stock" (at 0 0 0))
      (property "MANUFACTURER" "AnalogDevices" (at 0 0 0))
      (symbol "LTC4418IUF#TRPBF_0_0"
        (rectangle (start -10.16 -17.78) (end 10.16 17.78)
          (fill (type background))
        )
        (pin input line (at 15.24 -10.16 180) (length 5.08)
          (name "TMR")
          (number "1")
        )
        (pin output line (at 15.24 0 180) (length 5.08)
          (name "INTVCC")
          (number "10")
        )
        (pin output line (at -15.24 -15.24 0) (length 5.08)
          (name "G2")
          (number "11")
        )
        (pin power_in line (at -15.24 -12.7 0) (length 5.08)
          (name "VS2")
          (number "12")
        )
        (pin output line (at -15.24 -7.62 0) (length 5.08)
          (name "G1")
          (number "13")
        )
        (pin power_in line (at -15.24 -5.08 0) (length 5.08)
          (name "VS1")
          (number "14")
        )
        (pin output line (at 15.24 15.24 180) (length 5.08)
          (name "VOUT")
          (number "15")
        )
        (pin power_in line (at -15.24 5.08 0) (length 5.08)
          (name "V2")
          (number "16")
        )
        (pin power_in line (at -15.24 15.24 0) (length 5.08)
          (name "V1")
          (number "17")
        )
        (pin input line (at 15.24 -2.54 180) (length 5.08)
          (name "EN")
          (number "18")
        )
        (pin input line (at 15.24 -5.08 180) (length 5.08)
          (name "~{SHDN}")
          (number "19")
        )
        (pin input line (at -15.24 12.7 0) (length 5.08)
          (name "UV1")
          (number "2")
        )
        (pin input line (at 15.24 -12.7 180) (length 5.08)
          (name "HYS")
          (number "20")
        )
        (pin power_in line (at 15.24 -15.24 180) (length 5.08)
          (name "GND")
          (number "21")
        )
        (pin input line (at -15.24 10.16 0) (length 5.08)
          (name "OV1")
          (number "3")
        )
        (pin input line (at -15.24 2.54 0) (length 5.08)
          (name "UV2")
          (number "4")
        )
        (pin input line (at -15.24 0 0) (length 5.08)
          (name "OV2")
          (number "5")
        )
        (pin output line (at 15.24 10.16 180) (length 5.08)
          (name "~{VALID1}")
          (number "6")
        )
        (pin output line (at 15.24 7.62 180) (length 5.08)
          (name "~{VALID2}")
          (number "7")
        )
        (pin power_in line (at 15.24 -15.24 180) (length 5.08)
          (name "GND")
          (number "8")
        )
        (pin output line (at 15.24 5.08 180) (length 5.08)
          (name "CAS")
          (number "9")
        )
      )
    )
    (symbol "power:+12V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -3.81 0))
      (property "Value" "+12V" (at 0 3.556 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+12V\"" (at 0 0 0))
      (symbol "+12V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+12V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+12V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -6.35 0))
      (property "Value" "GND" (at 0 -3.81 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "power-flag" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
    (symbol "power:VCC" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -3.81 0))
      (property "Value" "VCC" (at 0 3.81 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"VCC\"" (at 0 0 0))
      (symbol "VCC_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "VCC_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "VCC")
          (number "1")
        )
      )
    )
  )
  (junction (at 158.75 100.33) (diameter 0) (color 0 0 0 0))
  (junction (at 106.68 36.83) (diameter 0) (color 0 0 0 0))
  (junction (at 137.16 54.61) (diameter 0) (color 0 0 0 0))
  (junction (at 50.8 119.38) (diameter 0) (color 0 0 0 0))
  (junction (at 152.4 68.58) (diameter 0) (color 0 0 0 0))
  (junction (at 154.94 45.72) (diameter 0) (color 0 0 0 0))
  (junction (at 151.13 160.02) (diameter 0) (color 0 0 0 0))
  (junction (at 158.75 152.4) (diameter 0) (color 0 0 0 0))
  (junction (at 144.78 160.02) (diameter 0) (color 0 0 0 0))
  (junction (at 158.75 107.95) (diameter 0) (color 0 0 0 0))
  (junction (at 177.8 45.72) (diameter 0) (color 0 0 0 0))
  (junction (at 151.13 38.1) (diameter 0) (color 0 0 0 0))
  (junction (at 154.94 38.1) (diameter 0) (color 0 0 0 0))
  (junction (at 50.8 90.17) (diameter 0) (color 0 0 0 0))
  (junction (at 73.66 54.61) (diameter 0) (color 0 0 0 0))
  (junction (at 104.14 48.26) (diameter 0) (color 0 0 0 0))
  (junction (at 144.78 43.18) (diameter 0) (color 0 0 0 0))
  (junction (at 125.73 152.4) (diameter 0) (color 0 0 0 0))
  (junction (at 153.67 160.02) (diameter 0) (color 0 0 0 0))
  (junction (at 87.63 43.18) (diameter 0) (color 0 0 0 0))
  (junction (at 144.78 167.64) (diameter 0) (color 0 0 0 0))
  (junction (at 50.8 101.6) (diameter 0) (color 0 0 0 0))
  (junction (at 152.4 63.5) (diameter 0) (color 0 0 0 0))
  (junction (at 152.4 66.04) (diameter 0) (color 0 0 0 0))
  (junction (at 137.16 55.88) (diameter 0) (color 0 0 0 0))
  (junction (at 143.51 152.4) (diameter 0) (color 0 0 0 0))
  (junction (at 144.78 38.1) (diameter 0) (color 0 0 0 0))
  (junction (at 50.8 130.81) (diameter 0) (color 0 0 0 0))
  (junction (at 82.55 52.07) (diameter 0) (color 0 0 0 0))
  (junction (at 96.52 41.91) (diameter 0) (color 0 0 0 0))
  (junction (at 63.5 54.61) (diameter 0) (color 0 0 0 0))
  (no_connect (at 137.16 48.26))
  (wire (pts (xy 92.71 48.26) (xy 104.14 48.26)))
  (wire (pts (xy 82.55 52.07) (xy 102.87 52.07)))
  (wire (pts (xy 116.84 135.89) (xy 125.73 135.89)))
  (wire (pts (xy 143.51 152.4) (xy 146.05 152.4)))
  (wire (pts (xy 87.63 43.18) (xy 87.63 44.45)))
  (wire (pts (xy 38.1 96.52) (xy 38.1 101.6)))
  (wire (pts (xy 158.75 107.95) (xy 166.37 107.95)))
  (wire (pts (xy 137.16 45.72) (xy 154.94 45.72)))
  (wire (pts (xy 137.16 53.34) (xy 137.16 54.61)))
  (wire (pts (xy 50.8 101.6) (xy 50.8 102.87)))
  (wire (pts (xy 144.78 38.1) (xy 151.13 38.1)))
  (wire (pts (xy 158.75 160.02) (xy 153.67 160.02)))
  (wire (pts (xy 97.79 66.04) (xy 106.68 66.04)))
  (wire (pts (xy 156.21 152.4) (xy 158.75 152.4)))
  (wire (pts (xy 137.16 68.58) (xy 152.4 68.58)))
  (wire (pts (xy 125.73 152.4) (xy 132.08 152.4)))
  (wire (pts (xy 137.16 66.04) (xy 152.4 66.04)))
  (wire (pts (xy 125.73 135.89) (xy 125.73 152.4)))
  (wire (pts (xy 152.4 54.61) (xy 152.4 63.5)))
  (wire (pts (xy 97.79 58.42) (xy 106.68 58.42)))
  (wire (pts (xy 137.16 54.61) (xy 137.16 55.88)))
  (wire (pts (xy 158.75 152.4) (xy 165.1 152.4)))
  (wire (pts (xy 137.16 55.88) (xy 137.16 58.42)))
  (wire (pts (xy 102.87 68.58) (xy 106.68 68.58)))
  (wire (pts (xy 143.51 140.97) (xy 143.51 152.4)))
  (wire (pts (xy 87.63 41.91) (xy 87.63 43.18)))
  (wire (pts (xy 152.4 63.5) (xy 152.4 66.04)))
  (wire (pts (xy 50.8 96.52) (xy 50.8 101.6)))
  (wire (pts (xy 64.77 129.54) (xy 71.12 129.54)))
  (wire (pts (xy 149.86 49.53) (xy 152.4 49.53)))
  (wire (pts (xy 38.1 90.17) (xy 50.8 90.17)))
  (wire (pts (xy 158.75 100.33) (xy 161.29 100.33)))
  (wire (pts (xy 170.18 45.72) (xy 172.72 45.72)))
  (wire (pts (xy 106.68 53.34) (xy 106.68 54.61)))
  (wire (pts (xy 64.77 121.92) (xy 71.12 121.92)))
  (wire (pts (xy 137.16 160.02) (xy 144.78 160.02)))
  (wire (pts (xy 102.87 60.96) (xy 106.68 60.96)))
  (wire (pts (xy 142.24 152.4) (xy 143.51 152.4)))
  (wire (pts (xy 106.68 27.94) (xy 106.68 36.83)))
  (wire (pts (xy 124.46 152.4) (xy 125.73 152.4)))
  (wire (pts (xy 137.16 43.18) (xy 144.78 43.18)))
  (wire (pts (xy 158.75 88.9) (xy 158.75 100.33)))
  (wire (pts (xy 50.8 119.38) (xy 50.8 123.19)))
  (wire (pts (xy 177.8 49.53) (xy 177.8 45.72)))
  (wire (pts (xy 137.16 38.1) (xy 144.78 38.1)))
  (wire (pts (xy 104.14 48.26) (xy 106.68 48.26)))
  (wire (pts (xy 154.94 45.72) (xy 154.94 43.18)))
  (wire (pts (xy 64.77 129.54) (xy 64.77 130.81)))
  (wire (pts (xy 101.6 41.91) (xy 101.6 40.64)))
  (wire (pts (xy 144.78 43.18) (xy 144.78 49.53)))
  (wire (pts (xy 50.8 130.81) (xy 50.8 132.08)))
  (wire (pts (xy 152.4 107.95) (xy 158.75 107.95)))
  (wire (pts (xy 38.1 101.6) (xy 50.8 101.6)))
  (wire (pts (xy 38.1 93.98) (xy 38.1 90.17)))
  (wire (pts (xy 104.14 36.83) (xy 106.68 36.83)))
  (wire (pts (xy 158.75 152.4) (xy 158.75 153.67)))
  (wire (pts (xy 177.8 38.1) (xy 154.94 38.1)))
  (wire (pts (xy 63.5 44.45) (xy 82.55 44.45)))
  (wire (pts (xy 96.52 41.91) (xy 101.6 41.91)))
  (wire (pts (xy 64.77 119.38) (xy 50.8 119.38)))
  (wire (pts (xy 102.87 50.8) (xy 106.68 50.8)))
  (wire (pts (xy 106.68 36.83) (xy 106.68 38.1)))
  (wire (pts (xy 50.8 125.73) (xy 50.8 130.81)))
  (wire (pts (xy 101.6 40.64) (xy 106.68 40.64)))
  (wire (pts (xy 63.5 44.45) (xy 63.5 54.61)))
  (wire (pts (xy 144.78 63.5) (xy 152.4 63.5)))
  (wire (pts (xy 50.8 90.17) (xy 50.8 93.98)))
  (wire (pts (xy 137.16 54.61) (xy 147.32 54.61)))
  (wire (pts (xy 64.77 121.92) (xy 64.77 119.38)))
  (wire (pts (xy 140.97 100.33) (xy 147.32 100.33)))
  (wire (pts (xy 78.74 52.07) (xy 82.55 52.07)))
  (wire (pts (xy 144.78 167.64) (xy 153.67 167.64)))
  (wire (pts (xy 152.4 66.04) (xy 152.4 68.58)))
  (wire (pts (xy 102.87 52.07) (xy 102.87 50.8)))
  (wire (pts (xy 104.14 45.72) (xy 104.14 48.26)))
  (wire (pts (xy 171.45 100.33) (xy 177.8 100.33)))
  (wire (pts (xy 64.77 130.81) (xy 50.8 130.81)))
  (wire (pts (xy 158.75 107.95) (xy 158.75 110.49)))
  (wire (pts (xy 92.71 48.26) (xy 92.71 46.99)))
  (wire (pts (xy 151.13 160.02) (xy 153.67 160.02)))
  (wire (pts (xy 87.63 43.18) (xy 106.68 43.18)))
  (wire (pts (xy 157.48 49.53) (xy 177.8 49.53)))
  (wire (pts (xy 73.66 52.07) (xy 73.66 54.61)))
  (wire (pts (xy 63.5 54.61) (xy 68.58 54.61)))
  (wire (pts (xy 144.78 171.45) (xy 144.78 167.64)))
  (wire (pts (xy 106.68 54.61) (xy 73.66 54.61)))
  (wire (pts (xy 92.71 41.91) (xy 96.52 41.91)))
  (wire (pts (xy 119.38 138.43) (xy 116.84 138.43)))
  (wire (pts (xy 96.52 36.83) (xy 99.06 36.83)))
  (wire (pts (xy 157.48 100.33) (xy 158.75 100.33)))
  (wire (pts (xy 82.55 46.99) (xy 87.63 46.99)))
  (wire (pts (xy 177.8 45.72) (xy 177.8 38.1)))
  (wire (pts (xy 154.94 45.72) (xy 165.1 45.72)))
  (wire (pts (xy 158.75 158.75) (xy 158.75 160.02)))
  (wire (pts (xy 119.38 140.97) (xy 119.38 138.43)))
  (wire (pts (xy 151.13 38.1) (xy 154.94 38.1)))
  (wire (pts (xy 137.16 63.5) (xy 139.7 63.5)))
  (wire (pts (xy 144.78 167.64) (xy 144.78 165.1)))
  (wire (pts (xy 144.78 160.02) (xy 151.13 160.02)))
  (text "P1:\nUV: 11.46V\nOV: 12.7 V" (at 67.31 36.83 0))
  (text "P2:\nUV: 4.85 V\nOV: 12.6 V" (at 49.53 50.8 0))
  (global_label "VS2" (shape input) (at 97.79 66.04 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 91.2972 66.04 0))
  )
  (global_label "Vbatt_12" (shape input) (at 104.14 45.72 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 92.9302 45.72 0))
  )
  (global_label "G2" (shape input) (at 102.87 68.58 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 97.4053 68.58 0))
  )
  (global_label "VS2" (shape input) (at 143.51 140.97 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 150.0028 140.97 0))
  )
  (global_label "VS1" (shape input) (at 97.79 58.42 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 91.2972 58.42 0))
  )
  (global_label "Vbatt_12" (shape input) (at 124.46 152.4 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 113.2502 152.4 0))
  )
  (global_label "G1" (shape input) (at 158.75 110.49 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 164.2147 110.49 0))
  )
  (global_label "VS1" (shape input) (at 158.75 88.9 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 165.2428 88.9 0))
  )
  (global_label "G2" (shape input) (at 144.78 171.45 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 150.2447 171.45 0))
  )
  (global_label "G1" (shape input) (at 102.87 60.96 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 97.4053 60.96 0))
  )
  (symbol (lib_id "power:VCC") (at 50.8 119.38 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR010" (at 50.8 123.19 0))
    (property "Value" "VCC" (at 50.8 114.3 0))
    (property "Footprint" "" (at 50.8 119.38 0))
    (property "Datasheet" "" (at 50.8 119.38 0))
    (pin "1")
    (instances
      (project "switcher"
        (path
          (reference "#PWR010") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "ups_12V"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_Small") (at 76.2 52.07 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R?" (at 76.2 49.53 90))
    (property "Value" "75K" (at 76.2 46.99 90))
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (at 76.2 52.07 0))
    (property "Datasheet" "~" (at 76.2 52.07 0))
    (pin "1")
    (pin "2")
    (instances
      (project "linky_reader"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "switcher"
        (path
          (reference "R11") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "room_sensors"
        (path
          (reference "R?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:D_Schottky") (at 153.67 163.83 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "D?" (at 158.75 166.37 90))
    (property "Value" "STPS1L30" (at 160.02 163.83 90))
    (property "Footprint" "Diode_SMD:D_SMA" (at 153.67 163.83 0))
    (property "Datasheet" "~" (at 153.67 163.83 0))
    (pin "1")
    (pin "2")
    (instances
      (project "linky"
        (path
          (reference "D?") (unit 1)
        )
      )
      (project "switcher"
        (path
          (reference "D3") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "D?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "D?") (unit 1)
        )
      )
      (project "room_sensors"
        (path
          (reference "D?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "aib:LTC4418IUF#TRPBF") (at 121.92 53.34 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U1" (at 121.92 30.48 0))
    (property "Value" "LTC4418IUF#TRPBF" (at 121.92 33.02 0))
    (property "Footprint" "aib:QFN50P400X400X80-21N" (at 121.92 53.34 0))
    (property "Datasheet" "" (at 121.92 53.34 0))
    (property "MF" "Analog Devices" (at 121.92 53.34 0))
    (property "MAXIMUM_PACKAGE_HEIGHT" "0.8mm" (at 121.92 53.34 0))
    (property "Package" "QFN -20 Analog Devices" (at 121.92 53.34 0))
    (property "Price" "None" (at 121.92 53.34 0))
    (property "Check_prices" "https://www.snapeda.com/parts/LTC4418IUF%23TRPBF/Analog+Devices/view-part/?ref=eda" (at 121.92 53.34 0))
    (property "STANDARD" "IPC7351B" (at 121.92 53.34 0))
    (property "PARTREV" "A" (at 121.92 53.34 0))
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/LTC4418IUF%23TRPBF/Analog+Devices/view-part/?ref=snap" (at 121.92 53.34 0))
    (property "MP" "LTC4418IUF#TRPBF" (at 121.92 53.34 0))
    (property "Purchase-URL" "https://pricing.snapeda.com/search?q=LTC4418IUF#TRPBF&ref=eda" (at 121.92 53.34 0))
    (property "Description" "\nDual Channel Prioritized PowerPath Controller\n" (at 121.92 53.34 0))
    (property "Availability" "In Stock" (at 121.92 53.34 0))
    (property "MANUFACTURER" "AnalogDevices" (at 121.92 53.34 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (instances
      (project "switcher"
        (path
          (reference "U1") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "U?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "U?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_Small") (at 144.78 40.64 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R?" (at 149.86 40.64 90))
    (property "Value" "100K" (at 147.32 40.64 90))
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (at 144.78 40.64 0))
    (property "Datasheet" "~" (at 144.78 40.64 0))
    (pin "1")
    (pin "2")
    (instances
      (project "linky_reader"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "switcher"
        (path
          (reference "R3") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "room_sensors"
        (path
          (reference "R?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_Small") (at 90.17 46.99 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R?" (at 90.17 50.8 90))
    (property "Value" "470K" (at 90.17 48.26 90))
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (at 90.17 46.99 0))
    (property "Datasheet" "~" (at 90.17 46.99 0))
    (pin "1")
    (pin "2")
    (instances
      (project "linky_reader"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "switcher"
        (path
          (reference "R8") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "room_sensors"
        (path
          (reference "R?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector:Conn_01x02_Pin") (at 111.76 138.43 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J7" (at 112.395 143.51 0))
    (property "Value" "P2 INPUT" (at 112.395 140.97 0))
    (property "Footprint" "Connector_AMASS:AMASS_XT30U-M_1x02_P5.0mm_Vertical" (at 111.76 138.43 0))
    (property "Datasheet" "~" (at 111.76 138.43 0))
    (pin "1")
    (pin "2")
    (instances
      (project "switcher"
        (path
          (reference "J7") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "J?") (unit 1)
        )
      )
      (project "ups_12V"
        (path
          (reference "J?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "J?") (unit 1)
        )
      )
      (project "room_sensors"
        (path
          (reference "J?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:VCC") (at 151.13 38.1 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR02" (at 151.13 41.91 0))
    (property "Value" "VCC" (at 151.13 33.02 0))
    (property "Footprint" "" (at 151.13 38.1 0))
    (property "Datasheet" "" (at 151.13 38.1 0))
    (pin "1")
    (instances
      (project "switcher"
        (path
          (reference "#PWR02") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Transistor_FET:DMP3013SFV") (at 151.13 154.94 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "Q4" (at 151.13 146.05 90))
    (property "Value" "DMP3013SFV" (at 151.13 148.59 90))
    (property "Footprint" "Package_SON:Diodes_PowerDI3333-8" (at 149.225 149.86 0))
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/DMP3013SFV.pdf" (at 151.13 154.94 90))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (instances
      (project "switcher"
        (path
          (reference "Q4") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "Q?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "Q?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C_Small") (at 158.75 156.21 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "C?" (at 161.29 154.9463 0))
    (property "Value" "100nF" (at 161.29 157.4863 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (at 158.75 156.21 0))
    (property "Datasheet" "~" (at 158.75 156.21 0))
    (pin "1")
    (pin "2")
    (instances
      (project "charger_proto"
        (path
          (reference "C?") (unit 1)
        )
      )
      (project "switcher"
        (path
          (reference "C6") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "C?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "C?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 50.8 102.87 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR09" (at 50.8 109.22 0))
    (property "Value" "GND" (at 50.8 107.95 0))
    (property "Footprint" "" (at 50.8 102.87 0))
    (property "Datasheet" "" (at 50.8 102.87 0))
    (pin "1")
    (instances
      (project "switcher"
        (path
          (reference "#PWR09") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "ups_12V"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "room_sensors"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_Small") (at 85.09 44.45 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R?" (at 83.82 41.91 90))
    (property "Value" "47K" (at 83.82 39.37 90))
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (at 85.09 44.45 0))
    (property "Datasheet" "~" (at 85.09 44.45 0))
    (pin "1")
    (pin "2")
    (instances
      (project "linky_reader"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "switcher"
        (path
          (reference "R6") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "room_sensors"
        (path
          (reference "R?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_Small") (at 154.94 49.53 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R?" (at 158.75 48.26 90))
    (property "Value" "1K" (at 158.75 50.8 90))
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (at 154.94 49.53 0))
    (property "Datasheet" "~" (at 154.94 49.53 0))
    (pin "1")
    (pin "2")
    (instances
      (project "linky"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "switcher"
        (path
          (reference "R10") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "R?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 50.8 132.08 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR011" (at 50.8 138.43 0))
    (property "Value" "GND" (at 50.8 137.16 0))
    (property "Footprint" "" (at 50.8 132.08 0))
    (property "Datasheet" "" (at 50.8 132.08 0))
    (pin "1")
    (instances
      (project "switcher"
        (path
          (reference "#PWR011") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "ups_12V"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "room_sensors"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_Small") (at 175.26 45.72 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R?" (at 175.26 40.64 90))
    (property "Value" "1K" (at 175.26 43.18 90))
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (at 175.26 45.72 0))
    (property "Datasheet" "~" (at 175.26 45.72 0))
    (pin "1")
    (pin "2")
    (instances
      (project "linky"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "switcher"
        (path
          (reference "R7") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "R?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:VCC") (at 165.1 152.4 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR014" (at 165.1 156.21 0))
    (property "Value" "VCC" (at 165.1 147.32 0))
    (property "Footprint" "" (at 165.1 152.4 0))
    (property "Datasheet" "" (at 165.1 152.4 0))
    (pin "1")
    (instances
      (project "switcher"
        (path
          (reference "#PWR014") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 153.67 88.9 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR05" (at 153.67 95.25 0))
    (property "Value" "GND" (at 149.86 91.44 0))
    (property "Footprint" "" (at 153.67 88.9 0))
    (property "Datasheet" "" (at 153.67 88.9 0))
    (pin "1")
    (instances
      (project "switcher"
        (path
          (reference "#PWR05") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "room_sensors"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector:Conn_01x02_Pin") (at 33.02 96.52 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J2" (at 33.655 101.6 0))
    (property "Value" "P1 INPUT" (at 33.655 99.06 0))
    (property "Footprint" "Connector_AMASS:AMASS_XT30U-M_1x02_P5.0mm_Vertical" (at 33.02 96.52 0))
    (property "Datasheet" "~" (at 33.02 96.52 0))
    (pin "1")
    (pin "2")
    (instances
      (project "switcher"
        (path
          (reference "J2") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "J?") (unit 1)
        )
      )
      (project "ups_12V"
        (path
          (reference "J?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "J?") (unit 1)
        )
      )
      (project "room_sensors"
        (path
          (reference "J?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C_Polarized") (at 71.12 125.73 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C?" (at 67.31 118.11 0))
    (property "Value" "680uF/50V" (at 67.31 120.65 0))
    (property "Footprint" "Capacitor_THT:CP_Radial_D13.0mm_P5.00mm" (at 72.0852 129.54 0))
    (property "Datasheet" "~" (at 71.12 125.73 0))
    (pin "1")
    (pin "2")
    (instances
      (project "charger_proto"
        (path
          (reference "C?") (unit 1)
        )
      )
      (project "switcher"
        (path
          (reference "C4") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "C?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C_Small") (at 149.86 54.61 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C?" (at 156.21 53.34 90))
    (property "Value" "100nF" (at 156.21 55.88 90))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (at 149.86 54.61 0))
    (property "Datasheet" "~" (at 149.86 54.61 0))
    (pin "1")
    (pin "2")
    (instances
      (project "charger_proto"
        (path
          (reference "C?") (unit 1)
        )
      )
      (project "switcher"
        (path
          (reference "C1") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "C?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "C?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+12V") (at 106.68 27.94 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR01" (at 106.68 31.75 0))
    (property "Value" "+12V" (at 106.68 22.86 0))
    (property "Footprint" "" (at 106.68 27.94 0))
    (property "Datasheet" "" (at 106.68 27.94 0))
    (pin "1")
    (instances
      (project "switcher"
        (path
          (reference "#PWR01") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "ups_12V"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:VCC") (at 177.8 100.33 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR08" (at 177.8 104.14 0))
    (property "Value" "VCC" (at 177.8 95.25 0))
    (property "Footprint" "" (at 177.8 100.33 0))
    (property "Datasheet" "" (at 177.8 100.33 0))
    (pin "1")
    (instances
      (project "switcher"
        (path
          (reference "#PWR08") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_Small") (at 82.55 49.53 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R?" (at 85.09 49.53 90))
    (property "Value" "0" (at 80.01 49.53 90))
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (at 82.55 49.53 0))
    (property "Datasheet" "~" (at 82.55 49.53 0))
    (pin "1")
    (pin "2")
    (instances
      (project "linky_reader"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "switcher"
        (path
          (reference "R9") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "room_sensors"
        (path
          (reference "R?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:LED_Small") (at 147.32 49.53 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D?" (at 147.3835 43.18 0))
    (property "Value" "Green" (at 147.3835 45.72 0))
    (property "Footprint" "Diode_SMD:D_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (at 147.32 49.53 90))
    (property "Datasheet" "~" (at 147.32 49.53 90))
    (pin "1")
    (pin "2")
    (instances
      (project "linky"
        (path
          (reference "D?") (unit 1)
        )
      )
      (project "switcher"
        (path
          (reference "D2") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "D?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "D?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_Small") (at 101.6 36.83 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R?" (at 101.6 34.29 90))
    (property "Value" "470K" (at 101.6 31.75 90))
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (at 101.6 36.83 0))
    (property "Datasheet" "~" (at 101.6 36.83 0))
    (pin "1")
    (pin "2")
    (instances
      (project "linky_reader"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "switcher"
        (path
          (reference "R1") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "room_sensors"
        (path
          (reference "R?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 152.4 68.58 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR04" (at 152.4 74.93 0))
    (property "Value" "GND" (at 152.4 73.66 0))
    (property "Footprint" "" (at 152.4 68.58 0))
    (property "Datasheet" "" (at 152.4 68.58 0))
    (pin "1")
    (instances
      (project "switcher"
        (path
          (reference "#PWR04") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "room_sensors"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector:Conn_01x02_Pin") (at 45.72 125.73 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J6" (at 46.355 130.81 0))
    (property "Value" "OUTPUT" (at 46.355 128.27 0))
    (property "Footprint" "Connector_AMASS:AMASS_XT30U-M_1x02_P5.0mm_Vertical" (at 45.72 125.73 0))
    (property "Datasheet" "~" (at 45.72 125.73 0))
    (pin "1")
    (pin "2")
    (instances
      (project "switcher"
        (path
          (reference "J6") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "J?") (unit 1)
        )
      )
      (project "ups_12V"
        (path
          (reference "J?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "J?") (unit 1)
        )
      )
      (project "room_sensors"
        (path
          (reference "J?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_name "GND_1") (lib_id "power:GND") (at 119.38 140.97 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR012" (at 119.38 147.32 0))
    (property "Value" "GND" (at 119.38 146.05 0))
    (property "Footprint" "" (at 119.38 140.97 0))
    (property "Datasheet" "" (at 119.38 140.97 0))
    (pin "1")
    (instances
      (project "switcher"
        (path
          (reference "#PWR012") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "ups_12V"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 138.43 140.97 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR013" (at 138.43 147.32 0))
    (property "Value" "GND" (at 134.62 142.24 0))
    (property "Footprint" "" (at 138.43 140.97 0))
    (property "Datasheet" "" (at 138.43 140.97 0))
    (pin "1")
    (instances
      (project "switcher"
        (path
          (reference "#PWR013") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "room_sensors"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C_Small") (at 140.97 140.97 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "C?" (at 140.9636 134.62 90))
    (property "Value" "100nF" (at 140.9636 137.16 90))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (at 140.97 140.97 0))
    (property "Datasheet" "~" (at 140.97 140.97 0))
    (pin "1")
    (pin "2")
    (instances
      (project "charger_proto"
        (path
          (reference "C?") (unit 1)
        )
      )
      (project "switcher"
        (path
          (reference "C5") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "C?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "C?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:LED_Small") (at 167.64 45.72 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D?" (at 167.7035 39.37 0))
    (property "Value" "Blue" (at 167.7035 41.91 0))
    (property "Footprint" "Diode_SMD:D_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (at 167.64 45.72 90))
    (property "Datasheet" "~" (at 167.64 45.72 90))
    (pin "1")
    (pin "2")
    (instances
      (project "linky"
        (path
          (reference "D?") (unit 1)
        )
      )
      (project "switcher"
        (path
          (reference "D1") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "D?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "D?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+12V") (at 140.97 100.33 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR07" (at 140.97 104.14 0))
    (property "Value" "+12V" (at 140.97 95.25 0))
    (property "Footprint" "" (at 140.97 100.33 0))
    (property "Datasheet" "" (at 140.97 100.33 0))
    (pin "1")
    (instances
      (project "switcher"
        (path
          (reference "#PWR07") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "ups_12V"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_Small") (at 154.94 40.64 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R?" (at 160.02 40.64 90))
    (property "Value" "100K" (at 157.48 40.64 90))
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (at 154.94 40.64 0))
    (property "Datasheet" "~" (at 154.94 40.64 0))
    (pin "1")
    (pin "2")
    (instances
      (project "linky_reader"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "switcher"
        (path
          (reference "R4") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "room_sensors"
        (path
          (reference "R?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Transistor_FET:DMP3013SFV") (at 137.16 154.94 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "Q3" (at 137.16 146.05 90))
    (property "Value" "DMP3013SFV" (at 137.16 148.59 90))
    (property "Footprint" "Package_SON:Diodes_PowerDI3333-8" (at 139.065 149.86 0))
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/DMP3013SFV.pdf" (at 137.16 154.94 90))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (instances
      (project "switcher"
        (path
          (reference "Q3") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "Q?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "Q?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector:Conn_01x02_Pin") (at 45.72 96.52 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J3" (at 46.355 101.6 0))
    (property "Value" "P1 INPUT" (at 46.355 99.06 0))
    (property "Footprint" "Connector_AMASS:AMASS_XT30U-M_1x02_P5.0mm_Vertical" (at 45.72 96.52 0))
    (property "Datasheet" "~" (at 45.72 96.52 0))
    (pin "1")
    (pin "2")
    (instances
      (project "switcher"
        (path
          (reference "J3") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "J?") (unit 1)
        )
      )
      (project "ups_12V"
        (path
          (reference "J?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "J?") (unit 1)
        )
      )
      (project "room_sensors"
        (path
          (reference "J?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_Small") (at 71.12 54.61 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R?" (at 69.85 52.07 90))
    (property "Value" "47K" (at 69.85 49.53 90))
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (at 71.12 54.61 0))
    (property "Datasheet" "~" (at 71.12 54.61 0))
    (pin "1")
    (pin "2")
    (instances
      (project "linky_reader"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "switcher"
        (path
          (reference "R12") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "room_sensors"
        (path
          (reference "R?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C_Small") (at 156.21 88.9 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "C?" (at 156.2036 82.55 90))
    (property "Value" "100nF" (at 156.2036 85.09 90))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (at 156.21 88.9 0))
    (property "Datasheet" "~" (at 156.21 88.9 0))
    (pin "1")
    (pin "2")
    (instances
      (project "charger_proto"
        (path
          (reference "C?") (unit 1)
        )
      )
      (project "switcher"
        (path
          (reference "C3") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "C?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "C?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Transistor_FET:DMP3013SFV") (at 152.4 102.87 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "Q1" (at 152.4 93.98 90))
    (property "Value" "DMP3013SFV" (at 152.4 96.52 90))
    (property "Footprint" "Package_SON:Diodes_PowerDI3333-8" (at 154.305 97.79 0))
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/DMP3013SFV.pdf" (at 152.4 102.87 90))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (instances
      (project "switcher"
        (path
          (reference "Q1") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "Q?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "Q?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_Small") (at 90.17 41.91 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R?" (at 90.17 39.37 90))
    (property "Value" "5.11K" (at 90.17 36.83 90))
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (at 90.17 41.91 0))
    (property "Datasheet" "~" (at 90.17 41.91 0))
    (pin "1")
    (pin "2")
    (instances
      (project "linky_reader"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "switcher"
        (path
          (reference "R5") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "room_sensors"
        (path
          (reference "R?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_Small") (at 144.78 162.56 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R?" (at 147.32 162.56 90))
    (property "Value" "1K" (at 142.24 162.56 90))
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (at 144.78 162.56 0))
    (property "Datasheet" "~" (at 144.78 162.56 0))
    (pin "1")
    (pin "2")
    (instances
      (project "linky_reader"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "switcher"
        (path
          (reference "R13") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "room_sensors"
        (path
          (reference "R?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C_Small") (at 142.24 63.5 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "C?" (at 142.2336 57.15 90))
    (property "Value" "100pF" (at 142.2336 59.69 90))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (at 142.24 63.5 0))
    (property "Datasheet" "~" (at 142.24 63.5 0))
    (pin "1")
    (pin "2")
    (instances
      (project "charger_proto"
        (path
          (reference "C?") (unit 1)
        )
      )
      (project "switcher"
        (path
          (reference "C2") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "C?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "C?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+12V") (at 50.8 90.17 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR06" (at 50.8 93.98 0))
    (property "Value" "+12V" (at 50.8 85.09 0))
    (property "Footprint" "" (at 50.8 90.17 0))
    (property "Datasheet" "" (at 50.8 90.17 0))
    (pin "1")
    (instances
      (project "switcher"
        (path
          (reference "#PWR06") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "ups_12V"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Transistor_FET:DMP3013SFV") (at 166.37 102.87 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "Q2" (at 166.37 93.98 90))
    (property "Value" "DMP3013SFV" (at 166.37 96.52 90))
    (property "Footprint" "Package_SON:Diodes_PowerDI3333-8" (at 164.465 97.79 0))
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/DMP3013SFV.pdf" (at 166.37 102.87 90))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (instances
      (project "switcher"
        (path
          (reference "Q2") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "Q?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "Q?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_Small") (at 96.52 39.37 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R?" (at 99.06 39.37 90))
    (property "Value" "75K" (at 93.98 39.37 90))
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (at 96.52 39.37 0))
    (property "Datasheet" "~" (at 96.52 39.37 0))
    (pin "1")
    (pin "2")
    (instances
      (project "linky_reader"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "switcher"
        (path
          (reference "R2") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "R?") (unit 1)
        )
      )
      (project "room_sensors"
        (path
          (reference "R?") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 63.5 54.61 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR03" (at 63.5 60.96 0))
    (property "Value" "GND" (at 59.69 55.88 0))
    (property "Footprint" "" (at 63.5 54.61 0))
    (property "Datasheet" "" (at 63.5 54.61 0))
    (pin "1")
    (instances
      (project "switcher"
        (path
          (reference "#PWR03") (unit 1)
        )
      )
      (project "charger"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "ups_5V"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
      (project "room_sensors"
        (path
          (reference "#PWR?") (unit 1)
        )
      )
    )
  )
  (sheet_instances
    (path (page "1"))
  )
)
