<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="17.45" y2="0" width="0" layer="20"/>
<wire x1="17.45" y1="0" x2="17.45" y2="22.85" width="0" layer="20"/>
<wire x1="17.45" y1="22.85" x2="0" y2="22.85" width="0" layer="20"/>
<wire x1="0" y1="22.85" x2="0" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>3V</text>
<text>3V</text>
<text>V+</text>
<text>V+</text>
<text>V+</text>
<text>irq7</text>
<text>ce8</text>
<text>cs9</text>
<text>10~</text>
<text>sda2</text>
<text>scl3</text>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>A3</text>
<text>5~</text>
<text>5~</text>
<text>6~</text>
<text>6~</text>
<text>4A6</text>
<text>Saul C. 3/13/23</text>
<text>MicroRGB-NRF24</text>
<text>Nothing to see here.</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X09">
<description>&lt;h3&gt;Plated Through Hole -9 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:9&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_09&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="nrf24l01plus">
<packages>
<package name="WIRELESS-NRF24L01">
<description>&lt;b&gt;2.4 GHz Wireless Module&lt;/b&gt; based on &lt;b&gt;NRF24L01&lt;/b&gt; chip</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="TO92">
<description>&lt;b&gt;TO-92&lt;/b&gt;</description>
</package>
<package name="C025-030X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 3 x 5 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="GG" library="SparkFun-Connectors" package="1X09" value="">
<attribute name="VALUE"/>
</element>
<element name="POWERSIDE" library="SparkFun-Connectors" package="1X09" value="">
<attribute name="VALUE"/>
</element>
<element name="M1" library="nrf24l01plus" package="WIRELESS-NRF24L01" value="WIRELESS-NRF24L01STANDARD"/>
<element name="RGB" library="SparkFun-Connectors" package="1X03_LONGPADS" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RGB1" library="SparkFun-Connectors" package="1X03_LONGPADS" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="adafruit" package="TO92" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="C025-030X050" value="">
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="C025-030X050" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="330">
<attribute name="PROD_ID" value="RES-00818"/>
</element>
<element name="R0" library="SparkFun-Resistors" package="0603" value="330">
<attribute name="PROD_ID" value="RES-00818"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="POWERSIDE" pad="9"/>
<contactref element="RGB" pad="2"/>
<contactref element="RGB1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="A3">
<contactref element="POWERSIDE" pad="8"/>
</signal>
<signal name="A2">
<contactref element="POWERSIDE" pad="7"/>
</signal>
<signal name="A1">
<contactref element="POWERSIDE" pad="6"/>
</signal>
<signal name="A0">
<contactref element="POWERSIDE" pad="5"/>
</signal>
<signal name="15">
<contactref element="POWERSIDE" pad="4"/>
<contactref element="M1" pad="5"/>
</signal>
<signal name="14">
<contactref element="POWERSIDE" pad="3"/>
<contactref element="M1" pad="7"/>
</signal>
<signal name="16">
<contactref element="POWERSIDE" pad="2"/>
<contactref element="M1" pad="6"/>
</signal>
<signal name="10">
<contactref element="POWERSIDE" pad="1"/>
</signal>
<signal name="GND">
<contactref element="GG" pad="9"/>
<contactref element="M1" pad="1"/>
<contactref element="RGB" pad="1"/>
<contactref element="RGB1" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="2">
<contactref element="GG" pad="8"/>
</signal>
<signal name="3">
<contactref element="GG" pad="7"/>
</signal>
<signal name="4">
<contactref element="GG" pad="6"/>
</signal>
<signal name="5">
<contactref element="GG" pad="5"/>
<contactref element="R0" pad="1"/>
</signal>
<signal name="6">
<contactref element="GG" pad="4"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="7">
<contactref element="GG" pad="3"/>
<contactref element="M1" pad="8"/>
</signal>
<signal name="8">
<contactref element="GG" pad="2"/>
<contactref element="M1" pad="3"/>
</signal>
<signal name="9">
<contactref element="GG" pad="1"/>
<contactref element="M1" pad="4"/>
</signal>
<signal name="3V">
<contactref element="M1" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="R1">
<contactref element="RGB1" pad="3"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="R0">
<contactref element="RGB" pad="3"/>
<contactref element="R0" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
