(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(paper "A4")
	(title_block
		(title "SOS business card")
		(date "2024-05-12")
		(rev "A")
		(company "Martynas J.")
	)
	(lib_symbols
		(symbol "4xxx:4075"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 1.27 0)
			)
			(property "Value" "4075"
				(at 0 -1.27 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4071bms-72bms-75bms.pdf"
				(at 0 0 0)
			)
			(property "Description" "Triple Or 3 inputs"
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "CMOS Or3"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "DIP?14*"
				(at 0 0 0)
			)
			(symbol "4075_1_1"
				(arc
					(start -3.81 -3.81)
					(mid -2.589 0)
					(end -3.81 3.81)
					(fill
						(type none)
					)
				)
				(arc
					(start -0.6096 -3.81)
					(mid 2.1842 -2.5851)
					(end 3.81 0)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -3.81 -3.81) (xy -0.635 -3.81)
					)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -3.81 3.81) (xy -0.635 3.81)
					)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -0.635 3.81) (xy -3.81 3.81) (xy -3.81 3.81) (xy -3.556 3.4036) (xy -3.0226 2.2606) (xy -2.6924 1.0414)
						(xy -2.6162 -0.254) (xy -2.7686 -1.4986) (xy -3.175 -2.7178) (xy -3.81 -3.81) (xy -3.81 -3.81)
						(xy -0.635 -3.81)
					)
					(fill
						(type background)
					)
				)
				(arc
					(start 3.81 0)
					(mid 2.1915 2.5936)
					(end -0.6096 3.81)
					(fill
						(type background)
					)
				)
				(pin input line
					(at -7.62 2.54 0)
					(length 4.318)
					(name "~")
					(number "1")
				)
				(pin input line
					(at -7.62 0 0)
					(length 4.953)
					(name "~")
					(number "2")
				)
				(pin input line
					(at -7.62 -2.54 0)
					(length 4.318)
					(name "~")
					(number "8")
				)
				(pin output line
					(at 7.62 0 180)
					(length 3.81)
					(name "~")
					(number "9")
				)
			)
			(symbol "4075_1_2"
				(arc
					(start 0 -3.81)
					(mid 3.7934 0)
					(end 0 3.81)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy 0 3.81) (xy -3.81 3.81) (xy -3.81 -3.81) (xy 0 -3.81)
					)
					(fill
						(type background)
					)
				)
				(pin input inverted
					(at -7.62 2.54 0)
					(length 3.81)
					(name "~")
					(number "1")
				)
				(pin input inverted
					(at -7.62 0 0)
					(length 3.81)
					(name "~")
					(number "2")
				)
				(pin input inverted
					(at -7.62 -2.54 0)
					(length 3.81)
					(name "~")
					(number "8")
				)
				(pin output inverted
					(at 7.62 0 180)
					(length 3.81)
					(name "~")
					(number "9")
				)
			)
			(symbol "4075_2_1"
				(arc
					(start -3.81 -3.81)
					(mid -2.589 0)
					(end -3.81 3.81)
					(fill
						(type none)
					)
				)
				(arc
					(start -0.6096 -3.81)
					(mid 2.1842 -2.5851)
					(end 3.81 0)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -3.81 -3.81) (xy -0.635 -3.81)
					)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -3.81 3.81) (xy -0.635 3.81)
					)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -0.635 3.81) (xy -3.81 3.81) (xy -3.81 3.81) (xy -3.556 3.4036) (xy -3.0226 2.2606) (xy -2.6924 1.0414)
						(xy -2.6162 -0.254) (xy -2.7686 -1.4986) (xy -3.175 -2.7178) (xy -3.81 -3.81) (xy -3.81 -3.81)
						(xy -0.635 -3.81)
					)
					(fill
						(type background)
					)
				)
				(arc
					(start 3.81 0)
					(mid 2.1915 2.5936)
					(end -0.6096 3.81)
					(fill
						(type background)
					)
				)
				(pin input line
					(at -7.62 2.54 0)
					(length 4.318)
					(name "~")
					(number "3")
				)
				(pin input line
					(at -7.62 0 0)
					(length 4.953)
					(name "~")
					(number "4")
				)
				(pin input line
					(at -7.62 -2.54 0)
					(length 4.318)
					(name "~")
					(number "5")
				)
				(pin output line
					(at 7.62 0 180)
					(length 3.81)
					(name "~")
					(number "6")
				)
			)
			(symbol "4075_2_2"
				(arc
					(start 0 -3.81)
					(mid 3.7934 0)
					(end 0 3.81)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy 0 3.81) (xy -3.81 3.81) (xy -3.81 -3.81) (xy 0 -3.81)
					)
					(fill
						(type background)
					)
				)
				(pin input inverted
					(at -7.62 2.54 0)
					(length 3.81)
					(name "~")
					(number "3")
				)
				(pin input inverted
					(at -7.62 0 0)
					(length 3.81)
					(name "~")
					(number "4")
				)
				(pin input inverted
					(at -7.62 -2.54 0)
					(length 3.81)
					(name "~")
					(number "5")
				)
				(pin output inverted
					(at 7.62 0 180)
					(length 3.81)
					(name "~")
					(number "6")
				)
			)
			(symbol "4075_3_1"
				(arc
					(start -3.81 -3.81)
					(mid -2.589 0)
					(end -3.81 3.81)
					(fill
						(type none)
					)
				)
				(arc
					(start -0.6096 -3.81)
					(mid 2.1842 -2.5851)
					(end 3.81 0)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -3.81 -3.81) (xy -0.635 -3.81)
					)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -3.81 3.81) (xy -0.635 3.81)
					)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -0.635 3.81) (xy -3.81 3.81) (xy -3.81 3.81) (xy -3.556 3.4036) (xy -3.0226 2.2606) (xy -2.6924 1.0414)
						(xy -2.6162 -0.254) (xy -2.7686 -1.4986) (xy -3.175 -2.7178) (xy -3.81 -3.81) (xy -3.81 -3.81)
						(xy -0.635 -3.81)
					)
					(fill
						(type background)
					)
				)
				(arc
					(start 3.81 0)
					(mid 2.1915 2.5936)
					(end -0.6096 3.81)
					(fill
						(type background)
					)
				)
				(pin output line
					(at 7.62 0 180)
					(length 3.81)
					(name "~")
					(number "10")
				)
				(pin input line
					(at -7.62 2.54 0)
					(length 4.318)
					(name "~")
					(number "11")
				)
				(pin input line
					(at -7.62 0 0)
					(length 4.953)
					(name "~")
					(number "12")
				)
				(pin input line
					(at -7.62 -2.54 0)
					(length 4.318)
					(name "~")
					(number "13")
				)
			)
			(symbol "4075_3_2"
				(arc
					(start 0 -3.81)
					(mid 3.7934 0)
					(end 0 3.81)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy 0 3.81) (xy -3.81 3.81) (xy -3.81 -3.81) (xy 0 -3.81)
					)
					(fill
						(type background)
					)
				)
				(pin output inverted
					(at 7.62 0 180)
					(length 3.81)
					(name "~")
					(number "10")
				)
				(pin input inverted
					(at -7.62 2.54 0)
					(length 3.81)
					(name "~")
					(number "11")
				)
				(pin input inverted
					(at -7.62 0 0)
					(length 3.81)
					(name "~")
					(number "12")
				)
				(pin input inverted
					(at -7.62 -2.54 0)
					(length 3.81)
					(name "~")
					(number "13")
				)
			)
			(symbol "4075_4_0"
				(pin power_in line
					(at 0 12.7 270)
					(length 5.08)
					(name "VDD")
					(number "14")
				)
				(pin power_in line
					(at 0 -12.7 90)
					(length 5.08)
					(name "VSS")
					(number "7")
				)
			)
			(symbol "4075_4_1"
				(rectangle
					(start -5.08 7.62)
					(end 5.08 -7.62)
					(fill
						(type background)
					)
				)
			)
		)
		(symbol "74xx:74HC590A"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -7.62 16.51 0)
			)
			(property "Value" "74HC590A"
				(at -7.62 -13.97 0)
			)
			(property "Footprint" ""
				(at 0 1.27 0)
			)
			(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74hc590a.pdf"
				(at 0 1.27 0)
			)
			(property "Description" "8-bit Binary Counter with Output Register 3-State Outputs, DIP-16/SOIC-16/SOIC-16W"
				(at 0 0 0)
			)
			(property "ki_keywords" "HCMOS Counter 3State"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SOIC*5.3x10.2mm*P1.27mm* SOIC*7.5x10.3mm*P1.27mm*"
				(at 0 0 0)
			)
			(symbol "74HC590A_1_0"
				(pin tri_state line
					(at 10.16 10.16 180)
					(length 2.54)
					(name "Q1")
					(number "1")
				)
				(pin input line
					(at -10.16 0 0)
					(length 2.54)
					(name "~{MRC}")
					(number "10")
				)
				(pin input line
					(at -10.16 7.62 0)
					(length 2.54)
					(name "CPC")
					(number "11")
				)
				(pin input line
					(at -10.16 12.7 0)
					(length 2.54)
					(name "~{CE}")
					(number "12")
				)
				(pin input line
					(at -10.16 5.08 0)
					(length 2.54)
					(name "CPR")
					(number "13")
				)
				(pin input line
					(at -10.16 -5.08 0)
					(length 2.54)
					(name "~{OE}")
					(number "14")
				)
				(pin tri_state line
					(at 10.16 12.7 180)
					(length 2.54)
					(name "Q0")
					(number "15")
				)
				(pin power_in line
					(at 0 17.78 270)
					(length 2.54)
					(name "VCC")
					(number "16")
				)
				(pin tri_state line
					(at 10.16 7.62 180)
					(length 2.54)
					(name "Q2")
					(number "2")
				)
				(pin tri_state line
					(at 10.16 5.08 180)
					(length 2.54)
					(name "Q3")
					(number "3")
				)
				(pin tri_state line
					(at 10.16 2.54 180)
					(length 2.54)
					(name "Q4")
					(number "4")
				)
				(pin tri_state line
					(at 10.16 0 180)
					(length 2.54)
					(name "Q5")
					(number "5")
				)
				(pin tri_state line
					(at 10.16 -2.54 180)
					(length 2.54)
					(name "Q6")
					(number "6")
				)
				(pin tri_state line
					(at 10.16 -5.08 180)
					(length 2.54)
					(name "Q7")
					(number "7")
				)
				(pin power_in line
					(at 0 -15.24 90)
					(length 2.54)
					(name "GND")
					(number "8")
				)
				(pin output line
					(at 10.16 -10.16 180)
					(length 2.54)
					(name "~{RCO}")
					(number "9")
				)
			)
			(symbol "74HC590A_1_1"
				(rectangle
					(start -7.62 15.24)
					(end 7.62 -12.7)
					(fill
						(type background)
					)
				)
			)
		)
		(symbol "74xx:74LS21"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 1.27 0)
			)
			(property "Value" "74LS21"
				(at 0 -1.27 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS21"
				(at 0 0 0)
			)
			(property "Description" "Dual 4-input AND"
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "TTL And4"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "DIP?12*"
				(at 0 0 0)
			)
			(symbol "74LS21_1_1"
				(arc
					(start -0.635 -4.445)
					(mid 3.7907 0)
					(end -0.635 4.445)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -0.635 4.445) (xy -3.81 4.445) (xy -3.81 -4.445) (xy -0.635 -4.445)
					)
					(fill
						(type background)
					)
				)
				(pin input line
					(at -7.62 3.81 0)
					(length 3.81)
					(name "~")
					(number "1")
				)
				(pin input line
					(at -7.62 1.27 0)
					(length 3.81)
					(name "~")
					(number "2")
				)
				(pin input line
					(at -7.62 -1.27 0)
					(length 3.81)
					(name "~")
					(number "4")
				)
				(pin input line
					(at -7.62 -3.81 0)
					(length 3.81)
					(name "~")
					(number "5")
				)
				(pin output line
					(at 7.62 0 180)
					(length 3.81)
					(name "~")
					(number "6")
				)
			)
			(symbol "74LS21_1_2"
				(arc
					(start -3.81 -4.445)
					(mid -2.5908 0)
					(end -3.81 4.445)
					(fill
						(type none)
					)
				)
				(arc
					(start -0.6096 -4.445)
					(mid 2.2246 -2.8422)
					(end 3.81 0)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -3.81 -4.445) (xy -0.635 -4.445)
					)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -3.81 4.445) (xy -0.635 4.445)
					)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -0.635 4.445) (xy -3.81 4.445) (xy -3.81 4.445) (xy -3.6322 4.0894) (xy -3.0988 2.921) (xy -2.7686 1.6764)
						(xy -2.6162 0.4318) (xy -2.6416 -0.8636) (xy -2.8702 -2.1082) (xy -3.2512 -3.3274) (xy -3.81 -4.445)
						(xy -3.81 -4.445) (xy -0.635 -4.445)
					)
					(fill
						(type background)
					)
				)
				(arc
					(start 3.81 0)
					(mid 2.2204 2.8379)
					(end -0.6096 4.445)
					(fill
						(type background)
					)
				)
				(pin input inverted
					(at -7.62 3.81 0)
					(length 3.81)
					(name "~")
					(number "1")
				)
				(pin input inverted
					(at -7.62 1.27 0)
					(length 4.826)
					(name "~")
					(number "2")
				)
				(pin input inverted
					(at -7.62 -1.27 0)
					(length 4.826)
					(name "~")
					(number "4")
				)
				(pin input inverted
					(at -7.62 -3.81 0)
					(length 3.81)
					(name "~")
					(number "5")
				)
				(pin output inverted
					(at 7.62 0 180)
					(length 3.81)
					(name "~")
					(number "6")
				)
			)
			(symbol "74LS21_2_1"
				(arc
					(start -0.635 -4.445)
					(mid 3.7907 0)
					(end -0.635 4.445)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -0.635 4.445) (xy -3.81 4.445) (xy -3.81 -4.445) (xy -0.635 -4.445)
					)
					(fill
						(type background)
					)
				)
				(pin input line
					(at -7.62 1.27 0)
					(length 3.81)
					(name "~")
					(number "10")
				)
				(pin input line
					(at -7.62 -1.27 0)
					(length 3.81)
					(name "~")
					(number "12")
				)
				(pin input line
					(at -7.62 -3.81 0)
					(length 3.81)
					(name "~")
					(number "13")
				)
				(pin output line
					(at 7.62 0 180)
					(length 3.81)
					(name "~")
					(number "8")
				)
				(pin input line
					(at -7.62 3.81 0)
					(length 3.81)
					(name "~")
					(number "9")
				)
			)
			(symbol "74LS21_2_2"
				(arc
					(start -3.81 -4.445)
					(mid -2.5908 0)
					(end -3.81 4.445)
					(fill
						(type none)
					)
				)
				(arc
					(start -0.6096 -4.445)
					(mid 2.2246 -2.8422)
					(end 3.81 0)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -3.81 -4.445) (xy -0.635 -4.445)
					)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -3.81 4.445) (xy -0.635 4.445)
					)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -0.635 4.445) (xy -3.81 4.445) (xy -3.81 4.445) (xy -3.6322 4.0894) (xy -3.0988 2.921) (xy -2.7686 1.6764)
						(xy -2.6162 0.4318) (xy -2.6416 -0.8636) (xy -2.8702 -2.1082) (xy -3.2512 -3.3274) (xy -3.81 -4.445)
						(xy -3.81 -4.445) (xy -0.635 -4.445)
					)
					(fill
						(type background)
					)
				)
				(arc
					(start 3.81 0)
					(mid 2.2204 2.8379)
					(end -0.6096 4.445)
					(fill
						(type background)
					)
				)
				(pin input inverted
					(at -7.62 1.27 0)
					(length 4.826)
					(name "~")
					(number "10")
				)
				(pin input inverted
					(at -7.62 -1.27 0)
					(length 4.826)
					(name "~")
					(number "12")
				)
				(pin input inverted
					(at -7.62 -3.81 0)
					(length 3.81)
					(name "~")
					(number "13")
				)
				(pin output inverted
					(at 7.62 0 180)
					(length 3.81)
					(name "~")
					(number "8")
				)
				(pin input inverted
					(at -7.62 3.81 0)
					(length 3.81)
					(name "~")
					(number "9")
				)
			)
			(symbol "74LS21_3_0"
				(pin power_in line
					(at 0 12.7 270)
					(length 5.08)
					(name "VCC")
					(number "14")
				)
				(pin power_in line
					(at 0 -12.7 90)
					(length 5.08)
					(name "GND")
					(number "7")
				)
			)
			(symbol "74LS21_3_1"
				(rectangle
					(start -5.08 7.62)
					(end 5.08 -7.62)
					(fill
						(type background)
					)
				)
			)
		)
		(symbol "74xx:74LV14"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 1.27 0)
			)
			(property "Value" "74LV14"
				(at 0 -1.27 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LV14"
				(at 0 0 0)
			)
			(property "Description" "Hex Inverter"
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "TTL not inv"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "DIP*W7.62mm*"
				(at 0 0 0)
			)
			(symbol "74LV14_1_0"
				(polyline
					(pts
						(xy -3.81 3.81) (xy -3.81 -3.81) (xy 3.81 0) (xy -3.81 3.81)
					)
					(fill
						(type background)
					)
				)
				(pin input line
					(at -7.62 0 0)
					(length 3.81)
					(name "~")
					(number "1")
				)
				(pin output inverted
					(at 7.62 0 180)
					(length 3.81)
					(name "~")
					(number "2")
				)
			)
			(symbol "74LV14_2_0"
				(polyline
					(pts
						(xy -3.81 3.81) (xy -3.81 -3.81) (xy 3.81 0) (xy -3.81 3.81)
					)
					(fill
						(type background)
					)
				)
				(pin input line
					(at -7.62 0 0)
					(length 3.81)
					(name "~")
					(number "3")
				)
				(pin output inverted
					(at 7.62 0 180)
					(length 3.81)
					(name "~")
					(number "4")
				)
			)
			(symbol "74LV14_3_0"
				(polyline
					(pts
						(xy -3.81 3.81) (xy -3.81 -3.81) (xy 3.81 0) (xy -3.81 3.81)
					)
					(fill
						(type background)
					)
				)
				(pin input line
					(at -7.62 0 0)
					(length 3.81)
					(name "~")
					(number "5")
				)
				(pin output inverted
					(at 7.62 0 180)
					(length 3.81)
					(name "~")
					(number "6")
				)
			)
			(symbol "74LV14_4_0"
				(polyline
					(pts
						(xy -3.81 3.81) (xy -3.81 -3.81) (xy 3.81 0) (xy -3.81 3.81)
					)
					(fill
						(type background)
					)
				)
				(pin output inverted
					(at 7.62 0 180)
					(length 3.81)
					(name "~")
					(number "8")
				)
				(pin input line
					(at -7.62 0 0)
					(length 3.81)
					(name "~")
					(number "9")
				)
			)
			(symbol "74LV14_5_0"
				(polyline
					(pts
						(xy -3.81 3.81) (xy -3.81 -3.81) (xy 3.81 0) (xy -3.81 3.81)
					)
					(fill
						(type background)
					)
				)
				(pin output inverted
					(at 7.62 0 180)
					(length 3.81)
					(name "~")
					(number "10")
				)
				(pin input line
					(at -7.62 0 0)
					(length 3.81)
					(name "~")
					(number "11")
				)
			)
			(symbol "74LV14_6_0"
				(polyline
					(pts
						(xy -3.81 3.81) (xy -3.81 -3.81) (xy 3.81 0) (xy -3.81 3.81)
					)
					(fill
						(type background)
					)
				)
				(pin output inverted
					(at 7.62 0 180)
					(length 3.81)
					(name "~")
					(number "12")
				)
				(pin input line
					(at -7.62 0 0)
					(length 3.81)
					(name "~")
					(number "13")
				)
			)
			(symbol "74LV14_7_0"
				(pin power_in line
					(at 0 12.7 270)
					(length 5.08)
					(name "3.3V")
					(number "14")
				)
				(pin power_in line
					(at 0 -12.7 90)
					(length 5.08)
					(name "GND")
					(number "7")
				)
			)
			(symbol "74LV14_7_1"
				(rectangle
					(start -5.08 7.62)
					(end 5.08 -7.62)
					(fill
						(type background)
					)
				)
			)
		)
		(symbol "Connector:Conn_01x01_Pin"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 2.54 0)
			)
			(property "Value" "Conn_01x01_Pin"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x01, script generated"
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x01_Pin_1_1"
				(polyline
					(pts
						(xy 1.27 0) (xy 0.8636 0)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0.8636 0.127)
					(end 0 -0.127)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at 5.08 0 180)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
			)
		)
		(symbol "Connector:USB_C_Receptacle_PowerOnly_6P"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 16.51 0)
			)
			(property "Value" "USB_C_Receptacle_PowerOnly_6P"
				(at 0 13.97 0)
			)
			(property "Footprint" ""
				(at 3.81 2.54 0)
			)
			(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
				(at 0 0 0)
			)
			(property "Description" "USB Power-Only 6P Type-C Receptacle connector"
				(at 0 0 0)
			)
			(property "ki_keywords" "usb universal serial bus type-C power-only charging-only 6P 6C"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "USB*C*Receptacle*"
				(at 0 0 0)
			)
			(symbol "USB_C_Receptacle_PowerOnly_6P_0_0"
				(rectangle
					(start -0.254 -12.7)
					(end 0.254 -11.684)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 10.16 -7.366)
					(end 9.144 -7.874)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 10.16 -4.826)
					(end 9.144 -5.334)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 10.16 7.874)
					(end 9.144 7.366)
					(fill
						(type none)
					)
				)
			)
			(symbol "USB_C_Receptacle_PowerOnly_6P_0_1"
				(rectangle
					(start -10.16 12.7)
					(end 10.16 -12.7)
					(fill
						(type background)
					)
				)
				(arc
					(start -8.89 -1.27)
					(mid -6.985 -3.1667)
					(end -5.08 -1.27)
					(fill
						(type none)
					)
				)
				(arc
					(start -7.62 -1.27)
					(mid -6.985 -1.9023)
					(end -6.35 -1.27)
					(fill
						(type none)
					)
				)
				(arc
					(start -7.62 -1.27)
					(mid -6.985 -1.9023)
					(end -6.35 -1.27)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -7.62 -1.27)
					(end -6.35 6.35)
					(fill
						(type outline)
					)
				)
				(arc
					(start -6.35 6.35)
					(mid -6.985 6.9823)
					(end -7.62 6.35)
					(fill
						(type none)
					)
				)
				(arc
					(start -6.35 6.35)
					(mid -6.985 6.9823)
					(end -7.62 6.35)
					(fill
						(type outline)
					)
				)
				(arc
					(start -5.08 6.35)
					(mid -6.985 8.2467)
					(end -8.89 6.35)
					(fill
						(type none)
					)
				)
				(circle
					(center -2.54 3.683)
					(radius 0.635)
					(fill
						(type outline)
					)
				)
				(circle
					(center 0 -3.302)
					(radius 1.27)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -8.89 -1.27) (xy -8.89 6.35)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -5.08 6.35) (xy -5.08 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -3.302) (xy 0 6.858)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -0.762) (xy -2.54 1.778) (xy -2.54 3.048)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0.508) (xy 2.54 3.048) (xy 2.54 4.318)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 6.858) (xy 0 9.398) (xy 1.27 6.858) (xy -1.27 6.858)
					)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 1.905 4.318)
					(end 3.175 5.588)
					(fill
						(type outline)
					)
				)
			)
			(symbol "USB_C_Receptacle_PowerOnly_6P_1_1"
				(pin passive line
					(at 0 -17.78 90)
					(length 5.08)
					(name "GND")
					(number "A12")
				)
				(pin bidirectional line
					(at 15.24 -5.08 180)
					(length 5.08)
					(name "CC1")
					(number "A5")
				)
				(pin passive line
					(at 15.24 7.62 180)
					(length 5.08)
					(name "VBUS")
					(number "A9")
				)
				(pin passive line
					(at 0 -17.78 90)
					(length 5.08) hide
					(name "GND")
					(number "B12")
				)
				(pin bidirectional line
					(at 15.24 -7.62 180)
					(length 5.08)
					(name "CC2")
					(number "B5")
				)
				(pin passive line
					(at 15.24 7.62 180)
					(length 5.08) hide
					(name "VBUS")
					(number "B9")
				)
				(pin passive line
					(at -7.62 -17.78 90)
					(length 5.08)
					(name "SHIELD")
					(number "S1")
				)
			)
		)
		(symbol "Device:Battery_Cell"
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "BT"
				(at 2.54 2.54 0)
			)
			(property "Value" "Battery_Cell"
				(at 2.54 0 0)
			)
			(property "Footprint" ""
				(at 0 1.524 90)
			)
			(property "Datasheet" "~"
				(at 0 1.524 90)
			)
			(property "Description" "Single-cell battery"
				(at 0 0 0)
			)
			(property "ki_keywords" "battery cell"
				(at 0 0 0)
			)
			(symbol "Battery_Cell_0_1"
				(rectangle
					(start -2.286 1.778)
					(end 2.286 1.524)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -1.524 1.016)
					(end 1.524 0.508)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 0 0.762) (xy 0 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.778) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 3.048) (xy 1.778 3.048)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 3.556) (xy 1.27 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Battery_Cell_1_1"
				(pin passive line
					(at 0 5.08 270)
					(length 2.54)
					(name "+")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 90)
					(length 2.54)
					(name "-")
					(number "2")
				)
			)
		)
		(symbol "Device:C_Small"
			(pin_numbers hide)
			(pin_names
				(offset 0.254) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.254 1.778 0)
			)
			(property "Value" "C_Small"
				(at 0.254 -2.032 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Unpolarized capacitor, small symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "capacitor cap"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "C_*"
				(at 0 0 0)
			)
			(symbol "C_Small_0_1"
				(polyline
					(pts
						(xy -1.524 -0.508) (xy 1.524 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.524 0.508) (xy 1.524 0.508)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "C_Small_1_1"
				(pin passive line
					(at 0 2.54 270)
					(length 2.032)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 90)
					(length 2.032)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Device:LED"
			(pin_numbers hide)
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "LED"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Light emitting diode"
				(at 0 0 0)
			)
			(property "ki_keywords" "LED diode"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*"
				(at 0 0 0)
			)
			(symbol "LED_0_1"
				(polyline
					(pts
						(xy -1.27 -1.27) (xy -1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 0) (xy 1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.27) (xy 1.27 1.27) (xy -1.27 0) (xy 1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.048 -0.762) (xy -4.572 -2.286) (xy -3.81 -2.286) (xy -4.572 -2.286) (xy -4.572 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.778 -0.762) (xy -3.302 -2.286) (xy -2.54 -2.286) (xy -3.302 -2.286) (xy -3.302 -1.524)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "LED_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
		)
		(symbol "Device:Q_PMOS_GDSD"
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "Q"
				(at 5.08 1.27 0)
			)
			(property "Value" "Q_PMOS_GDSD"
				(at 5.08 -1.27 0)
			)
			(property "Footprint" ""
				(at 5.08 2.54 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "P-MOSFET transistor, gate/drain/source, drain connected to mounting plane"
				(at 0 0 0)
			)
			(property "ki_keywords" "transistor PMOS P-MOS P-MOSFET"
				(at 0 0 0)
			)
			(symbol "Q_PMOS_GDSD_0_1"
				(polyline
					(pts
						(xy 0.254 0) (xy -2.54 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.254 1.905) (xy 0.254 -1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -1.27) (xy 0.762 -2.286)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 0.508) (xy 0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 2.286) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 -2.54) (xy 2.54 0) (xy 0.762 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 2.54) (xy 2.54 2.54) (xy 2.54 1.778)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 1.778) (xy 3.302 1.778) (xy 3.302 -1.778) (xy 0.762 -1.778)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 0) (xy 1.27 0.381) (xy 1.27 -0.381) (xy 2.286 0)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 2.794 -0.508) (xy 2.921 -0.381) (xy 3.683 -0.381) (xy 3.81 -0.254)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -0.381) (xy 2.921 0.254) (xy 3.683 0.254) (xy 3.302 -0.381)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 1.651 0)
					(radius 2.794)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -1.778)
					(radius 0.254)
					(fill
						(type outline)
					)
				)
				(circle
					(center 2.54 1.778)
					(radius 0.254)
					(fill
						(type outline)
					)
				)
			)
			(symbol "Q_PMOS_GDSD_1_1"
				(pin input line
					(at -5.08 0 0)
					(length 2.54)
					(name "G")
					(number "1")
				)
				(pin passive line
					(at 2.54 5.08 270)
					(length 2.54)
					(name "D")
					(number "2")
				)
				(pin passive line
					(at 2.54 -5.08 90)
					(length 2.54)
					(name "S")
					(number "3")
				)
				(pin passive line
					(at 5.08 5.08 270)
					(length 2.54)
					(name "D")
					(number "4")
				)
			)
		)
		(symbol "Device:R"
			(pin_numbers hide)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Diode:MBRA340"
			(pin_numbers hide)
			(pin_names hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "MBRA340"
				(at 0 -2.54 0)
			)
			(property "Footprint" "Diode_SMD:D_SMA"
				(at 0 -4.445 0)
			)
			(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MBRA340T3-D.PDF"
				(at 0 0 0)
			)
			(property "Description" "40V 3A Schottky Barrier Rectifier Diode, SMA(DO-214AC)"
				(at 0 0 0)
			)
			(property "ki_keywords" "diode Schottky"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "D*SMA*"
				(at 0 0 0)
			)
			(symbol "MBRA340_0_1"
				(polyline
					(pts
						(xy 1.27 0) (xy -1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 1.27) (xy 1.27 -1.27) (xy -1.27 0) (xy 1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.905 0.635) (xy -1.905 1.27) (xy -1.27 1.27) (xy -1.27 -1.27) (xy -0.635 -1.27) (xy -0.635 -0.635)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "MBRA340_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
		)
		(symbol "Switch:SW_SPDT"
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SW"
				(at 0 5.08 0)
			)
			(property "Value" "SW_SPDT"
				(at 0 -5.08 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 -7.62 0)
			)
			(property "Description" "Switch, single pole double throw"
				(at 0 0 0)
			)
			(property "ki_keywords" "switch single-pole double-throw spdt ON-ON"
				(at 0 0 0)
			)
			(symbol "SW_SPDT_0_1"
				(circle
					(center -2.032 0)
					(radius 0.4572)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.651 0.254) (xy 1.651 2.286)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.032 -2.54)
					(radius 0.4572)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.032 2.54)
					(radius 0.4572)
					(fill
						(type none)
					)
				)
			)
			(symbol "SW_SPDT_1_1"
				(rectangle
					(start -3.175 3.81)
					(end 3.175 -3.81)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at 5.08 2.54 180)
					(length 2.54)
					(name "A")
					(number "1")
				)
				(pin passive line
					(at -5.08 0 0)
					(length 2.54)
					(name "B")
					(number "2")
				)
				(pin passive line
					(at 5.08 -2.54 180)
					(length 2.54)
					(name "C")
					(number "3")
				)
			)
		)
		(symbol "Timer:TLC555xD"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -10.16 8.89 0)
			)
			(property "Value" "TLC555xD"
				(at 2.54 8.89 0)
			)
			(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
				(at 21.59 -10.16 0)
			)
			(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlc555.pdf"
				(at 21.59 -10.16 0)
			)
			(property "Description" "Single LinCMOS Timer, 555 compatible, SOIC-8"
				(at 0 0 0)
			)
			(property "ki_keywords" "single timer 555"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
				(at 0 0 0)
			)
			(symbol "TLC555xD_0_0"
				(pin power_in line
					(at 0 -10.16 90)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin power_in line
					(at 0 10.16 270)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
			)
			(symbol "TLC555xD_0_1"
				(rectangle
					(start -8.89 -7.62)
					(end 8.89 7.62)
					(fill
						(type background)
					)
				)
				(rectangle
					(start -8.89 -7.62)
					(end 8.89 7.62)
					(fill
						(type background)
					)
				)
			)
			(symbol "TLC555xD_1_1"
				(pin input line
					(at -12.7 5.08 0)
					(length 3.81)
					(name "TR")
					(number "2")
				)
				(pin output line
					(at 12.7 5.08 180)
					(length 3.81)
					(name "Q")
					(number "3")
				)
				(pin input inverted
					(at -12.7 -5.08 0)
					(length 3.81)
					(name "R")
					(number "4")
				)
				(pin input line
					(at -12.7 0 0)
					(length 3.81)
					(name "CV")
					(number "5")
				)
				(pin input line
					(at 12.7 -5.08 180)
					(length 3.81)
					(name "THR")
					(number "6")
				)
				(pin input line
					(at 12.7 0 180)
					(length 3.81)
					(name "DIS")
					(number "7")
				)
			)
		)
		(symbol "Transistor_FET:BSS138"
			(pin_names hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "Q"
				(at 5.08 1.905 0)
			)
			(property "Value" "BSS138"
				(at 5.08 0 0)
			)
			(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
				(at 5.08 -1.905 0)
			)
			(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BSS138-D.PDF"
				(at 5.08 -3.81 0)
			)
			(property "Description" "50V Vds, 0.22A Id, N-Channel MOSFET, SOT-23"
				(at 0 0 0)
			)
			(property "ki_keywords" "N-Channel MOSFET"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "SOT?23*"
				(at 0 0 0)
			)
			(symbol "BSS138_0_1"
				(polyline
					(pts
						(xy 0.254 0) (xy -2.54 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.254 1.905) (xy 0.254 -1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -1.27) (xy 0.762 -2.286)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 0.508) (xy 0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 2.286) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 2.54) (xy 2.54 1.778)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 -2.54) (xy 2.54 0) (xy 0.762 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -1.778) (xy 3.302 -1.778) (xy 3.302 1.778) (xy 0.762 1.778)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 0) (xy 2.032 0.381) (xy 2.032 -0.381) (xy 1.016 0)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 2.794 0.508) (xy 2.921 0.381) (xy 3.683 0.381) (xy 3.81 0.254)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 0.381) (xy 2.921 -0.254) (xy 3.683 -0.254) (xy 3.302 0.381)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 1.651 0)
					(radius 2.794)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -1.778)
					(radius 0.254)
					(fill
						(type outline)
					)
				)
				(circle
					(center 2.54 1.778)
					(radius 0.254)
					(fill
						(type outline)
					)
				)
			)
			(symbol "BSS138_1_1"
				(pin input line
					(at -5.08 0 0)
					(length 2.54)
					(name "G")
					(number "1")
				)
				(pin passive line
					(at 2.54 -5.08 90)
					(length 2.54)
					(name "S")
					(number "2")
				)
				(pin passive line
					(at 2.54 5.08 270)
					(length 2.54)
					(name "D")
					(number "3")
				)
			)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
		(symbol "power:VCC"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "VCC"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"VCC\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "VCC_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "VCC_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
	)
	(junction
		(at 184.15 46.99)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 129.54 125.73)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 191.77 46.99)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 224.79 124.46)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 121.92 140.97)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 129.54 143.51)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 184.15 38.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 109.22 128.27)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 266.7 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 168.91 46.99)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 124.46 168.91)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 114.3 105.41)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 236.22 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 168.91 132.08)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 76.2 116.84)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 228.6 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 57.15 33.02)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 124.46 132.08)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 114.3 143.51)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 191.77 38.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 43.18 125.73)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 129.54 115.57)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 243.84 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 241.3 123.19)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 199.39 46.99)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 176.53 46.99)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 129.54 99.06)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 116.84 116.84)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 266.7 57.15)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 161.29 38.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 121.92 123.19)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 259.08 53.34)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 236.22 134.62)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 106.68 158.75)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 57.15 49.53)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 129.54 107.95)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 111.76 116.84)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 243.84 139.7)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 168.91 38.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 68.58 151.13)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 176.53 38.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 71.12 132.08)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 246.38 34.29)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 29.21 58.42)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 63.5 134.62)
	)
	(no_connect
		(at 92.71 162.56)
	)
	(no_connect
		(at 69.85 35.56)
	)
	(no_connect
		(at 63.5 132.08)
	)
	(no_connect
		(at 63.5 137.16)
	)
	(wire
		(pts
			(xy 29.21 58.42) (xy 33.02 58.42)
		)
	)
	(wire
		(pts
			(xy 176.53 38.1) (xy 168.91 38.1)
		)
	)
	(wire
		(pts
			(xy 57.15 36.83) (xy 57.15 33.02)
		)
	)
	(wire
		(pts
			(xy 129.54 125.73) (xy 129.54 128.27)
		)
	)
	(wire
		(pts
			(xy 259.08 50.8) (xy 259.08 53.34)
		)
	)
	(wire
		(pts
			(xy 161.29 38.1) (xy 161.29 40.64)
		)
	)
	(wire
		(pts
			(xy 129.54 168.91) (xy 124.46 168.91)
		)
	)
	(wire
		(pts
			(xy 144.78 127) (xy 153.67 127)
		)
	)
	(wire
		(pts
			(xy 68.58 168.91) (xy 124.46 168.91)
		)
	)
	(wire
		(pts
			(xy 224.79 134.62) (xy 236.22 134.62)
		)
	)
	(wire
		(pts
			(xy 191.77 45.72) (xy 191.77 46.99)
		)
	)
	(wire
		(pts
			(xy 129.54 132.08) (xy 129.54 130.81)
		)
	)
	(wire
		(pts
			(xy 176.53 46.99) (xy 184.15 46.99)
		)
	)
	(wire
		(pts
			(xy 246.38 45.72) (xy 246.38 50.8)
		)
	)
	(wire
		(pts
			(xy 40.64 125.73) (xy 43.18 125.73)
		)
	)
	(wire
		(pts
			(xy 184.15 46.99) (xy 184.15 45.72)
		)
	)
	(wire
		(pts
			(xy 151.13 149.86) (xy 153.67 149.86)
		)
	)
	(wire
		(pts
			(xy 151.13 119.38) (xy 153.67 119.38)
		)
	)
	(wire
		(pts
			(xy 266.7 48.26) (xy 266.7 49.53)
		)
	)
	(wire
		(pts
			(xy 243.84 139.7) (xy 243.84 140.97)
		)
	)
	(wire
		(pts
			(xy 236.22 144.78) (xy 236.22 149.86)
		)
	)
	(wire
		(pts
			(xy 246.38 50.8) (xy 259.08 50.8)
		)
	)
	(wire
		(pts
			(xy 243.84 149.86) (xy 243.84 148.59)
		)
	)
	(wire
		(pts
			(xy 191.77 46.99) (xy 184.15 46.99)
		)
	)
	(wire
		(pts
			(xy 153.67 96.52) (xy 153.67 116.84)
		)
	)
	(wire
		(pts
			(xy 109.22 128.27) (xy 109.22 156.21)
		)
	)
	(wire
		(pts
			(xy 73.66 128.27) (xy 77.47 128.27)
		)
	)
	(wire
		(pts
			(xy 124.46 132.08) (xy 129.54 132.08)
		)
	)
	(wire
		(pts
			(xy 109.22 128.27) (xy 124.46 128.27)
		)
	)
	(wire
		(pts
			(xy 63.5 129.54) (xy 68.58 129.54)
		)
	)
	(wire
		(pts
			(xy 114.3 143.51) (xy 114.3 105.41)
		)
	)
	(wire
		(pts
			(xy 63.5 142.24) (xy 64.77 142.24)
		)
	)
	(wire
		(pts
			(xy 106.68 171.45) (xy 106.68 158.75)
		)
	)
	(wire
		(pts
			(xy 129.54 173.99) (xy 76.2 173.99)
		)
	)
	(wire
		(pts
			(xy 184.15 38.1) (xy 176.53 38.1)
		)
	)
	(wire
		(pts
			(xy 124.46 115.57) (xy 129.54 115.57)
		)
	)
	(wire
		(pts
			(xy 124.46 168.91) (xy 124.46 161.29)
		)
	)
	(wire
		(pts
			(xy 236.22 151.13) (xy 236.22 149.86)
		)
	)
	(wire
		(pts
			(xy 224.79 134.62) (xy 224.79 133.35)
		)
	)
	(wire
		(pts
			(xy 151.13 157.48) (xy 151.13 149.86)
		)
	)
	(wire
		(pts
			(xy 68.58 151.13) (xy 77.47 151.13)
		)
	)
	(wire
		(pts
			(xy 153.67 127) (xy 153.67 121.92)
		)
	)
	(wire
		(pts
			(xy 199.39 38.1) (xy 199.39 40.64)
		)
	)
	(wire
		(pts
			(xy 246.38 34.29) (xy 246.38 38.1)
		)
	)
	(wire
		(pts
			(xy 224.79 124.46) (xy 231.14 124.46)
		)
	)
	(wire
		(pts
			(xy 144.78 96.52) (xy 153.67 96.52)
		)
	)
	(wire
		(pts
			(xy 266.7 46.99) (xy 266.7 48.26)
		)
	)
	(wire
		(pts
			(xy 121.92 123.19) (xy 129.54 123.19)
		)
	)
	(wire
		(pts
			(xy 168.91 38.1) (xy 168.91 40.64)
		)
	)
	(polyline
		(pts
			(xy 210.185 76.2) (xy 210.185 157.48)
		)
	)
	(wire
		(pts
			(xy 184.15 38.1) (xy 191.77 38.1)
		)
	)
	(wire
		(pts
			(xy 176.53 38.1) (xy 176.53 40.64)
		)
	)
	(wire
		(pts
			(xy 114.3 92.71) (xy 129.54 92.71)
		)
	)
	(wire
		(pts
			(xy 129.54 176.53) (xy 114.3 176.53)
		)
	)
	(wire
		(pts
			(xy 144.78 157.48) (xy 151.13 157.48)
		)
	)
	(wire
		(pts
			(xy 233.68 43.18) (xy 233.68 45.72)
		)
	)
	(wire
		(pts
			(xy 259.08 53.34) (xy 259.08 57.15)
		)
	)
	(wire
		(pts
			(xy 92.71 128.27) (xy 109.22 128.27)
		)
	)
	(wire
		(pts
			(xy 266.7 34.29) (xy 266.7 39.37)
		)
	)
	(wire
		(pts
			(xy 191.77 46.99) (xy 199.39 46.99)
		)
	)
	(wire
		(pts
			(xy 50.8 45.72) (xy 48.26 45.72)
		)
	)
	(wire
		(pts
			(xy 48.26 33.02) (xy 57.15 33.02)
		)
	)
	(wire
		(pts
			(xy 228.6 40.64) (xy 228.6 48.26)
		)
	)
	(wire
		(pts
			(xy 71.12 139.7) (xy 77.47 139.7)
		)
	)
	(wire
		(pts
			(xy 48.26 58.42) (xy 48.26 48.26)
		)
	)
	(wire
		(pts
			(xy 116.84 95.25) (xy 116.84 116.84)
		)
	)
	(wire
		(pts
			(xy 63.5 119.38) (xy 71.12 119.38)
		)
	)
	(wire
		(pts
			(xy 224.79 120.65) (xy 224.79 124.46)
		)
	)
	(wire
		(pts
			(xy 241.3 121.92) (xy 241.3 123.19)
		)
	)
	(wire
		(pts
			(xy 236.22 149.86) (xy 243.84 149.86)
		)
	)
	(wire
		(pts
			(xy 71.12 132.08) (xy 71.12 139.7)
		)
	)
	(wire
		(pts
			(xy 25.4 58.42) (xy 29.21 58.42)
		)
	)
	(wire
		(pts
			(xy 144.78 172.72) (xy 153.67 172.72)
		)
	)
	(wire
		(pts
			(xy 116.84 116.84) (xy 111.76 116.84)
		)
	)
	(wire
		(pts
			(xy 114.3 176.53) (xy 114.3 143.51)
		)
	)
	(wire
		(pts
			(xy 71.12 119.38) (xy 71.12 105.41)
		)
	)
	(wire
		(pts
			(xy 57.15 33.02) (xy 59.69 33.02)
		)
	)
	(wire
		(pts
			(xy 111.76 153.67) (xy 111.76 116.84)
		)
	)
	(wire
		(pts
			(xy 191.77 38.1) (xy 191.77 40.64)
		)
	)
	(wire
		(pts
			(xy 184.15 134.62) (xy 185.42 134.62)
		)
	)
	(wire
		(pts
			(xy 241.3 123.19) (xy 245.11 123.19)
		)
	)
	(wire
		(pts
			(xy 129.54 113.03) (xy 129.54 115.57)
		)
	)
	(wire
		(pts
			(xy 111.76 116.84) (xy 92.71 116.84)
		)
	)
	(wire
		(pts
			(xy 43.18 125.73) (xy 43.18 127)
		)
	)
	(wire
		(pts
			(xy 29.21 66.04) (xy 29.21 58.42)
		)
	)
	(wire
		(pts
			(xy 184.15 40.64) (xy 184.15 38.1)
		)
	)
	(wire
		(pts
			(xy 106.68 139.7) (xy 106.68 158.75)
		)
	)
	(wire
		(pts
			(xy 266.7 95.25) (xy 266.7 93.98)
		)
	)
	(wire
		(pts
			(xy 151.13 111.76) (xy 151.13 119.38)
		)
	)
	(wire
		(pts
			(xy 124.46 161.29) (xy 129.54 161.29)
		)
	)
	(wire
		(pts
			(xy 129.54 97.79) (xy 129.54 99.06)
		)
	)
	(wire
		(pts
			(xy 259.08 57.15) (xy 266.7 57.15)
		)
	)
	(wire
		(pts
			(xy 114.3 105.41) (xy 114.3 92.71)
		)
	)
	(wire
		(pts
			(xy 121.92 151.13) (xy 92.71 151.13)
		)
	)
	(wire
		(pts
			(xy 63.5 124.46) (xy 73.66 124.46)
		)
	)
	(wire
		(pts
			(xy 129.54 125.73) (xy 116.84 125.73)
		)
	)
	(wire
		(pts
			(xy 124.46 107.95) (xy 124.46 105.41)
		)
	)
	(wire
		(pts
			(xy 71.12 132.08) (xy 124.46 132.08)
		)
	)
	(wire
		(pts
			(xy 241.3 123.19) (xy 241.3 124.46)
		)
	)
	(wire
		(pts
			(xy 71.12 127) (xy 71.12 132.08)
		)
	)
	(wire
		(pts
			(xy 233.68 45.72) (xy 246.38 45.72)
		)
	)
	(wire
		(pts
			(xy 243.84 149.86) (xy 251.46 149.86)
		)
	)
	(wire
		(pts
			(xy 124.46 138.43) (xy 124.46 132.08)
		)
	)
	(wire
		(pts
			(xy 73.66 116.84) (xy 76.2 116.84)
		)
	)
	(wire
		(pts
			(xy 68.58 151.13) (xy 68.58 168.91)
		)
	)
	(wire
		(pts
			(xy 144.78 142.24) (xy 153.67 142.24)
		)
	)
	(wire
		(pts
			(xy 124.46 128.27) (xy 124.46 115.57)
		)
	)
	(wire
		(pts
			(xy 121.92 140.97) (xy 121.92 151.13)
		)
	)
	(wire
		(pts
			(xy 76.2 116.84) (xy 77.47 116.84)
		)
	)
	(wire
		(pts
			(xy 228.6 35.56) (xy 228.6 34.29)
		)
	)
	(wire
		(pts
			(xy 168.91 132.08) (xy 168.91 134.62)
		)
	)
	(wire
		(pts
			(xy 236.22 132.08) (xy 236.22 134.62)
		)
	)
	(wire
		(pts
			(xy 76.2 173.99) (xy 76.2 116.84)
		)
	)
	(wire
		(pts
			(xy 199.39 46.99) (xy 199.39 49.53)
		)
	)
	(wire
		(pts
			(xy 73.66 121.92) (xy 73.66 116.84)
		)
	)
	(wire
		(pts
			(xy 129.54 143.51) (xy 129.54 146.05)
		)
	)
	(wire
		(pts
			(xy 176.53 45.72) (xy 176.53 46.99)
		)
	)
	(wire
		(pts
			(xy 73.66 124.46) (xy 73.66 128.27)
		)
	)
	(wire
		(pts
			(xy 41.91 58.42) (xy 48.26 58.42)
		)
	)
	(wire
		(pts
			(xy 129.54 143.51) (xy 114.3 143.51)
		)
	)
	(wire
		(pts
			(xy 199.39 45.72) (xy 199.39 46.99)
		)
	)
	(wire
		(pts
			(xy 92.71 105.41) (xy 114.3 105.41)
		)
	)
	(wire
		(pts
			(xy 153.67 172.72) (xy 153.67 152.4)
		)
	)
	(wire
		(pts
			(xy 43.18 124.46) (xy 43.18 125.73)
		)
	)
	(wire
		(pts
			(xy 224.79 125.73) (xy 224.79 124.46)
		)
	)
	(wire
		(pts
			(xy 121.92 99.06) (xy 121.92 123.19)
		)
	)
	(wire
		(pts
			(xy 92.71 139.7) (xy 106.68 139.7)
		)
	)
	(wire
		(pts
			(xy 57.15 49.53) (xy 57.15 44.45)
		)
	)
	(wire
		(pts
			(xy 228.6 34.29) (xy 246.38 34.29)
		)
	)
	(wire
		(pts
			(xy 114.3 105.41) (xy 124.46 105.41)
		)
	)
	(wire
		(pts
			(xy 63.5 121.92) (xy 73.66 121.92)
		)
	)
	(wire
		(pts
			(xy 129.54 156.21) (xy 109.22 156.21)
		)
	)
	(wire
		(pts
			(xy 199.39 38.1) (xy 191.77 38.1)
		)
	)
	(wire
		(pts
			(xy 71.12 105.41) (xy 77.47 105.41)
		)
	)
	(wire
		(pts
			(xy 168.91 46.99) (xy 176.53 46.99)
		)
	)
	(wire
		(pts
			(xy 129.54 107.95) (xy 124.46 107.95)
		)
	)
	(wire
		(pts
			(xy 168.91 45.72) (xy 168.91 46.99)
		)
	)
	(wire
		(pts
			(xy 168.91 119.38) (xy 168.91 132.08)
		)
	)
	(wire
		(pts
			(xy 106.68 158.75) (xy 129.54 158.75)
		)
	)
	(polyline
		(pts
			(xy 16.51 76.835) (xy 276.225 76.835)
		)
	)
	(wire
		(pts
			(xy 121.92 140.97) (xy 129.54 140.97)
		)
	)
	(wire
		(pts
			(xy 259.08 48.26) (xy 266.7 48.26)
		)
	)
	(wire
		(pts
			(xy 129.54 99.06) (xy 129.54 100.33)
		)
	)
	(wire
		(pts
			(xy 153.67 142.24) (xy 153.67 147.32)
		)
	)
	(wire
		(pts
			(xy 222.25 124.46) (xy 224.79 124.46)
		)
	)
	(wire
		(pts
			(xy 121.92 123.19) (xy 121.92 140.97)
		)
	)
	(wire
		(pts
			(xy 69.85 30.48) (xy 72.39 30.48)
		)
	)
	(polyline
		(pts
			(xy 210.185 16.51) (xy 210.185 76.2)
		)
	)
	(wire
		(pts
			(xy 68.58 129.54) (xy 68.58 151.13)
		)
	)
	(wire
		(pts
			(xy 144.78 111.76) (xy 151.13 111.76)
		)
	)
	(wire
		(pts
			(xy 121.92 99.06) (xy 129.54 99.06)
		)
	)
	(wire
		(pts
			(xy 129.54 171.45) (xy 106.68 171.45)
		)
	)
	(wire
		(pts
			(xy 129.54 153.67) (xy 111.76 153.67)
		)
	)
	(wire
		(pts
			(xy 168.91 38.1) (xy 161.29 38.1)
		)
	)
	(wire
		(pts
			(xy 129.54 138.43) (xy 124.46 138.43)
		)
	)
	(wire
		(pts
			(xy 72.39 30.48) (xy 72.39 29.21)
		)
	)
	(wire
		(pts
			(xy 116.84 116.84) (xy 116.84 125.73)
		)
	)
	(wire
		(pts
			(xy 50.8 58.42) (xy 50.8 45.72)
		)
	)
	(wire
		(pts
			(xy 57.15 29.21) (xy 57.15 33.02)
		)
	)
	(wire
		(pts
			(xy 161.29 46.99) (xy 168.91 46.99)
		)
	)
	(wire
		(pts
			(xy 161.29 45.72) (xy 161.29 46.99)
		)
	)
	(wire
		(pts
			(xy 129.54 107.95) (xy 129.54 110.49)
		)
	)
	(wire
		(pts
			(xy 247.65 139.7) (xy 243.84 139.7)
		)
	)
	(wire
		(pts
			(xy 63.5 127) (xy 71.12 127)
		)
	)
	(wire
		(pts
			(xy 116.84 95.25) (xy 129.54 95.25)
		)
	)
	(wire
		(pts
			(xy 168.91 137.16) (xy 168.91 149.86)
		)
	)
	(text_box "V_IN: MAX 40V "
		(exclude_from_sim no)
		(at 229.87 107.315 0)
		(size 20.32 4.445)
		(fill
			(type none)
		)
	)
	(text_box "CLK: 2Hz 50% duty cycle"
		(exclude_from_sim no)
		(at 233.045 22.86 0)
		(size 27.94 4.445)
		(fill
			(type none)
		)
	)
	(text_box "Place near IC VCC pins"
		(exclude_from_sim no)
		(at 167.64 30.48 0)
		(size 27.94 4.445)
		(fill
			(type none)
		)
	)
	(text_box "USB PWR: 5V 3A MAX"
		(exclude_from_sim no)
		(at 54.61 67.945 0)
		(size 27.94 4.445)
		(fill
			(type none)
		)
	)
	(text "Main Logic Circuit"
		(exclude_from_sim no)
		(at 18.542 85.598 0)
	)
	(text "Clock Generator"
		(exclude_from_sim no)
		(at 213.36 18.288 0)
	)
	(text "Power"
		(exclude_from_sim no)
		(at 17.018 17.78 0)
	)
	(text "Load / Output"
		(exclude_from_sim no)
		(at 213.868 85.852 0)
	)
	(global_label "SIG_OUT"
		(shape input)
		(at 247.65 139.7 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 258.3157 139.7 0)
		)
	)
	(global_label "CLK"
		(shape output)
		(at 259.08 43.18 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 265.6333 43.18 0)
		)
	)
	(global_label "CLK"
		(shape input)
		(at 40.64 125.73 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 34.0867 125.73 0)
		)
	)
	(global_label "SIG_OUT"
		(shape output)
		(at 185.42 134.62 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 196.0857 134.62 0)
		)
	)
	(global_label "SIG_OUT"
		(shape input)
		(at 259.08 100.33 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 248.4143 100.33 0)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 43.18 137.16 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR030"
			(at 36.83 137.16 0)
		)
		(property "Value" "GND"
			(at 39.37 137.1599 90)
		)
		(property "Footprint" ""
			(at 43.18 137.16 0)
		)
		(property "Datasheet" ""
			(at 43.18 137.16 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 43.18 137.16 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR030")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "74xx:74HC590A")
		(at 53.34 132.08 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U7"
			(at 55.5341 111.76 0)
		)
		(property "Value" "74HC590A"
			(at 55.5341 114.3 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 53.34 130.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74hc590a.pdf"
			(at 53.34 130.81 0)
		)
		(property "Description" "8-bit Binary Counter with Output Register 3-State Outputs, DIP-16/SOIC-16/SOIC-16W"
			(at 53.34 132.08 0)
		)
		(pin "6")
		(pin "9")
		(pin "5")
		(pin "3")
		(pin "2")
		(pin "16")
		(pin "8")
		(pin "1")
		(pin "14")
		(pin "7")
		(pin "12")
		(pin "11")
		(pin "10")
		(pin "15")
		(pin "13")
		(pin "4")
		(instances
			(project "sos_business_card"
				(path
					(reference "U7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x01_Pin")
		(at 62.23 49.53 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J2"
			(at 61.595 44.45 0)
		)
		(property "Value" "GND"
			(at 61.595 46.99 0)
		)
		(property "Footprint" "MountingHole:MountingHole_2.5mm_Pad_TopBottom"
			(at 62.23 49.53 0)
		)
		(property "Datasheet" "~"
			(at 62.23 49.53 0)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 62.23 49.53 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "J2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 228.6 48.26 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR010"
			(at 222.25 48.26 0)
		)
		(property "Value" "GND"
			(at 224.79 48.2599 90)
		)
		(property "Footprint" ""
			(at 228.6 48.26 0)
		)
		(property "Datasheet" ""
			(at 228.6 48.26 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 228.6 48.26 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR010")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 161.29 43.18 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C2"
			(at 157.734 40.132 0)
		)
		(property "Value" "100n"
			(at 164.338 45.212 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 161.29 43.18 0)
		)
		(property "Datasheet" "~"
			(at 161.29 43.18 0)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 161.29 43.18 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "C2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "4xxx:4075")
		(at 143.51 41.91 0)
		(unit 4)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U5"
			(at 144.272 32.766 0)
		)
		(property "Value" "SN74HCS4075"
			(at 150.622 48.768 90)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 143.51 41.91 0)
		)
		(property "Datasheet" "https://www.ti.com/cn/lit/ds/symlink/sn74hcs4075.pdf"
			(at 143.51 41.91 0)
		)
		(property "Description" "Triple Or 3 inputs"
			(at 143.51 41.91 0)
		)
		(pin "4")
		(pin "12")
		(pin "10")
		(pin "7")
		(pin "9")
		(pin "8")
		(pin "11")
		(pin "2")
		(pin "1")
		(pin "14")
		(pin "3")
		(pin "13")
		(pin "5")
		(pin "6")
		(instances
			(project "sos_business_card"
				(path
					(reference "U5")
					(unit 4)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 176.53 43.18 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C4"
			(at 172.974 40.132 0)
		)
		(property "Value" "100n"
			(at 179.578 45.212 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 176.53 43.18 0)
		)
		(property "Datasheet" "~"
			(at 176.53 43.18 0)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 176.53 43.18 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "C4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 246.38 34.29 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR07"
			(at 246.38 38.1 0)
		)
		(property "Value" "VCC"
			(at 246.38 29.21 0)
		)
		(property "Footprint" ""
			(at 246.38 34.29 0)
		)
		(property "Datasheet" ""
			(at 246.38 34.29 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 246.38 34.29 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR07")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 97.79 29.21 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR03"
			(at 97.79 33.02 0)
		)
		(property "Value" "VCC"
			(at 97.79 24.13 0)
		)
		(property "Footprint" ""
			(at 97.79 29.21 0)
		)
		(property "Datasheet" ""
			(at 97.79 29.21 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 97.79 29.21 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "4xxx:4075")
		(at 176.53 134.62 0)
		(unit 3)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U5"
			(at 176.53 125.73 0)
		)
		(property "Value" "SN74HCS4075"
			(at 176.53 128.27 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 176.53 134.62 0)
		)
		(property "Datasheet" "https://www.ti.com/cn/lit/ds/symlink/sn74hcs4075.pdf"
			(at 176.53 134.62 0)
		)
		(property "Description" "Triple Or 3 inputs"
			(at 176.53 134.62 0)
		)
		(pin "4")
		(pin "12")
		(pin "10")
		(pin "7")
		(pin "9")
		(pin "8")
		(pin "11")
		(pin "2")
		(pin "1")
		(pin "14")
		(pin "3")
		(pin "13")
		(pin "5")
		(pin "6")
		(instances
			(project "sos_business_card"
				(path
					(reference "U5")
					(unit 3)
				)
			)
		)
	)
	(symbol
		(lib_id "74xx:74LS21")
		(at 128.27 41.91 0)
		(unit 3)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U4"
			(at 129.54 32.766 0)
		)
		(property "Value" "SN74HC21QDRQ1"
			(at 135.128 49.784 90)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 128.27 41.91 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74hc21-q1.pdf"
			(at 128.27 41.91 0)
		)
		(property "Description" "Dual 4-input AND"
			(at 128.27 41.91 0)
		)
		(pin "8")
		(pin "2")
		(pin "7")
		(pin "6")
		(pin "5")
		(pin "1")
		(pin "4")
		(pin "9")
		(pin "12")
		(pin "13")
		(pin "10")
		(pin "14")
		(instances
			(project "sos_business_card"
				(path
					(reference "U4")
					(unit 3)
				)
			)
		)
	)
	(symbol
		(lib_id "74xx:74LV14")
		(at 85.09 128.27 0)
		(unit 3)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U1"
			(at 88.392 125.73 0)
		)
		(property "Value" "SN74LV04A"
			(at 84.836 122.936 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 85.09 128.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LV04a"
			(at 85.09 128.27 0)
		)
		(property "Description" "Hex Inverter"
			(at 85.09 128.27 0)
		)
		(pin "14")
		(pin "13")
		(pin "7")
		(pin "10")
		(pin "6")
		(pin "2")
		(pin "4")
		(pin "9")
		(pin "8")
		(pin "1")
		(pin "3")
		(pin "5")
		(pin "12")
		(pin "11")
		(instances
			(project "sos_business_card"
				(path
					(reference "U1")
					(unit 3)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 143.51 54.61 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR018"
			(at 143.51 60.96 0)
		)
		(property "Value" "GND"
			(at 143.51 59.69 0)
		)
		(property "Footprint" ""
			(at 143.51 54.61 0)
		)
		(property "Datasheet" ""
			(at 143.51 54.61 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 143.51 54.61 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR018")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Transistor_FET:BSS138")
		(at 264.16 100.33 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "Q1"
			(at 270.51 99.0599 0)
		)
		(property "Value" "BSS138"
			(at 270.51 101.5999 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 269.24 102.235 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BSS138-D.PDF"
			(at 269.24 104.14 0)
		)
		(property "Description" "50V Vds, 0.22A Id, N-Channel MOSFET, SOT-23"
			(at 264.16 100.33 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "sos_business_card"
				(path
					(reference "Q1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 184.15 43.18 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C5"
			(at 180.594 40.132 0)
		)
		(property "Value" "100n"
			(at 187.198 45.212 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 184.15 43.18 0)
		)
		(property "Datasheet" "~"
			(at 184.15 43.18 0)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 184.15 43.18 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "C5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 50.8 62.23 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R4"
			(at 53.34 60.9599 0)
		)
		(property "Value" "5.1k"
			(at 53.34 63.4999 0)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 49.022 62.23 90)
		)
		(property "Datasheet" "~"
			(at 50.8 62.23 0)
		)
		(property "Description" "Resistor"
			(at 50.8 62.23 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "sos_business_card"
				(path
					(reference "R4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "74xx:74LS21")
		(at 137.16 127 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U3"
			(at 137.1503 118.11 0)
		)
		(property "Value" "SN74HC21QDRQ1"
			(at 137.1503 120.65 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 137.16 127 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74hc21-q1.pdf"
			(at 137.16 127 0)
		)
		(property "Description" "Dual 4-input AND"
			(at 137.16 127 0)
		)
		(pin "8")
		(pin "2")
		(pin "7")
		(pin "6")
		(pin "5")
		(pin "1")
		(pin "4")
		(pin "9")
		(pin "12")
		(pin "13")
		(pin "10")
		(pin "14")
		(instances
			(project "sos_business_card"
				(path
					(reference "U3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 228.6 38.1 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C1"
			(at 223.266 36.068 0)
		)
		(property "Value" "100n"
			(at 222.758 40.132 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 228.6 38.1 0)
		)
		(property "Datasheet" "~"
			(at 228.6 38.1 0)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 228.6 38.1 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "C1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 199.39 49.53 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR012"
			(at 199.39 55.88 0)
		)
		(property "Value" "GND"
			(at 199.39 54.61 0)
		)
		(property "Footprint" ""
			(at 199.39 49.53 0)
		)
		(property "Datasheet" ""
			(at 199.39 49.53 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 199.39 49.53 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR012")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 97.79 54.61 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR015"
			(at 97.79 60.96 0)
		)
		(property "Value" "GND"
			(at 97.79 59.69 0)
		)
		(property "Footprint" ""
			(at 97.79 54.61 0)
		)
		(property "Datasheet" ""
			(at 97.79 54.61 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 97.79 54.61 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR015")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "74xx:74LS21")
		(at 137.16 172.72 0)
		(unit 2)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U4"
			(at 137.1503 163.83 0)
		)
		(property "Value" "SN74HC21QDRQ1"
			(at 137.1503 166.37 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 137.16 172.72 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74hc21-q1.pdf"
			(at 137.16 172.72 0)
		)
		(property "Description" "Dual 4-input AND"
			(at 137.16 172.72 0)
		)
		(pin "8")
		(pin "2")
		(pin "7")
		(pin "6")
		(pin "5")
		(pin "1")
		(pin "4")
		(pin "9")
		(pin "12")
		(pin "13")
		(pin "10")
		(pin "14")
		(instances
			(project "sos_business_card"
				(path
					(reference "U4")
					(unit 2)
				)
			)
		)
	)
	(symbol
		(lib_id "74xx:74LV14")
		(at 85.09 116.84 0)
		(unit 2)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U1"
			(at 88.392 113.792 0)
		)
		(property "Value" "SN74LV04A"
			(at 85.09 111.252 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 85.09 116.84 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LV04a"
			(at 85.09 116.84 0)
		)
		(property "Description" "Hex Inverter"
			(at 85.09 116.84 0)
		)
		(pin "14")
		(pin "13")
		(pin "7")
		(pin "10")
		(pin "6")
		(pin "2")
		(pin "4")
		(pin "9")
		(pin "8")
		(pin "1")
		(pin "3")
		(pin "5")
		(pin "12")
		(pin "11")
		(instances
			(project "sos_business_card"
				(path
					(reference "U1")
					(unit 2)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 266.7 59.69 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C9"
			(at 269.24 58.4135 0)
		)
		(property "Value" "330n"
			(at 269.24 60.9535 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 266.7 59.69 0)
		)
		(property "Datasheet" "~"
			(at 266.7 59.69 0)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 266.7 59.69 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "C9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 50.8 66.04 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR023"
			(at 50.8 72.39 0)
		)
		(property "Value" "GND"
			(at 50.8 71.12 0)
		)
		(property "Footprint" ""
			(at 50.8 66.04 0)
		)
		(property "Datasheet" ""
			(at 50.8 66.04 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 50.8 66.04 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR023")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 53.34 147.32 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR032"
			(at 53.34 153.67 0)
		)
		(property "Value" "GND"
			(at 53.34 152.4 0)
		)
		(property "Footprint" ""
			(at 53.34 147.32 0)
		)
		(property "Datasheet" ""
			(at 53.34 147.32 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 53.34 147.32 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR032")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "74xx:74LV14")
		(at 85.09 105.41 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U1"
			(at 88.392 102.108 0)
		)
		(property "Value" "SN74LV04A"
			(at 84.836 99.822 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 85.09 105.41 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LV04a"
			(at 85.09 105.41 0)
		)
		(property "Description" "Hex Inverter"
			(at 85.09 105.41 0)
		)
		(pin "14")
		(pin "13")
		(pin "7")
		(pin "10")
		(pin "6")
		(pin "2")
		(pin "4")
		(pin "9")
		(pin "8")
		(pin "1")
		(pin "3")
		(pin "5")
		(pin "12")
		(pin "11")
		(instances
			(project "sos_business_card"
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x01_Pin")
		(at 250.19 123.19 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J3"
			(at 249.555 118.11 0)
		)
		(property "Value" "V_OUT"
			(at 249.555 120.65 0)
		)
		(property "Footprint" "MountingHole:MountingHole_2.5mm_Pad_TopBottom"
			(at 250.19 123.19 0)
		)
		(property "Datasheet" "~"
			(at 250.19 123.19 0)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 250.19 123.19 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "J3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 246.38 58.42 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR019"
			(at 246.38 64.77 0)
		)
		(property "Value" "GND"
			(at 246.38 63.5 0)
		)
		(property "Footprint" ""
			(at 246.38 58.42 0)
		)
		(property "Datasheet" ""
			(at 246.38 58.42 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 246.38 58.42 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR019")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 224.79 113.03 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR025"
			(at 224.79 116.84 0)
		)
		(property "Value" "PWR"
			(at 224.79 107.95 0)
		)
		(property "Footprint" ""
			(at 224.79 113.03 0)
		)
		(property "Datasheet" ""
			(at 224.79 113.03 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 224.79 113.03 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR025")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 266.7 120.65 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR028"
			(at 266.7 127 0)
		)
		(property "Value" "GND"
			(at 266.7 125.73 0)
		)
		(property "Footprint" ""
			(at 266.7 120.65 0)
		)
		(property "Datasheet" ""
			(at 266.7 120.65 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 266.7 120.65 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR028")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 224.79 129.54 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R6"
			(at 227.33 128.2699 0)
		)
		(property "Value" "100k"
			(at 227.33 130.8099 0)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 223.012 129.54 90)
		)
		(property "Datasheet" "~"
			(at 224.79 129.54 0)
		)
		(property "Description" "Resistor"
			(at 224.79 129.54 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "sos_business_card"
				(path
					(reference "R6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x01_Pin")
		(at 256.54 149.86 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J5"
			(at 255.905 144.78 0)
		)
		(property "Value" "GND"
			(at 255.905 147.32 0)
		)
		(property "Footprint" "MountingHole:MountingHole_2.5mm_Pad_TopBottom"
			(at 256.54 149.86 0)
		)
		(property "Datasheet" "~"
			(at 256.54 149.86 0)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 256.54 149.86 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "J5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 199.39 43.18 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C7"
			(at 195.834 40.132 0)
		)
		(property "Value" "100n"
			(at 202.438 45.212 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 199.39 43.18 0)
		)
		(property "Datasheet" "~"
			(at 199.39 43.18 0)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 199.39 43.18 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "C7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 128.27 29.21 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR05"
			(at 128.27 33.02 0)
		)
		(property "Value" "VCC"
			(at 128.27 24.13 0)
		)
		(property "Footprint" ""
			(at 128.27 29.21 0)
		)
		(property "Datasheet" ""
			(at 128.27 29.21 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 128.27 29.21 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR05")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "74xx:74LS21")
		(at 97.79 41.91 0)
		(unit 3)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U2"
			(at 99.06 32.766 0)
		)
		(property "Value" "SN74HC21QDRQ1"
			(at 104.902 49.53 90)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 97.79 41.91 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74hc21-q1.pdf"
			(at 97.79 41.91 0)
		)
		(property "Description" "Dual 4-input AND"
			(at 97.79 41.91 0)
		)
		(pin "8")
		(pin "2")
		(pin "7")
		(pin "6")
		(pin "5")
		(pin "1")
		(pin "4")
		(pin "9")
		(pin "12")
		(pin "13")
		(pin "10")
		(pin "14")
		(instances
			(project "sos_business_card"
				(path
					(reference "U2")
					(unit 3)
				)
			)
		)
	)
	(symbol
		(lib_id "74xx:74LV14")
		(at 82.55 41.91 0)
		(unit 7)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U1"
			(at 83.82 32.766 0)
		)
		(property "Value" "SN74LV04A"
			(at 89.662 46.99 90)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 82.55 41.91 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LV04a"
			(at 82.55 41.91 0)
		)
		(property "Description" "Hex Inverter"
			(at 82.55 41.91 0)
		)
		(pin "14")
		(pin "13")
		(pin "7")
		(pin "10")
		(pin "6")
		(pin "2")
		(pin "4")
		(pin "9")
		(pin "8")
		(pin "1")
		(pin "3")
		(pin "5")
		(pin "12")
		(pin "11")
		(instances
			(project "sos_business_card"
				(path
					(reference "U1")
					(unit 7)
				)
			)
		)
	)
	(symbol
		(lib_id "74xx:74LV14")
		(at 85.09 151.13 0)
		(unit 5)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U1"
			(at 88.646 148.336 0)
		)
		(property "Value" "SN74LV04A"
			(at 85.09 145.542 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 85.09 151.13 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LV04a"
			(at 85.09 151.13 0)
		)
		(property "Description" "Hex Inverter"
			(at 85.09 151.13 0)
		)
		(pin "14")
		(pin "13")
		(pin "7")
		(pin "10")
		(pin "6")
		(pin "2")
		(pin "4")
		(pin "9")
		(pin "8")
		(pin "1")
		(pin "3")
		(pin "5")
		(pin "12")
		(pin "11")
		(instances
			(project "sos_business_card"
				(path
					(reference "U1")
					(unit 5)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 266.7 43.18 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 269.24 41.9099 0)
		)
		(property "Value" "10k"
			(at 269.24 44.4499 0)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 264.922 43.18 90)
		)
		(property "Datasheet" "~"
			(at 266.7 43.18 0)
		)
		(property "Description" "Resistor"
			(at 266.7 43.18 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "sos_business_card"
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "74xx:74LS21")
		(at 137.16 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U2"
			(at 137.1503 87.63 0)
		)
		(property "Value" "SN74HC21QDRQ1"
			(at 137.1503 90.17 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 137.16 96.52 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74hc21-q1.pdf"
			(at 137.16 96.52 0)
		)
		(property "Description" "Dual 4-input AND"
			(at 137.16 96.52 0)
		)
		(pin "8")
		(pin "2")
		(pin "7")
		(pin "6")
		(pin "5")
		(pin "1")
		(pin "4")
		(pin "9")
		(pin "12")
		(pin "13")
		(pin "10")
		(pin "14")
		(instances
			(project "sos_business_card"
				(path
					(reference "U2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 236.22 151.13 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR033"
			(at 236.22 157.48 0)
		)
		(property "Value" "GND"
			(at 236.22 156.21 0)
		)
		(property "Footprint" ""
			(at 236.22 151.13 0)
		)
		(property "Datasheet" ""
			(at 236.22 151.13 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 236.22 151.13 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR033")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 113.03 29.21 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR04"
			(at 113.03 33.02 0)
		)
		(property "Value" "VCC"
			(at 113.03 24.13 0)
		)
		(property "Footprint" ""
			(at 113.03 29.21 0)
		)
		(property "Datasheet" ""
			(at 113.03 29.21 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 113.03 29.21 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:Battery_Cell")
		(at 57.15 41.91 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "BT1"
			(at 60.96 38.7984 0)
		)
		(property "Value" "Battery_Cell"
			(at 60.96 41.3384 0)
		)
		(property "Footprint" "Battery:BatteryHolder_Keystone_3034_1x20mm"
			(at 57.15 40.386 90)
		)
		(property "Datasheet" "~"
			(at 57.15 40.386 90)
		)
		(property "Description" "Single-cell battery"
			(at 57.15 41.91 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "sos_business_card"
				(path
					(reference "BT1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 266.7 116.84 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R5"
			(at 269.24 115.5699 0)
		)
		(property "Value" "100"
			(at 269.24 118.1099 0)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 264.922 116.84 90)
		)
		(property "Datasheet" "~"
			(at 266.7 116.84 0)
		)
		(property "Description" "Resistor"
			(at 266.7 116.84 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "sos_business_card"
				(path
					(reference "R5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 161.29 38.1 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR09"
			(at 161.29 41.91 0)
		)
		(property "Value" "VCC"
			(at 161.29 33.02 0)
		)
		(property "Footprint" ""
			(at 161.29 38.1 0)
		)
		(property "Datasheet" ""
			(at 161.29 38.1 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 161.29 38.1 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR09")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "4xxx:4075")
		(at 161.29 119.38 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U5"
			(at 161.29 110.49 0)
		)
		(property "Value" "SN74HCS4075"
			(at 161.29 113.03 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 161.29 119.38 0)
		)
		(property "Datasheet" "https://www.ti.com/cn/lit/ds/symlink/sn74hcs4075.pdf"
			(at 161.29 119.38 0)
		)
		(property "Description" "Triple Or 3 inputs"
			(at 161.29 119.38 0)
		)
		(pin "4")
		(pin "12")
		(pin "10")
		(pin "7")
		(pin "9")
		(pin "8")
		(pin "11")
		(pin "2")
		(pin "1")
		(pin "14")
		(pin "3")
		(pin "13")
		(pin "5")
		(pin "6")
		(instances
			(project "sos_business_card"
				(path
					(reference "U5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 82.55 54.61 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR014"
			(at 82.55 60.96 0)
		)
		(property "Value" "GND"
			(at 82.55 59.69 0)
		)
		(property "Footprint" ""
			(at 82.55 54.61 0)
		)
		(property "Datasheet" ""
			(at 82.55 54.61 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 82.55 54.61 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR014")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 233.68 53.34 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR013"
			(at 237.49 53.34 0)
		)
		(property "Value" "VCC"
			(at 229.87 53.3399 90)
		)
		(property "Footprint" ""
			(at 233.68 53.34 0)
		)
		(property "Datasheet" ""
			(at 233.68 53.34 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 233.68 53.34 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR013")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Transistor_FET:BSS138")
		(at 238.76 139.7 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "Q3"
			(at 232.41 138.4299 0)
		)
		(property "Value" "BSS138"
			(at 232.41 140.9699 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 233.68 141.605 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BSS138-D.PDF"
			(at 233.68 143.51 0)
		)
		(property "Description" "50V Vds, 0.22A Id, N-Channel MOSFET, SOT-23"
			(at 238.76 139.7 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "sos_business_card"
				(path
					(reference "Q3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 168.91 43.18 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C3"
			(at 165.354 40.132 0)
		)
		(property "Value" "100n"
			(at 171.958 45.212 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 168.91 43.18 0)
		)
		(property "Datasheet" "~"
			(at 168.91 43.18 0)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 168.91 43.18 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "C3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 191.77 43.18 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C6"
			(at 188.214 40.132 0)
		)
		(property "Value" "100n"
			(at 194.818 45.212 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 191.77 43.18 0)
		)
		(property "Datasheet" "~"
			(at 191.77 43.18 0)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 191.77 43.18 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "C6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Timer:TLC555xD")
		(at 246.38 48.26 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U6"
			(at 248.5741 35.56 0)
		)
		(property "Value" "TLC555"
			(at 248.5741 38.1 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 267.97 58.42 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlc555.pdf"
			(at 267.97 58.42 0)
		)
		(property "Description" "Single LinCMOS Timer, 555 compatible, SOIC-8"
			(at 246.38 48.26 0)
		)
		(pin "2")
		(pin "4")
		(pin "3")
		(pin "8")
		(pin "5")
		(pin "7")
		(pin "1")
		(pin "6")
		(instances
			(project "sos_business_card"
				(path
					(reference "U6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 72.39 29.21 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 72.39 33.02 0)
		)
		(property "Value" "VCC"
			(at 72.39 24.13 0)
		)
		(property "Footprint" ""
			(at 72.39 29.21 0)
		)
		(property "Datasheet" ""
			(at 72.39 29.21 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 72.39 29.21 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 41.91 62.23 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R3"
			(at 44.45 60.9599 0)
		)
		(property "Value" "5.1k"
			(at 44.45 63.4999 0)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 40.132 62.23 90)
		)
		(property "Datasheet" "~"
			(at 41.91 62.23 0)
		)
		(property "Description" "Resistor"
			(at 41.91 62.23 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "sos_business_card"
				(path
					(reference "R3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 266.7 62.23 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR020"
			(at 266.7 68.58 0)
		)
		(property "Value" "GND"
			(at 266.7 67.31 0)
		)
		(property "Footprint" ""
			(at 266.7 62.23 0)
		)
		(property "Datasheet" ""
			(at 266.7 62.23 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 266.7 62.23 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR020")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 231.14 48.26 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C8"
			(at 231.1463 41.91 90)
		)
		(property "Value" "10n"
			(at 231.1463 44.45 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 231.14 48.26 0)
		)
		(property "Datasheet" "~"
			(at 231.14 48.26 0)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 231.14 48.26 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "C8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 243.84 144.78 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R7"
			(at 246.38 143.5099 0)
		)
		(property "Value" "100k"
			(at 246.38 146.0499 0)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 242.062 144.78 90)
		)
		(property "Datasheet" "~"
			(at 243.84 144.78 0)
		)
		(property "Description" "Resistor"
			(at 243.84 144.78 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "sos_business_card"
				(path
					(reference "R7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:LED")
		(at 266.7 109.22 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D1"
			(at 270.51 109.5374 90)
		)
		(property "Value" "LED"
			(at 270.51 112.0774 90)
		)
		(property "Footprint" "LED_SMD:LED_1206_3216Metric"
			(at 266.7 109.22 0)
		)
		(property "Datasheet" "~"
			(at 266.7 109.22 0)
		)
		(property "Description" "Light emitting diode"
			(at 266.7 109.22 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "74xx:74LS21")
		(at 113.03 41.91 0)
		(unit 3)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U3"
			(at 114.3 32.766 0)
		)
		(property "Value" "SN74HC21QDRQ1"
			(at 120.142 49.784 90)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 113.03 41.91 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74hc21-q1.pdf"
			(at 113.03 41.91 0)
		)
		(property "Description" "Dual 4-input AND"
			(at 113.03 41.91 0)
		)
		(pin "8")
		(pin "2")
		(pin "7")
		(pin "6")
		(pin "5")
		(pin "1")
		(pin "4")
		(pin "9")
		(pin "12")
		(pin "13")
		(pin "10")
		(pin "14")
		(instances
			(project "sos_business_card"
				(path
					(reference "U3")
					(unit 3)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 266.7 53.34 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R2"
			(at 269.24 52.0699 0)
		)
		(property "Value" "1M"
			(at 269.24 54.6099 0)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 264.922 53.34 90)
		)
		(property "Datasheet" "~"
			(at 266.7 53.34 0)
		)
		(property "Description" "Resistor"
			(at 266.7 53.34 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "sos_business_card"
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x01_Pin")
		(at 217.17 124.46 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J4"
			(at 217.805 119.38 0)
		)
		(property "Value" "V_IN"
			(at 217.805 121.92 0)
		)
		(property "Footprint" "MountingHole:MountingHole_2.5mm_Pad_TopBottom"
			(at 217.17 124.46 0)
		)
		(property "Datasheet" "~"
			(at 217.17 124.46 0)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 217.17 124.46 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "J4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 77.47 162.56 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR034"
			(at 81.28 162.56 0)
		)
		(property "Value" "VCC"
			(at 73.66 162.5599 90)
		)
		(property "Footprint" ""
			(at 77.47 162.56 0)
		)
		(property "Datasheet" ""
			(at 77.47 162.56 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 77.47 162.56 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR034")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 43.18 132.08 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR029"
			(at 46.99 132.08 0)
		)
		(property "Value" "VCC"
			(at 39.37 132.0799 90)
		)
		(property "Footprint" ""
			(at 43.18 132.08 0)
		)
		(property "Datasheet" ""
			(at 43.18 132.08 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 43.18 132.08 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR029")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 113.03 54.61 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR016"
			(at 113.03 60.96 0)
		)
		(property "Value" "GND"
			(at 113.03 59.69 0)
		)
		(property "Footprint" ""
			(at 113.03 54.61 0)
		)
		(property "Datasheet" ""
			(at 113.03 54.61 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 113.03 54.61 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR016")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 143.51 29.21 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR06"
			(at 143.51 33.02 0)
		)
		(property "Value" "VCC"
			(at 143.51 24.13 0)
		)
		(property "Footprint" ""
			(at 143.51 29.21 0)
		)
		(property "Datasheet" ""
			(at 143.51 29.21 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 143.51 29.21 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR06")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 43.18 119.38 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR027"
			(at 36.83 119.38 0)
		)
		(property "Value" "GND"
			(at 39.37 119.3799 90)
		)
		(property "Footprint" ""
			(at 43.18 119.38 0)
		)
		(property "Datasheet" ""
			(at 43.18 119.38 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 43.18 119.38 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR027")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 82.55 29.21 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR02"
			(at 82.55 33.02 0)
		)
		(property "Value" "VCC"
			(at 82.55 24.13 0)
		)
		(property "Footprint" ""
			(at 82.55 29.21 0)
		)
		(property "Datasheet" ""
			(at 82.55 29.21 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 82.55 29.21 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 57.15 29.21 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR035"
			(at 57.15 33.02 0)
		)
		(property "Value" "PWR"
			(at 57.15 24.13 0)
		)
		(property "Footprint" ""
			(at 57.15 29.21 0)
		)
		(property "Datasheet" ""
			(at 57.15 29.21 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 57.15 29.21 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR035")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 64.77 142.24 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR031"
			(at 60.96 142.24 0)
		)
		(property "Value" "VCC"
			(at 68.58 142.2399 90)
		)
		(property "Footprint" ""
			(at 64.77 142.24 0)
		)
		(property "Datasheet" ""
			(at 64.77 142.24 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 64.77 142.24 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR031")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:Q_PMOS_GDSD")
		(at 236.22 127 270)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "Q2"
			(at 232.156 118.364 90)
		)
		(property "Value" "IRF5305"
			(at 234.696 120.65 90)
		)
		(property "Footprint" "my:TO-220-3_Horizontal_TabDown_2"
			(at 238.76 121.92 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IRF5305-DataSheet-v01_01-EN.pdf?fileId=5546d462533600a4015355e370101993"
			(at 236.22 127 0)
		)
		(property "Description" "P-MOSFET transistor, gate/drain/source, drain connected to mounting plane"
			(at 236.22 127 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(instances
			(project "sos_business_card"
				(path
					(reference "Q2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:MBRA340")
		(at 224.79 116.84 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "D2"
			(at 227.076 113.792 90)
		)
		(property "Value" "MBRS540T3G"
			(at 227.076 115.824 90)
		)
		(property "Footprint" "Diode_SMD:D_SMC"
			(at 229.235 116.84 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/mbrs540t3-d.pdf"
			(at 224.79 116.84 0)
		)
		(property "Description" "40V 5A Schottky Barrier Rectifier Diode, SMC"
			(at 224.79 116.84 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "sos_business_card"
				(path
					(reference "D2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 53.34 114.3 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR026"
			(at 53.34 118.11 0)
		)
		(property "Value" "VCC"
			(at 53.34 109.22 0)
		)
		(property "Footprint" ""
			(at 53.34 114.3 0)
		)
		(property "Datasheet" ""
			(at 53.34 114.3 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 53.34 114.3 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR026")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "4xxx:4075")
		(at 161.29 149.86 0)
		(unit 2)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U5"
			(at 161.29 140.97 0)
		)
		(property "Value" "SN74HCS4075"
			(at 161.29 143.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 161.29 149.86 0)
		)
		(property "Datasheet" "https://www.ti.com/cn/lit/ds/symlink/sn74hcs4075.pdf"
			(at 161.29 149.86 0)
		)
		(property "Description" "Triple Or 3 inputs"
			(at 161.29 149.86 0)
		)
		(pin "4")
		(pin "12")
		(pin "10")
		(pin "7")
		(pin "9")
		(pin "8")
		(pin "11")
		(pin "2")
		(pin "1")
		(pin "14")
		(pin "3")
		(pin "13")
		(pin "5")
		(pin "6")
		(instances
			(project "sos_business_card"
				(path
					(reference "U5")
					(unit 2)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 266.7 34.29 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR08"
			(at 266.7 38.1 0)
		)
		(property "Value" "VCC"
			(at 266.7 29.21 0)
		)
		(property "Footprint" ""
			(at 266.7 34.29 0)
		)
		(property "Datasheet" ""
			(at 266.7 34.29 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 266.7 34.29 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR08")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "74xx:74LV14")
		(at 85.09 162.56 0)
		(unit 6)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U1"
			(at 88.9 159.766 0)
		)
		(property "Value" "SN74LV04A"
			(at 85.09 157.226 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 85.09 162.56 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LV04a"
			(at 85.09 162.56 0)
		)
		(property "Description" "Hex Inverter"
			(at 85.09 162.56 0)
		)
		(pin "14")
		(pin "13")
		(pin "7")
		(pin "10")
		(pin "6")
		(pin "2")
		(pin "4")
		(pin "9")
		(pin "8")
		(pin "1")
		(pin "3")
		(pin "5")
		(pin "12")
		(pin "11")
		(instances
			(project "sos_business_card"
				(path
					(reference "U1")
					(unit 6)
				)
			)
		)
	)
	(symbol
		(lib_id "74xx:74LS21")
		(at 137.16 142.24 0)
		(unit 2)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U3"
			(at 137.1503 133.35 0)
		)
		(property "Value" "SN74HC21QDRQ1"
			(at 137.1503 135.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 137.16 142.24 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74hc21-q1.pdf"
			(at 137.16 142.24 0)
		)
		(property "Description" "Dual 4-input AND"
			(at 137.16 142.24 0)
		)
		(pin "8")
		(pin "2")
		(pin "7")
		(pin "6")
		(pin "5")
		(pin "1")
		(pin "4")
		(pin "9")
		(pin "12")
		(pin "13")
		(pin "10")
		(pin "14")
		(instances
			(project "sos_business_card"
				(path
					(reference "U3")
					(unit 2)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 128.27 54.61 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR017"
			(at 128.27 60.96 0)
		)
		(property "Value" "GND"
			(at 128.27 59.69 0)
		)
		(property "Footprint" ""
			(at 128.27 54.61 0)
		)
		(property "Datasheet" ""
			(at 128.27 54.61 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 128.27 54.61 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR017")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "74xx:74LV14")
		(at 85.09 139.7 0)
		(unit 4)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U1"
			(at 88.646 136.906 0)
		)
		(property "Value" "SN74LV04A"
			(at 85.09 134.112 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 85.09 139.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LV04a"
			(at 85.09 139.7 0)
		)
		(property "Description" "Hex Inverter"
			(at 85.09 139.7 0)
		)
		(pin "14")
		(pin "13")
		(pin "7")
		(pin "10")
		(pin "6")
		(pin "2")
		(pin "4")
		(pin "9")
		(pin "8")
		(pin "1")
		(pin "3")
		(pin "5")
		(pin "12")
		(pin "11")
		(instances
			(project "sos_business_card"
				(path
					(reference "U1")
					(unit 4)
				)
			)
		)
	)
	(symbol
		(lib_id "74xx:74LS21")
		(at 137.16 157.48 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U4"
			(at 137.1503 148.59 0)
		)
		(property "Value" "SN74HC21QDRQ1"
			(at 137.1503 151.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 137.16 157.48 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74hc21-q1.pdf"
			(at 137.16 157.48 0)
		)
		(property "Description" "Dual 4-input AND"
			(at 137.16 157.48 0)
		)
		(pin "8")
		(pin "2")
		(pin "7")
		(pin "6")
		(pin "5")
		(pin "1")
		(pin "4")
		(pin "9")
		(pin "12")
		(pin "13")
		(pin "10")
		(pin "14")
		(instances
			(project "sos_business_card"
				(path
					(reference "U4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:USB_C_Receptacle_PowerOnly_6P")
		(at 33.02 40.64 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J1"
			(at 33.02 22.86 0)
		)
		(property "Value" "USB_C_Receptacle_PowerOnly_6P"
			(at 33.02 25.4 0)
		)
		(property "Footprint" "Connector_USB:USB_C_Receptacle_GCT_USB4125-xx-x_6P_TopMnt_Horizontal"
			(at 36.83 38.1 0)
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 33.02 40.64 0)
		)
		(property "Description" "USB Power-Only 6P Type-C Receptacle connector"
			(at 33.02 40.64 0)
		)
		(pin "S1")
		(pin "B5")
		(pin "B9")
		(pin "A12")
		(pin "A5")
		(pin "A9")
		(pin "B12")
		(instances
			(project "sos_business_card"
				(path
					(reference "J1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 41.91 66.04 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR022"
			(at 41.91 72.39 0)
		)
		(property "Value" "GND"
			(at 41.91 71.12 0)
		)
		(property "Footprint" ""
			(at 41.91 66.04 0)
		)
		(property "Datasheet" ""
			(at 41.91 66.04 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 41.91 66.04 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR022")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 57.15 49.53 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR011"
			(at 57.15 55.88 0)
		)
		(property "Value" "GND"
			(at 57.15 54.61 0)
		)
		(property "Footprint" ""
			(at 57.15 49.53 0)
		)
		(property "Datasheet" ""
			(at 57.15 49.53 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 57.15 49.53 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR011")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "74xx:74LS21")
		(at 137.16 111.76 0)
		(unit 2)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U2"
			(at 137.1503 102.87 0)
		)
		(property "Value" "SN74HC21QDRQ1"
			(at 137.1503 105.41 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 137.16 111.76 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74hc21-q1.pdf"
			(at 137.16 111.76 0)
		)
		(property "Description" "Dual 4-input AND"
			(at 137.16 111.76 0)
		)
		(pin "8")
		(pin "2")
		(pin "7")
		(pin "6")
		(pin "5")
		(pin "1")
		(pin "4")
		(pin "9")
		(pin "12")
		(pin "13")
		(pin "10")
		(pin "14")
		(instances
			(project "sos_business_card"
				(path
					(reference "U2")
					(unit 2)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_SPDT")
		(at 64.77 33.02 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW1"
			(at 64.77 24.13 0)
		)
		(property "Value" "SW_SPDT"
			(at 64.77 26.67 0)
		)
		(property "Footprint" "Button_Switch_SMD:SW_SPDT_PCM12"
			(at 64.77 33.02 0)
		)
		(property "Datasheet" "~"
			(at 64.77 40.64 0)
		)
		(property "Description" "Switch, single pole double throw"
			(at 64.77 33.02 0)
		)
		(pin "2")
		(pin "1")
		(pin "3")
		(instances
			(project "sos_business_card"
				(path
					(reference "SW1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 29.21 66.04 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR021"
			(at 29.21 72.39 0)
		)
		(property "Value" "GND"
			(at 29.21 71.12 0)
		)
		(property "Footprint" ""
			(at 29.21 66.04 0)
		)
		(property "Datasheet" ""
			(at 29.21 66.04 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 29.21 66.04 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR021")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 266.7 93.98 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR024"
			(at 266.7 97.79 0)
		)
		(property "Value" "VCC"
			(at 266.7 88.9 0)
		)
		(property "Footprint" ""
			(at 266.7 93.98 0)
		)
		(property "Datasheet" ""
			(at 266.7 93.98 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 266.7 93.98 0)
		)
		(pin "1")
		(instances
			(project "sos_business_card"
				(path
					(reference "#PWR024")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
)
