<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<library>
<description>SOLLEC Products</description>
<packages>
<package name="FANSTEL_FT840_DB">
</package>
</packages>
<symbols>
<symbol name="EPR_TDVBT840_DB">
<pin name="VCC" direction="pas"/>
<pin name="UART_TX" direction="pas"/>
<pin name="UART_RX" direction="pas"/>
<pin name="PO2" direction="pas"/>
<pin name="RESET" direction="pas"/>
<pin name="P26/SDA" direction="pas"/>
<pin name="P27/SCL" direction="pas"/>
<pin name="P03" direction="pas"/>
<pin name="NC@1" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC@2" direction="pas"/>
<pin name="NC@3" direction="pas"/>
<pin name="NC@4" direction="pas"/>
<pin name="NC@5" direction="pas"/>
<pin name="NC@6" direction="pas"/>
<pin name="P11/BUTTON" direction="pas"/>
<pin name="P13/LED" direction="pas"/>
<pin name="P100_SWO" direction="pas"/>
<pin name="SWCLK" direction="pas"/>
<pin name="SWDIO" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="EPR_TDVBT840_DB" prefix="MOD">
<gates>
<gate name="PART_1" symbol="EPR_TDVBT840_DB"/>
</gates>
<devices>
<device name="" package="FANSTEL_FT840_DB">
<connects>
<connect gate="PART_1" pin="VCC" pad="1"/>
<connect gate="PART_1" pin="UART_TX" pad="2"/>
<connect gate="PART_1" pin="UART_RX" pad="3"/>
<connect gate="PART_1" pin="PO2" pad="4"/>
<connect gate="PART_1" pin="RESET" pad="5"/>
<connect gate="PART_1" pin="P26/SDA" pad="6"/>
<connect gate="PART_1" pin="P27/SCL" pad="7"/>
<connect gate="PART_1" pin="P03" pad="8"/>
<connect gate="PART_1" pin="NC@1" pad="9"/>
<connect gate="PART_1" pin="GND" pad="10 21"/>
<connect gate="PART_1" pin="NC@2" pad="11"/>
<connect gate="PART_1" pin="NC@3" pad="12"/>
<connect gate="PART_1" pin="NC@4" pad="13"/>
<connect gate="PART_1" pin="NC@5" pad="14"/>
<connect gate="PART_1" pin="NC@6" pad="15"/>
<connect gate="PART_1" pin="P11/BUTTON" pad="16"/>
<connect gate="PART_1" pin="P13/LED" pad="17"/>
<connect gate="PART_1" pin="P100_SWO" pad="18"/>
<connect gate="PART_1" pin="SWCLK" pad="19"/>
<connect gate="PART_1" pin="SWDIO" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="VALUE" value="EPR_TDVBT840_DB"/>
<attribute name="MANUFACTURER" value="SOLLEC"/>
<attribute name="CODE" value="SCODE"/>
<attribute name="REF" value="EPR-TDVBT84001"/>
<attribute name="DIST_REF" value="SREF"/>
<attribute name="DREF" value="DREF"/>
<attribute name="DIST" value="DIST"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
