<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="154.305" y1="102.87" x2="14.625" y2="102.87" width="0" layer="20"/>
<wire x1="14.625" y1="102.87" x2="9.525" y2="97.77" width="0" layer="20" curve="90"/>
<wire x1="9.525" y1="97.77" x2="9.525" y2="8.89" width="0" layer="20"/>
<wire x1="9.525" y1="8.89" x2="14.605" y2="3.81" width="0" layer="20" curve="90"/>
<wire x1="14.605" y1="3.81" x2="154.305" y2="3.81" width="0" layer="20"/>
<wire x1="154.305" y1="3.81" x2="159.385" y2="8.89" width="0" layer="20" curve="90"/>
<wire x1="159.385" y1="8.89" x2="159.385" y2="97.79" width="0" layer="20"/>
<wire x1="159.385" y1="97.79" x2="154.305" y2="102.87" width="0" layer="20" curve="90"/>
<text>100n</text>
<text>100n</text>
<text>100n</text>
<text>100n</text>
<text>100n</text>
<text>100n</text>
<text>+200V</text>
<text>GND</text>
<text>(+12V) (GND)</text>
<text>+12V</text>
<text>GND</text>
<text>GND</text>
<text>Nixie power supply</text>
<text>CR2032
Backup
Battery</text>
<text>+3V</text>
<text>7805</text>
<text>Minutes</text>
<text>Hours</text>
<text>Mode</text>
<text>DS18B20</text>
<text>RTC module</text>
<text>10uF</text>
<text>10uF</text>
<text>+</text>
<text>+</text>
<text>SDA</text>
<text>SCL</text>
<text>+5V</text>
<text>GND</text>
<text>74141</text>
<text>74141</text>
<text>74141</text>
<text>74141</text>
<text>74141</text>
<text>74HC595</text>
<text>74141</text>
<text>74HC595</text>
<text>74HC595</text>
<text>ATMEGA328</text>
<text>10k</text>
<text>4k7</text>
<text>4k7</text>
<text>4k7</text>
<text>1k5</text>
<text>1k5</text>
<text>(BOBRICIUS)</text>
<text>MOSI</text>
<text>MISO</text>
<text>SCK</text>
<text>RES</text>
<text>Light</text>
<text>*Seconds*</text>
<text>*Minutes*</text>
<text>*Hours*</text>
<text>Speaker</text>
<text>+HV</text>
<text>GND</text>
<text>GND</text>
<text>+5V</text>
<text>D2</text>
<text>Micro-USB
Power only</text>
<text>USB
Power only</text>
<text>+5V</text>
<text>GND</text>
<text>4k7</text>
<text>BC547</text>
<text>ISP</text>
<hole x="119.305" y="78.6" drill="2.2"/>
<hole x="146.305" y="78.6" drill="2.2"/>
<hole x="146.305" y="99.6" drill="2.2"/>
<hole x="119.305" y="99.6" drill="2.2"/>
<text>MC34063 HV PSU V1.2.</text>
<text>MC34063 HV PSU V1.2.</text>
<text>https://www.tindie.com/stores/bobricius/</text>
<text>+</text>
<text>+</text>
<text>HV10W</text>
<text>HV10W</text>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.5">
<description>1/2W Resistor, 0.5" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="78XXL">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
<package name="POWER_JACK_PTH">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="DIL16">
<description>DIL-16</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-10UF-25V">
</package>
</packages>
</library>
<library name="ScottCustom">
<packages>
<package name="IN-14">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,6-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.6 mm, round</description>
</package>
</packages>
</library>
<library name="JVN">
<packages>
<package name="SO16W">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
wide body 7.5 mm/JEDEC MS-013AA</description>
</package>
</packages>
</library>
<library name="es">
<packages>
<package name="BATTCOM_20MM_PTH">
</package>
</packages>
</library>
<library name="microbuilder">
<packages>
<package name="MOUNTINGHOLE_3.0_PLATEDTHIN">
</package>
<package name="WS2812B">
</package>
<package name="4UCONN_20329_V2">
</package>
</packages>
</library>
<library name="rc-master-smd">
<packages>
<package name="C0603">
<description>&lt;b&gt;SMD CHIP CAP&lt;/b&gt; - 0603</description>
</package>
</packages>
</library>
<library name="switch-omron">
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="avr">
<packages>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt; 0.3 inch</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="0204/5">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 5 mm</description>
</package>
<package name="C050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3-NS">
</package>
</packages>
</library>
<library name="marks">
<packages>
<package name="HV03">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="CH_connectors">
<packages>
<package name="USB-B-PTH">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH-SIDEEZ">
</package>
<package name="BUZZER-12MM-NS">
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92-AMMO">
</package>
</packages>
</library>
<library name="transistor-npn">
<description>&lt;b&gt;NPN Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="trans">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="SOT23-BEC">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="SOD123">
<description>&lt;b&gt;SMALL OUTLINE DIODE&lt;/b&gt;</description>
</package>
<package name="SOD323-W">
<description>&lt;b&gt;SOD323 Wave soldering&lt;/b&gt; Philips SC01_Mounting_1996.pdf</description>
</package>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
<package name="INDUCTOR11X11">
</package>
<package name="C1206K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1206 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3216</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="E5-10,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 10.5 mm</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="mc34063">
<packages>
<package name="SO8">
</package>
</packages>
</library>
<library name="switch">
<packages>
<package name="RTRIM3296W">
<description>&lt;b&gt;Trimm resistor&lt;/b&gt; BOURNS&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="my-mosfet">
<packages>
<package name="TO220V-BIGHOLE-V2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="SparkFun" package="AXIAL-0.5" value="">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun" package="AXIAL-0.5" value="">
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun" package="AXIAL-0.5" value="">
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun" package="AXIAL-0.5" value="">
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun" package="AXIAL-0.5" value="">
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun" package="AXIAL-0.5" value="">
<attribute name="VALUE"/>
</element>
<element name="IC6" library="dp_devices" package="DIL16" value="IC_74141-DIP-16"/>
<element name="IC7" library="dp_devices" package="DIL16" value="IC_74141-DIP-16"/>
<element name="IC8" library="dp_devices" package="DIL16" value="IC_74141-DIP-16"/>
<element name="IC9" library="dp_devices" package="DIL16" value="IC_74141-DIP-16"/>
<element name="IC10" library="dp_devices" package="DIL16" value="IC_74141-DIP-16"/>
<element name="IC11" library="dp_devices" package="DIL16" value="IC_74141-DIP-16"/>
<element name="IC12" library="SparkFun" package="DIL16" value="74LS595N"/>
<element name="IC1" library="SparkFun" package="DIL16" value="74LS595N"/>
<element name="IC2" library="SparkFun" package="DIL16" value="74LS595N"/>
<element name="IC3" library="SparkFun" package="78XXL" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Passives" package="CPOL-RADIAL-10UF-25V" value="10uF"/>
<element name="C2" library="SparkFun-Passives" package="CPOL-RADIAL-10UF-25V" value="10uF"/>
<element name="TUBE-1" library="ScottCustom" package="IN-14" value="IN-14"/>
<element name="TUBE-2" library="ScottCustom" package="IN-14" value="IN-14"/>
<element name="TUBE-3" library="ScottCustom" package="IN-14" value="IN-14"/>
<element name="TUBE-4" library="ScottCustom" package="IN-14" value="IN-14"/>
<element name="TUBE-5" library="ScottCustom" package="IN-14" value="IN-14"/>
<element name="TUBE-6" library="ScottCustom" package="IN-14" value="IN-14"/>
<element name="H1" library="holes" package="3,6-PAD" value="MOUNT-PAD-ROUND3.6"/>
<element name="H2" library="holes" package="3,6-PAD" value="MOUNT-PAD-ROUND3.6"/>
<element name="H3" library="holes" package="3,6-PAD" value="MOUNT-PAD-ROUND3.6"/>
<element name="H4" library="holes" package="3,6-PAD" value="MOUNT-PAD-ROUND3.6"/>
<element name="IC4" library="JVN" package="SO16W" value="DS3231">
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun" package="POWER_JACK_PTH" value="POWER_JACKPTH"/>
<element name="BATTERY" library="es" package="BATTCOM_20MM_PTH" value="">
<attribute name="VALUE"/>
</element>
<element name="S4" library="switch-omron" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="VALUE"/>
</element>
<element name="S5" library="switch-omron" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="VALUE"/>
</element>
<element name="S6" library="switch-omron" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="VALUE"/>
</element>
<element name="IC5" library="avr" package="DIL28-3" value="ATMEGA328-20P"/>
<element name="LED1" library="led" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="0204/5" value="1k"/>
<element name="JP4" library="SparkFun-Connectors" package="2X3-NS" value="">
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="0204/5" value="1k"/>
<element name="R12" library="rcl" package="0204/5" value="1k"/>
<element name="R13" library="rcl" package="0204/5" value="1k"/>
<element name="LED2" library="led" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="0204/5" value="1k"/>
<element name="U$16" library="microbuilder" package="MOUNTINGHOLE_3.0_PLATEDTHIN" value="MOUNTINGHOLE3.0THIN"/>
<element name="U$17" library="microbuilder" package="MOUNTINGHOLE_3.0_PLATEDTHIN" value="MOUNTINGHOLE3.0THIN"/>
<element name="R8" library="rcl" package="0204/5" value="4k7"/>
<element name="U$20" library="marks" package="HV03" value=""/>
<element name="C6" library="rcl" package="C050-025X075" value="100n"/>
<element name="C5" library="rcl" package="C050-025X075" value="100n"/>
<element name="C7" library="rcl" package="C050-025X075" value="100n"/>
<element name="C8" library="rcl" package="C050-025X075" value="100n"/>
<element name="C9" library="rcl" package="C050-025X075" value="100n"/>
<element name="C10" library="rcl" package="C050-025X075" value="100n"/>
<element name="JP1" library="pinhead" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="microbuilder" package="WS2812B" value="WS2812B5050"/>
<element name="LED4" library="microbuilder" package="WS2812B" value="WS2812B5050"/>
<element name="LED5" library="microbuilder" package="WS2812B" value="WS2812B5050"/>
<element name="LED6" library="microbuilder" package="WS2812B" value="WS2812B5050"/>
<element name="LED7" library="microbuilder" package="WS2812B" value="WS2812B5050"/>
<element name="LED8" library="microbuilder" package="WS2812B" value="WS2812B5050"/>
<element name="X5" library="CH_connectors" package="USB-B-PTH" value="USBPTH"/>
<element name="X3" library="microbuilder" package="4UCONN_20329_V2" value="microUSB"/>
<element name="JP2" library="pinhead" package="1X05" value="">
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Electromechanical" package="TACTILE-PTH-SIDEEZ" value="BUTTON"/>
<element name="S7" library="SparkFun-Electromechanical" package="TACTILE-PTH-SIDEEZ" value="BUTTON"/>
<element name="S8" library="SparkFun-Electromechanical" package="TACTILE-PTH-SIDEEZ" value="BUTTON"/>
<element name="S2" library="switch-omron" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="VALUE"/>
</element>
<element name="S3" library="SparkFun-Electromechanical" package="TACTILE-PTH-SIDEEZ" value="BUTTON"/>
<element name="U1" library="SparkFun-Sensors" package="TO-92-AMMO" value="DS18B20">
<attribute name="STORE_ID" value="SEN-00245"/>
</element>
<element name="Q1" library="transistor-npn" package="TO92" value="2N5088"/>
<element name="R9" library="rcl" package="0204/5" value="4k7"/>
<element name="C11" library="rc-master-smd" package="C0603" value="100n"/>
<element name="C12" library="rc-master-smd" package="C0603" value="100n"/>
<element name="C13" library="rc-master-smd" package="C0603" value="100n"/>
<element name="C14" library="rc-master-smd" package="C0603" value="100n"/>
<element name="C15" library="rc-master-smd" package="C0603" value="100n"/>
<element name="C16" library="rc-master-smd" package="C0603" value="100n"/>
<element name="SG1" library="SparkFun-Electromechanical" package="BUZZER-12MM-NS" value="BUZZERNS"/>
<element name="IC13" library="mc34063" package="SO8" value="MC34063-SO">
<attribute name="VALUE"/>
</element>
<element name="R14" library="trans" package="R0603" value="12k">
<attribute name="VALUE"/>
</element>
<element name="Q2" library="trans" package="SOT23-BEC" value="PNP">
<attribute name="VALUE"/>
</element>
<element name="C3" library="trans" package="C0603" value="390pF">
<attribute name="VALUE"/>
</element>
<element name="R15" library="trans" package="R0603" value="1k0">
<attribute name="VALUE"/>
</element>
<element name="C4" library="trans" package="C0603" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VIN" library="SparkFun" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HVOUT" library="SparkFun" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="my-mosfet" package="TO220V-BIGHOLE-V2" value="">
<attribute name="VALUE"/>
</element>
<element name="R16" library="trans" package="R1206" value="0r25">
<attribute name="VALUE"/>
</element>
<element name="D1" library="trans" package="SMA-DIODE" value="DIODE-SCHOTTKYSMA"/>
<element name="D2" library="trans" package="SOD123" value="T4">
<attribute name="VALUE"/>
</element>
<element name="L1" library="trans" package="INDUCTOR11X11" value="100uH">
<attribute name="NAME"/>
</element>
<element name="R17" library="trans" package="R1206" value="1M">
<attribute name="VALUE"/>
</element>
<element name="C17" library="trans" package="C1206K" value="0u1/250V">
<attribute name="VALUE"/>
</element>
<element name="R18" library="switch" package="RTRIM3296W" value="20k">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="marks" package="HV03" value=""/>
<element name="R19" library="trans" package="R1206" value="1M">
<attribute name="VALUE"/>
</element>
<element name="R20" library="trans" package="R0603" value="50k">
<attribute name="VALUE"/>
</element>
<element name="C18" library="trans" package="C0603" value="100pF">
<attribute name="VALUE"/>
</element>
<element name="C19" library="trans" package="C0603" value="0u1">
<attribute name="VALUE"/>
</element>
<element name="D4" library="trans" package="SMA-DIODE" value="">
<attribute name="VALUE"/>
</element>
<element name="D3" library="trans" package="SOD323-W" value="T4">
<attribute name="VALUE"/>
</element>
<element name="Q4" library="trans" package="SOT23-BEC" value="PNP">
<attribute name="VALUE"/>
</element>
<element name="C20" library="trans" package="E5-10,5" value="">
<attribute name="VALUE"/>
</element>
<element name="C21" library="trans" package="C1206" value="0u1/35v">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="trans" package="C1206" value="100uF/35V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="8"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC6" pad="12"/>
<contactref element="IC9" pad="12"/>
<contactref element="IC10" pad="12"/>
<contactref element="IC7" pad="12"/>
<contactref element="IC8" pad="12"/>
<contactref element="IC11" pad="12"/>
<contactref element="IC12" pad="8"/>
<contactref element="IC12" pad="13"/>
<contactref element="IC1" pad="13"/>
<contactref element="IC2" pad="13"/>
<contactref element="IC3" pad="GND"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC2" pad="8"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="IC4" pad="13"/>
<contactref element="IC4" pad="12"/>
<contactref element="IC4" pad="11"/>
<contactref element="IC4" pad="10"/>
<contactref element="IC4" pad="9"/>
<contactref element="IC4" pad="5"/>
<contactref element="IC4" pad="6"/>
<contactref element="IC4" pad="7"/>
<contactref element="IC4" pad="8"/>
<contactref element="BATTERY" pad="-"/>
<contactref element="S4" pad="1"/>
<contactref element="S4" pad="2"/>
<contactref element="S5" pad="2"/>
<contactref element="S5" pad="1"/>
<contactref element="S6" pad="1"/>
<contactref element="S6" pad="2"/>
<contactref element="IC5" pad="22"/>
<contactref element="IC5" pad="8"/>
<contactref element="JP4" pad="6"/>
<contactref element="LED1" pad="K"/>
<contactref element="J1" pad="GNDBREAK"/>
<contactref element="J1" pad="GND"/>
<contactref element="LED2" pad="K"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="LED3" pad="3-GND"/>
<contactref element="LED4" pad="3-GND"/>
<contactref element="LED5" pad="3-GND"/>
<contactref element="LED6" pad="3-GND"/>
<contactref element="LED7" pad="3-GND"/>
<contactref element="LED8" pad="3-GND"/>
<contactref element="X3" pad="GND"/>
<contactref element="X3" pad="SPRT@4"/>
<contactref element="X3" pad="BASE@1"/>
<contactref element="X3" pad="SPRT@2"/>
<contactref element="X3" pad="SPRT@1"/>
<contactref element="X3" pad="BASE@2"/>
<contactref element="X3" pad="SPRT@3"/>
<contactref element="X5" pad="GND"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP2" pad="1"/>
<contactref element="S8" pad="2"/>
<contactref element="S7" pad="2"/>
<contactref element="S1" pad="2"/>
<contactref element="S2" pad="1"/>
<contactref element="S2" pad="2"/>
<contactref element="S3" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="Q1" pad="3"/>
<contactref element="C15" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="V+">
<contactref element="R1" pad="P$2"/>
<contactref element="R7" pad="P$2"/>
<contactref element="R3" pad="P$2"/>
<contactref element="R6" pad="P$2"/>
<contactref element="R5" pad="P$2"/>
<contactref element="R2" pad="P$2"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$71">
<contactref element="IC9" pad="6"/>
<contactref element="IC12" pad="1"/>
</signal>
<signal name="N$79">
<contactref element="IC12" pad="4"/>
<contactref element="IC6" pad="7"/>
</signal>
<signal name="N$80">
<contactref element="IC12" pad="5"/>
<contactref element="IC6" pad="6"/>
</signal>
<signal name="N$83">
<contactref element="IC12" pad="9"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="N$84">
<contactref element="IC1" pad="9"/>
<contactref element="IC2" pad="14"/>
</signal>
<signal name="VIN">
<contactref element="IC3" pad="IN"/>
<contactref element="C1" pad="1"/>
<contactref element="J1" pad="PWR"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="P$1"/>
<contactref element="TUBE-1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="R7" pad="P$1"/>
<contactref element="TUBE-2" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="P$1"/>
<contactref element="TUBE-3" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="P$1"/>
<contactref element="TUBE-4" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="R6" pad="P$1"/>
<contactref element="TUBE-5" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="R5" pad="P$1"/>
<contactref element="TUBE-6" pad="A"/>
</signal>
<signal name="VCC">
<contactref element="IC4" pad="2"/>
<contactref element="JP4" pad="2"/>
<contactref element="IC5" pad="7"/>
<contactref element="IC5" pad="20"/>
<contactref element="R11" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="IC6" pad="5"/>
<contactref element="IC7" pad="5"/>
<contactref element="IC8" pad="5"/>
<contactref element="IC11" pad="5"/>
<contactref element="IC10" pad="5"/>
<contactref element="IC9" pad="5"/>
<contactref element="IC12" pad="16"/>
<contactref element="IC1" pad="16"/>
<contactref element="IC2" pad="16"/>
<contactref element="IC12" pad="10"/>
<contactref element="IC1" pad="10"/>
<contactref element="IC2" pad="10"/>
<contactref element="IC3" pad="OUT"/>
<contactref element="C2" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="LED5" pad="1-VDD"/>
<contactref element="LED3" pad="1-VDD"/>
<contactref element="LED4" pad="1-VDD"/>
<contactref element="X3" pad="VBUS"/>
<contactref element="X5" pad="VBUS"/>
<contactref element="JP2" pad="4"/>
<contactref element="U1" pad="3"/>
<contactref element="C16" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="LED8" pad="1-VDD"/>
<contactref element="LED6" pad="1-VDD"/>
<contactref element="LED7" pad="1-VDD"/>
<contactref element="SG1" pad="-"/>
</signal>
<signal name="MISO">
<contactref element="IC5" pad="18"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="IC5" pad="19"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="RESET">
<contactref element="IC5" pad="1"/>
<contactref element="JP4" pad="5"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="IC5" pad="17"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="SDA">
<contactref element="IC4" pad="15"/>
<contactref element="IC5" pad="27"/>
<contactref element="R12" pad="1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="IC4" pad="16"/>
<contactref element="IC5" pad="28"/>
<contactref element="R13" pad="1"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="PPS">
<contactref element="IC4" pad="3"/>
</signal>
<signal name="N$102">
<contactref element="IC4" pad="14"/>
<contactref element="BATTERY" pad="+"/>
</signal>
<signal name="D7">
<contactref element="IC5" pad="13"/>
<contactref element="IC12" pad="14"/>
</signal>
<signal name="TXD">
<contactref element="IC5" pad="3"/>
</signal>
<signal name="D2">
<contactref element="IC5" pad="4"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="D3">
<contactref element="IC5" pad="5"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="D5">
<contactref element="IC5" pad="11"/>
<contactref element="IC12" pad="12"/>
<contactref element="IC1" pad="12"/>
<contactref element="IC2" pad="12"/>
</signal>
<signal name="D6">
<contactref element="IC5" pad="12"/>
<contactref element="IC12" pad="11"/>
<contactref element="IC1" pad="11"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="D4">
<contactref element="IC5" pad="6"/>
<contactref element="R8" pad="1"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="AREF_RAW">
<contactref element="IC5" pad="21"/>
</signal>
<signal name="A0">
<contactref element="IC5" pad="23"/>
<contactref element="S5" pad="3"/>
<contactref element="S7" pad="1"/>
</signal>
<signal name="A1">
<contactref element="IC5" pad="24"/>
<contactref element="S6" pad="3"/>
<contactref element="S8" pad="1"/>
</signal>
<signal name="A2">
<contactref element="IC5" pad="25"/>
<contactref element="S2" pad="3"/>
<contactref element="S3" pad="1"/>
</signal>
<signal name="A3">
<contactref element="IC5" pad="26"/>
<contactref element="LED6" pad="4-DIN"/>
</signal>
<signal name="D8">
<contactref element="IC5" pad="14"/>
<contactref element="S1" pad="1"/>
<contactref element="S4" pad="3"/>
</signal>
<signal name="D9">
<contactref element="IC5" pad="15"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="D10">
<contactref element="IC5" pad="16"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$103">
<contactref element="R10" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="RXD">
<contactref element="IC5" pad="2"/>
</signal>
<signal name="N$104">
<contactref element="IC5" pad="9"/>
</signal>
<signal name="N$105">
<contactref element="IC5" pad="10"/>
</signal>
<signal name="N$89">
<contactref element="R4" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$94">
<contactref element="LED3" pad="2-DOUT"/>
<contactref element="LED4" pad="4-DIN"/>
</signal>
<signal name="N$95">
<contactref element="LED4" pad="2-DOUT"/>
<contactref element="LED5" pad="4-DIN"/>
</signal>
<signal name="N$97">
<contactref element="LED6" pad="2-DOUT"/>
<contactref element="LED7" pad="4-DIN"/>
</signal>
<signal name="N$98">
<contactref element="LED7" pad="2-DOUT"/>
<contactref element="LED8" pad="4-DIN"/>
</signal>
<signal name="N$99">
<contactref element="LED3" pad="4-DIN"/>
<contactref element="LED8" pad="2-DOUT"/>
</signal>
<signal name="N$100">
<contactref element="Q1" pad="2"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$101">
<contactref element="Q1" pad="1"/>
<contactref element="SG1" pad="+"/>
</signal>
<signal name="N$57">
<contactref element="IC8" pad="13"/>
<contactref element="TUBE-6" pad="1"/>
</signal>
<signal name="N$58">
<contactref element="IC8" pad="14"/>
<contactref element="TUBE-6" pad="2"/>
</signal>
<signal name="N$59">
<contactref element="TUBE-6" pad="3"/>
<contactref element="IC8" pad="15"/>
</signal>
<signal name="N$60">
<contactref element="IC8" pad="16"/>
<contactref element="TUBE-6" pad="4"/>
</signal>
<signal name="N$61">
<contactref element="IC8" pad="2"/>
<contactref element="TUBE-6" pad="5"/>
</signal>
<signal name="N$62">
<contactref element="IC8" pad="1"/>
<contactref element="TUBE-6" pad="6"/>
</signal>
<signal name="N$63">
<contactref element="IC8" pad="11"/>
<contactref element="TUBE-6" pad="0"/>
</signal>
<signal name="N$64">
<contactref element="IC8" pad="10"/>
<contactref element="TUBE-6" pad="9"/>
</signal>
<signal name="N$65">
<contactref element="TUBE-6" pad="8"/>
<contactref element="IC8" pad="9"/>
</signal>
<signal name="N$66">
<contactref element="IC8" pad="8"/>
<contactref element="TUBE-6" pad="7"/>
</signal>
<signal name="N$47">
<contactref element="TUBE-1" pad="1"/>
<contactref element="IC9" pad="13"/>
</signal>
<signal name="N$48">
<contactref element="TUBE-1" pad="2"/>
<contactref element="IC9" pad="14"/>
</signal>
<signal name="N$49">
<contactref element="TUBE-1" pad="3"/>
<contactref element="IC9" pad="15"/>
</signal>
<signal name="N$50">
<contactref element="TUBE-1" pad="4"/>
<contactref element="IC9" pad="16"/>
</signal>
<signal name="N$51">
<contactref element="TUBE-1" pad="5"/>
<contactref element="IC9" pad="2"/>
</signal>
<signal name="N$52">
<contactref element="TUBE-1" pad="6"/>
<contactref element="IC9" pad="1"/>
</signal>
<signal name="N$53">
<contactref element="TUBE-1" pad="0"/>
<contactref element="IC9" pad="11"/>
</signal>
<signal name="N$54">
<contactref element="TUBE-1" pad="9"/>
<contactref element="IC9" pad="10"/>
</signal>
<signal name="N$55">
<contactref element="TUBE-1" pad="8"/>
<contactref element="IC9" pad="9"/>
</signal>
<signal name="N$56">
<contactref element="TUBE-1" pad="7"/>
<contactref element="IC9" pad="8"/>
</signal>
<signal name="N$37">
<contactref element="TUBE-2" pad="1"/>
<contactref element="IC6" pad="13"/>
</signal>
<signal name="N$38">
<contactref element="TUBE-2" pad="2"/>
<contactref element="IC6" pad="14"/>
</signal>
<signal name="N$39">
<contactref element="TUBE-2" pad="3"/>
<contactref element="IC6" pad="15"/>
</signal>
<signal name="N$40">
<contactref element="TUBE-2" pad="4"/>
<contactref element="IC6" pad="16"/>
</signal>
<signal name="N$41">
<contactref element="TUBE-2" pad="5"/>
<contactref element="IC6" pad="2"/>
</signal>
<signal name="N$42">
<contactref element="TUBE-2" pad="6"/>
<contactref element="IC6" pad="1"/>
</signal>
<signal name="N$43">
<contactref element="TUBE-2" pad="0"/>
<contactref element="IC6" pad="11"/>
</signal>
<signal name="N$44">
<contactref element="TUBE-2" pad="9"/>
<contactref element="IC6" pad="10"/>
</signal>
<signal name="N$45">
<contactref element="TUBE-2" pad="8"/>
<contactref element="IC6" pad="9"/>
</signal>
<signal name="N$46">
<contactref element="TUBE-2" pad="7"/>
<contactref element="IC6" pad="8"/>
</signal>
<signal name="N$27">
<contactref element="TUBE-3" pad="1"/>
<contactref element="IC7" pad="13"/>
</signal>
<signal name="N$28">
<contactref element="TUBE-3" pad="2"/>
<contactref element="IC7" pad="14"/>
</signal>
<signal name="N$29">
<contactref element="TUBE-3" pad="3"/>
<contactref element="IC7" pad="15"/>
</signal>
<signal name="N$30">
<contactref element="TUBE-3" pad="4"/>
<contactref element="IC7" pad="16"/>
</signal>
<signal name="N$31">
<contactref element="TUBE-3" pad="5"/>
<contactref element="IC7" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="TUBE-3" pad="6"/>
<contactref element="IC7" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="TUBE-3" pad="0"/>
<contactref element="IC7" pad="11"/>
</signal>
<signal name="N$34">
<contactref element="TUBE-3" pad="9"/>
<contactref element="IC7" pad="10"/>
</signal>
<signal name="N$35">
<contactref element="TUBE-3" pad="8"/>
<contactref element="IC7" pad="9"/>
</signal>
<signal name="N$36">
<contactref element="TUBE-3" pad="7"/>
<contactref element="IC7" pad="8"/>
</signal>
<signal name="N$17">
<contactref element="TUBE-4" pad="1"/>
<contactref element="IC10" pad="13"/>
</signal>
<signal name="N$18">
<contactref element="TUBE-4" pad="2"/>
<contactref element="IC10" pad="14"/>
</signal>
<signal name="N$19">
<contactref element="TUBE-4" pad="3"/>
<contactref element="IC10" pad="15"/>
</signal>
<signal name="N$20">
<contactref element="TUBE-4" pad="4"/>
<contactref element="IC10" pad="16"/>
</signal>
<signal name="N$21">
<contactref element="TUBE-4" pad="5"/>
<contactref element="IC10" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="TUBE-4" pad="6"/>
<contactref element="IC10" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="TUBE-4" pad="0"/>
<contactref element="IC10" pad="11"/>
</signal>
<signal name="N$24">
<contactref element="TUBE-4" pad="9"/>
<contactref element="IC10" pad="10"/>
</signal>
<signal name="N$25">
<contactref element="TUBE-4" pad="8"/>
<contactref element="IC10" pad="9"/>
</signal>
<signal name="N$26">
<contactref element="TUBE-4" pad="7"/>
<contactref element="IC10" pad="8"/>
</signal>
<signal name="N$7">
<contactref element="TUBE-5" pad="1"/>
<contactref element="IC11" pad="13"/>
</signal>
<signal name="N$8">
<contactref element="TUBE-5" pad="2"/>
<contactref element="IC11" pad="14"/>
</signal>
<signal name="N$9">
<contactref element="TUBE-5" pad="3"/>
<contactref element="IC11" pad="15"/>
</signal>
<signal name="N$10">
<contactref element="TUBE-5" pad="4"/>
<contactref element="IC11" pad="16"/>
</signal>
<signal name="N$11">
<contactref element="TUBE-5" pad="5"/>
<contactref element="IC11" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="TUBE-5" pad="6"/>
<contactref element="IC11" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="TUBE-5" pad="0"/>
<contactref element="IC11" pad="11"/>
</signal>
<signal name="N$14">
<contactref element="TUBE-5" pad="9"/>
<contactref element="IC11" pad="10"/>
</signal>
<signal name="N$15">
<contactref element="TUBE-5" pad="8"/>
<contactref element="IC11" pad="9"/>
</signal>
<signal name="N$16">
<contactref element="TUBE-5" pad="7"/>
<contactref element="IC11" pad="8"/>
</signal>
<signal name="N$72">
<contactref element="IC12" pad="3"/>
<contactref element="IC9" pad="3"/>
</signal>
<signal name="N$73">
<contactref element="IC9" pad="4"/>
<contactref element="IC12" pad="2"/>
</signal>
<signal name="N$74">
<contactref element="IC9" pad="7"/>
<contactref element="IC12" pad="15"/>
</signal>
<signal name="N$106">
<contactref element="IC12" pad="6"/>
<contactref element="IC6" pad="4"/>
</signal>
<signal name="N$108">
<contactref element="IC12" pad="7"/>
<contactref element="IC6" pad="3"/>
</signal>
<signal name="N$67">
<contactref element="IC7" pad="6"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$70">
<contactref element="IC7" pad="3"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$75">
<contactref element="IC7" pad="4"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$76">
<contactref element="IC7" pad="7"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="N$68">
<contactref element="IC10" pad="7"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="N$69">
<contactref element="IC10" pad="6"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$77">
<contactref element="IC10" pad="4"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$78">
<contactref element="IC10" pad="3"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$81">
<contactref element="IC11" pad="6"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="N$86">
<contactref element="IC11" pad="3"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="N$87">
<contactref element="IC11" pad="4"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$88">
<contactref element="IC11" pad="7"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="N$82">
<contactref element="IC2" pad="4"/>
<contactref element="IC8" pad="7"/>
</signal>
<signal name="N$85">
<contactref element="IC2" pad="5"/>
<contactref element="IC8" pad="6"/>
</signal>
<signal name="N$90">
<contactref element="IC2" pad="6"/>
<contactref element="IC8" pad="4"/>
</signal>
<signal name="N$91">
<contactref element="IC2" pad="7"/>
<contactref element="IC8" pad="3"/>
</signal>
<signal name="VCCHV">
<contactref element="VIN" pad="1"/>
<contactref element="R16" pad="2"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="GNDHW">
<contactref element="IC13" pad="4"/>
<contactref element="C3" pad="1"/>
<contactref element="Q2" pad="3"/>
<contactref element="R15" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="VIN" pad="2"/>
<contactref element="HVOUT" pad="1"/>
<contactref element="C17" pad="2"/>
<contactref element="Q3" pad="3"/>
<contactref element="C18" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="Q4" pad="3"/>
<contactref element="C20" pad="-"/>
<contactref element="C21" pad="2"/>
<contactref element="C22" pad="2"/>
</signal>
<signal name="N$92">
<contactref element="C3" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="D3" pad="C"/>
<contactref element="Q4" pad="2"/>
</signal>
<signal name="SUP">
<contactref element="IC13" pad="7"/>
<contactref element="IC13" pad="1"/>
<contactref element="L1" pad="P$2"/>
<contactref element="C21" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="IC13" pad="8"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$93">
<contactref element="IC13" pad="2"/>
<contactref element="Q2" pad="1"/>
<contactref element="R15" pad="2"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$96">
<contactref element="Q2" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="N$107">
<contactref element="HVOUT" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="C17" pad="1"/>
<contactref element="R17" pad="2"/>
<contactref element="C20" pad="+"/>
</signal>
<signal name="SW">
<contactref element="D1" pad="A"/>
<contactref element="L1" pad="P$1"/>
<contactref element="Q3" pad="2"/>
</signal>
<signal name="HVFB">
<contactref element="IC13" pad="5"/>
<contactref element="C4" pad="1"/>
<contactref element="R19" pad="2"/>
<contactref element="R20" pad="2"/>
<contactref element="R18" pad="1"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="N$109">
<contactref element="R17" pad="1"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="N$110">
<contactref element="R14" pad="2"/>
<contactref element="R20" pad="1"/>
<contactref element="R18" pad="3"/>
</signal>
<signal name="N$111">
<contactref element="IC13" pad="6"/>
<contactref element="C19" pad="2"/>
<contactref element="D4" pad="C"/>
</signal>
<signal name="N$112">
<contactref element="IC13" pad="3"/>
<contactref element="D3" pad="A"/>
<contactref element="Q4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
