<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.1.0">
<drawing>
<board>
<plain>
<wire x1="78.74" y1="2.2225" x2="78.74" y2="61.2775" width="0" layer="20"/>
<wire x1="0" y1="2.2225" x2="0" y2="61.2775" width="0" layer="20"/>
<wire x1="0" y1="2.2225" x2="2.2225" y2="0" width="0" layer="20"/>
<wire x1="0" y1="61.2775" x2="2.2225" y2="63.5" width="0" layer="20"/>
<wire x1="2.2225" y1="63.5" x2="76.5175" y2="63.5" width="0" layer="20"/>
<wire x1="76.5175" y1="63.5" x2="78.74" y2="61.2775" width="0" layer="20"/>
<wire x1="2.2225" y1="0" x2="76.5175" y2="0" width="0" layer="20"/>
<wire x1="76.5175" y1="0" x2="78.74" y2="2.2225" width="0" layer="20"/>
<text>NTSC Shield</text>
<text>Ryan Clarke
KJ6MSG</text>
<text>RAW</text>
<text>+V</text>
<text>50</text>
<text>40</text>
<text>34</text>
<text>32</text>
<text>29</text>
<text>26</text>
<text>23</text>
<text>21</text>
<text>16</text>
<text>14</text>
<text>11</text>
<text>9</text>
<text>7</text>
<text>5</text>
<text>1</text>
<text>143</text>
<text>141</text>
<text>139</text>
<text>137</text>
<text>133</text>
<text>131</text>
<text>126</text>
<text>123</text>
<text>GND</text>
<text>GND</text>
<text>51</text>
<text>41</text>
<text>35</text>
<text>33</text>
<text>30</text>
<text>27</text>
<text>24</text>
<text>22</text>
<text>17</text>
<text>15</text>
<text>12</text>
<text>10</text>
<text>8</text>
<text>6</text>
<text>2</text>
<text>144</text>
<text>142</text>
<text>140</text>
<text>138</text>
<text>134</text>
<text>132</text>
<text>127</text>
<text>124</text>
<text>GND</text>
<text>GND</text>
<text>SUS</text>
<text>58</text>
<text>67</text>
<text>75</text>
<text>79</text>
<text>81</text>
<text>83</text>
<text>85</text>
<text>88</text>
<text>93</text>
<text>95</text>
<text>98</text>
<text>100</text>
<text>102</text>
<text>105</text>
<text>112</text>
<text>115</text>
<text>117</text>
<text>119</text>
<text>121</text>
<text>TMS</text>
<text>TDI</text>
<text>RST</text>
<text>RAW</text>
<text>+V</text>
<text>DONE</text>
<text>57</text>
<text>66</text>
<text>74</text>
<text>78</text>
<text>80</text>
<text>82</text>
<text>84</text>
<text>87</text>
<text>92</text>
<text>94</text>
<text>97</text>
<text>99</text>
<text>101</text>
<text>104</text>
<text>111</text>
<text>114</text>
<text>116</text>
<text>118</text>
<text>120</text>
<text>TDO</text>
<text>TCK</text>
<text>GND</text>
<text>AREF</text>
<text>A9</text>
<text>A7</text>
<text>A5</text>
<text>A1</text>
<text>GND</text>
<text>A8</text>
<text>A6</text>
<text>A4</text>
<text>A0</text>
</plain>
<libraries>
<library name="kj6msg">
<description>&lt;b&gt;KJ6MSG Eagle Library&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Ryan Clarke&lt;br&gt;
kj6msg@arrl.net</description>
<packages>
<package name="1206">
<description>SparkFun</description>
</package>
<package name="1206-POL">
<description>SparkFun</description>
</package>
<package name="MD-40SM">
<description>&lt;b&gt;CUI, Inc. Mini-DIN Connector&lt;/b&gt;
&lt;br&gt;
Ryan Clarke, KJ6MSG</description>
</package>
<package name="RCJ-01">
<description>&lt;b&gt;CUI, Inc. RCA Jack, Right Angle&lt;/b&gt;
&lt;br&gt;
Ryan Clarke, KJ6MSG</description>
</package>
<package name="1210">
<description>SparkFun</description>
</package>
<package name="TSSOP-28">
<description>&lt;b&gt;28-pin Thin Shrink Small Outline Package&lt;/b&gt;
&lt;br&gt;
4.40mm body
&lt;br&gt;
Ryan Clarke, KJ6MSG</description>
</package>
<package name="4-SMD">
<description>&lt;b&gt;4-pin SMD, no lead&lt;/b&gt;
&lt;br&gt;
Ryan Clarke, KJ6MSG</description>
</package>
<package name="TSOP-44">
<description>&lt;b&gt;44-pin Thin Small Outline Package II&lt;/b&gt;
&lt;br&gt;
400-mil body
&lt;br&gt;
Ryan Clarke, KJ6MSG</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DUMMY">
<description>NOTHING HERE!!! For when you want a symbol with no package as an option against symbols with a package.</description>
</package>
</packages>
</library>
<library name="EmbeddedMicro-Mojo">
<packages>
<package name="MOJO_V3">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="kj6msg" package="1206" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="kj6msg" package="1206" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="kj6msg" package="1206" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="kj6msg" package="1206" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="kj6msg" package="1206" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="kj6msg" package="1206" value="27p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="kj6msg" package="1206" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="kj6msg" package="1206-POL" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="kj6msg" package="1206" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="kj6msg" package="1206-POL" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="kj6msg" package="1206" value="0.01u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FRAME1" library="SparkFun-Aesthetics" package="DUMMY" value="FRAME-LETTERNO_PACKAGE">
<attribute name="DESIGNER" value="Nobody"/>
<attribute name="VERSION" value="v01"/>
</element>
<element name="J1" library="kj6msg" package="MD-40SM" value="MD-40SM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="kj6msg" package="RCJ-01" value="RCJ-014">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="kj6msg" package="1210" value="68u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="kj6msg" package="1206" value="510">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="kj6msg" package="1206" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="kj6msg" package="1206" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="kj6msg" package="1206" value="375">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="kj6msg" package="1206" value="300">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="kj6msg" package="1206" value="375">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="kj6msg" package="1206" value="300">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="kj6msg" package="1206" value="375">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="kj6msg" package="1206" value="300">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="kj6msg" package="1206" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="kj6msg" package="1206" value="510">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="kj6msg" package="1206" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="kj6msg" package="1206" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="kj6msg" package="1206" value="510">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="kj6msg" package="1206" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="kj6msg" package="1206" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="kj6msg" package="1206" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="EmbeddedMicro-Mojo" package="MOJO_V3" value="MOJOV3"/>
<element name="U1" library="kj6msg" package="TSSOP-28" value="AD723ARU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="kj6msg" package="4-SMD" value="ASV-14.31818MHZ-EJ-T">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="kj6msg" package="TSOP-44" value="AS7C38096A-10TIN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="GND@5"/>
<contactref element="U$1" pad="GND@1"/>
<contactref element="U$1" pad="GND@2"/>
<contactref element="U$1" pad="GND@3"/>
<contactref element="U$1" pad="GND@4"/>
<contactref element="U$1" pad="GND@6"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="12"/>
<contactref element="U1" pad="14"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="J2" pad="P$1"/>
<contactref element="J2" pad="P$2"/>
<contactref element="J2" pad="P$3"/>
<contactref element="J1" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="C6" pad="-"/>
<contactref element="C8" pad="-"/>
<contactref element="U1" pad="28"/>
<contactref element="R13" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="R17" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="U3" pad="34"/>
<contactref element="C10" pad="2"/>
<contactref element="U3" pad="12"/>
<contactref element="U3" pad="8"/>
<contactref element="C11" pad="2"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="HSYNC">
<contactref element="U1" pad="15"/>
<contactref element="U$1" pad="11"/>
</signal>
<signal name="VSYNC">
<contactref element="U1" pad="16"/>
<contactref element="U$1" pad="12"/>
</signal>
<signal name="RIN">
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="GIN">
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="BIN">
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="GIN'">
<contactref element="C2" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="RIN'">
<contactref element="C1" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="BIN'">
<contactref element="R1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="B0">
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="100"/>
</signal>
<signal name="B1">
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="99"/>
</signal>
<signal name="G2">
<contactref element="R3" pad="1"/>
<contactref element="U$1" pad="95"/>
</signal>
<signal name="G1">
<contactref element="R4" pad="1"/>
<contactref element="U$1" pad="97"/>
</signal>
<signal name="G0">
<contactref element="R5" pad="1"/>
<contactref element="U$1" pad="98"/>
</signal>
<signal name="R0">
<contactref element="R8" pad="1"/>
<contactref element="U$1" pad="94"/>
</signal>
<signal name="R1">
<contactref element="R7" pad="1"/>
<contactref element="U$1" pad="93"/>
</signal>
<signal name="4FSC">
<contactref element="U1" pad="17"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="21"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="C4" pad="1"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="CVSET">
<contactref element="U1" pad="19"/>
<contactref element="R13" pad="2"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="CV">
<contactref element="U1" pad="20"/>
<contactref element="R12" pad="1"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="C">
<contactref element="U1" pad="23"/>
<contactref element="R16" pad="1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="CSET">
<contactref element="U1" pad="24"/>
<contactref element="R17" pad="1"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="Y">
<contactref element="U1" pad="26"/>
<contactref element="J1" pad="4"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="YSET">
<contactref element="U1" pad="27"/>
<contactref element="R15" pad="2"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="A5">
<contactref element="U3" pad="41"/>
<contactref element="U$1" pad="34"/>
</signal>
<signal name="A6">
<contactref element="U3" pad="40"/>
<contactref element="U$1" pad="33"/>
</signal>
<signal name="A7">
<contactref element="U3" pad="39"/>
<contactref element="U$1" pad="32"/>
</signal>
<signal name="A8">
<contactref element="U3" pad="38"/>
<contactref element="U$1" pad="30"/>
</signal>
<signal name="!OE!">
<contactref element="U3" pad="37"/>
<contactref element="U$1" pad="29"/>
</signal>
<signal name="DQ7">
<contactref element="U3" pad="36"/>
<contactref element="U$1" pad="27"/>
</signal>
<signal name="DQ6">
<contactref element="U3" pad="35"/>
<contactref element="U$1" pad="26"/>
</signal>
<signal name="DQ5">
<contactref element="U3" pad="32"/>
<contactref element="U$1" pad="24"/>
</signal>
<signal name="DQ4">
<contactref element="U3" pad="31"/>
<contactref element="U$1" pad="23"/>
</signal>
<signal name="A9">
<contactref element="U3" pad="30"/>
<contactref element="U$1" pad="22"/>
</signal>
<signal name="A10">
<contactref element="U3" pad="29"/>
<contactref element="U$1" pad="21"/>
</signal>
<signal name="A11">
<contactref element="U3" pad="28"/>
<contactref element="U$1" pad="17"/>
</signal>
<signal name="A12">
<contactref element="U3" pad="27"/>
<contactref element="U$1" pad="16"/>
</signal>
<signal name="A13">
<contactref element="U3" pad="26"/>
<contactref element="U$1" pad="15"/>
</signal>
<signal name="A14">
<contactref element="U3" pad="25"/>
<contactref element="U$1" pad="14"/>
</signal>
<signal name="A15">
<contactref element="U3" pad="20"/>
<contactref element="U$1" pad="88"/>
</signal>
<signal name="A16">
<contactref element="U3" pad="19"/>
<contactref element="U$1" pad="87"/>
</signal>
<signal name="A17">
<contactref element="U3" pad="18"/>
<contactref element="U$1" pad="85"/>
</signal>
<signal name="A18">
<contactref element="U3" pad="17"/>
<contactref element="U$1" pad="84"/>
</signal>
<signal name="A19">
<contactref element="U3" pad="16"/>
<contactref element="U$1" pad="83"/>
</signal>
<signal name="!WE!">
<contactref element="U3" pad="15"/>
<contactref element="U$1" pad="82"/>
</signal>
<signal name="DQ3">
<contactref element="U3" pad="14"/>
<contactref element="U$1" pad="81"/>
</signal>
<signal name="DQ2">
<contactref element="U3" pad="13"/>
<contactref element="U$1" pad="80"/>
</signal>
<signal name="DQ1">
<contactref element="U3" pad="10"/>
<contactref element="U$1" pad="79"/>
</signal>
<signal name="DQ0">
<contactref element="U3" pad="9"/>
<contactref element="U$1" pad="78"/>
</signal>
<signal name="A0">
<contactref element="U3" pad="7"/>
<contactref element="U$1" pad="75"/>
</signal>
<signal name="A1">
<contactref element="U3" pad="6"/>
<contactref element="U$1" pad="74"/>
</signal>
<signal name="A2">
<contactref element="U3" pad="5"/>
<contactref element="U$1" pad="67"/>
</signal>
<signal name="A3">
<contactref element="U3" pad="4"/>
<contactref element="U$1" pad="66"/>
</signal>
<signal name="A4">
<contactref element="U3" pad="3"/>
<contactref element="U$1" pad="58"/>
</signal>
<signal name="R2">
<contactref element="U$1" pad="92"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="3V3">
<contactref element="U$1" pad="V@2"/>
<contactref element="U$1" pad="V@1"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="13"/>
<contactref element="C6" pad="+"/>
<contactref element="C5" pad="1"/>
<contactref element="U1" pad="22"/>
<contactref element="U1" pad="25"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="+"/>
<contactref element="U2" pad="4"/>
<contactref element="C9" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="U3" pad="33"/>
<contactref element="C10" pad="1"/>
<contactref element="U3" pad="11"/>
<contactref element="C11" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
