<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.1">
<drawing>
<board>
<plain>
<wire x1="-2.794" y1="21.082" x2="31.75" y2="21.082" width="0.0762" layer="20"/>
<wire x1="-2.794" y1="-0.762" x2="32.004" y2="-0.762" width="0.0762" layer="20"/>
<wire x1="-2.794" y1="21.082" x2="-4.318" y2="19.558" width="0.0762" layer="20" curve="90"/>
<wire x1="-4.318" y1="19.558" x2="-4.318" y2="0.762" width="0.0762" layer="20"/>
<wire x1="-4.318" y1="0.762" x2="-2.794" y2="-0.762" width="0.0762" layer="20" curve="90"/>
<wire x1="32.004" y1="-0.762" x2="34.29" y2="1.524" width="0.0762" layer="20" curve="90"/>
<wire x1="34.29" y1="18.542" x2="31.75" y2="21.082" width="0.0762" layer="20" curve="90"/>
<text>SDA</text>
<text>SCL</text>
<text>D4</text>
<text>5V</text>
<text>0V</text>
<text>4.096 PIXELS more...</text>
<text>... that are YOURS !</text>
<wire x1="34.29" y1="18.542" x2="34.29" y2="16.51" width="0.0762" layer="20"/>
<wire x1="34.29" y1="1.524" x2="34.29" y2="4.064" width="0.0762" layer="20"/>
<wire x1="34.29" y1="4.064" x2="33.782" y2="4.572" width="0.0762" layer="20" curve="90"/>
<wire x1="33.782" y1="4.572" x2="33.528" y2="4.572" width="0.0762" layer="20"/>
<wire x1="33.528" y1="4.572" x2="33.02" y2="5.08" width="0.0762" layer="20" curve="-90"/>
<wire x1="33.02" y1="5.08" x2="33.02" y2="15.494" width="0.0762" layer="20"/>
<wire x1="33.02" y1="15.494" x2="33.528" y2="16.002" width="0.0762" layer="20" curve="-90"/>
<wire x1="33.528" y1="16.002" x2="33.782" y2="16.002" width="0.0762" layer="20"/>
<wire x1="33.782" y1="16.002" x2="34.29" y2="16.51" width="0.0762" layer="20" curve="90"/>
<text>Made for use with FP2 !</text>
<text>Made by Cherry97</text>
<text>Rev. 1.0</text>
</plain>
<libraries>
<library name="microbuilder">
<packages>
<package name="UG-2832HSWEG02_WRAPUNDER">
</package>
<package name="0805">
<description>0805 (2012 Metric)</description>
</package>
<package name="SOT23-WIDE">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="SOD-323F">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08">
<description>&lt;h3&gt;Plated Through Hole -8 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-IC-Power">
<description>&lt;h3&gt;SparkFun Power Driver and Management ICs&lt;/h3&gt;
In this library you'll find anything that has to do with power delivery, or making power supplies.
&lt;p&gt;Contents:
&lt;ul&gt;&lt;li&gt;LDOs&lt;/li&gt;
&lt;li&gt;Boost/Buck controllers&lt;/li&gt;
&lt;li&gt;Charge pump controllers&lt;/li&gt;
&lt;li&gt;Power sequencers&lt;/li&gt;
&lt;li&gt;Power switches&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LCD1" library="microbuilder" package="UG-2832HSWEG02_WRAPUNDER" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="microbuilder" package="0805" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="microbuilder" package="0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="microbuilder" package="0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="microbuilder" package="0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="microbuilder" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="microbuilder" package="0805" value="10uF">
<attribute name="NAME"/>
</element>
<element name="R3" library="microbuilder" package="0805" value="390K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="microbuilder" package="0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="microbuilder" package="0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="R8" library="microbuilder" package="0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="microbuilder" package="0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="C7" library="microbuilder" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="microbuilder" package="0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="adafruit" package="SOD-323F" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="microbuilder" package="SOT23-WIDE" value="BSS138">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="microbuilder" package="SOT23-WIDE" value="BSS138">
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-IC-Power" package="SOT223" value="AMS1117 3.3V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="VREG-08170"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VBREF">
<contactref element="LCD1" pad="6"/>
</signal>
<signal name="N$1">
<contactref element="LCD1" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="C1" pad="1"/>
<contactref element="LCD1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="LCD1" pad="3"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="C2" pad="1"/>
<contactref element="LCD1" pad="4"/>
</signal>
<signal name="GND">
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="LCD1" pad="7"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="J3" pad="5"/>
<contactref element="J3" pad="6"/>
<contactref element="J3" pad="7"/>
<contactref element="J3" pad="8"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="LCD1" pad="13"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="LCD1" pad="12"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="LCD1" pad="14"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="RES_3.3V">
<contactref element="LCD1" pad="9"/>
<contactref element="R5" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="3.3V">
<contactref element="LCD1" pad="5"/>
<contactref element="C3" pad="2"/>
<contactref element="LCD1" pad="8"/>
<contactref element="C4" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="Q1" pad="1"/>
<contactref element="Q2" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="SDA_5.0V">
<contactref element="R8" pad="1"/>
<contactref element="Q1" pad="3"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="SCL_5.0V">
<contactref element="R9" pad="1"/>
<contactref element="Q2" pad="3"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="RES_5.0V">
<contactref element="D1" pad="C"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="SDA_3.3V">
<contactref element="R4" pad="1"/>
<contactref element="LCD1" pad="11"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="SCL_3.3V">
<contactref element="R7" pad="1"/>
<contactref element="LCD1" pad="10"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="J3" pad="4"/>
<contactref element="J3" pad="3"/>
<contactref element="J3" pad="2"/>
<contactref element="J3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
