Tools Required for Constructing Boney the Skeleton Dog.

Metal cutting band saw

Drill press with ½’’ Chuck

Hand drill with ½’’ chuck

Bench vise

Heat gun

Drill bit index 1/16’’ to ½’’

Taps 3mm, 4-40, 6-32, 10-24 and Tap handle

Metal file Set

Center punch and Hammer

Utility Knife

Multi Tool Wire Stripper (Will need to cut 6/32 and 4-40 screws)

Solder Iron

Nut drivers Sets SAE and Metric or socket set

Needle nose pliers

SAE combination wrenches 1/4’’, 5/16’’, 3/8’’

Hack saw

¼’’ Rotary Die grinder and bits

Screw driver set or a good #1 and #2 Philips

Combination square

Measuring device