<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.1">
<drawing>
<board>
<plain>
<circle x="12.7" y="12.7" radius="12.7158625" width="0.0254" layer="20"/>
<text>  Designed by
Nicholas Junker</text>
</plain>
<libraries>
<library name="Atmel_By_element14_Batch_1-00">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="SOIC127P798X216-8N">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="SOT23-BEC">
<description>TO-236 ITT Intermetall</description>
</package>
</packages>
</library>
<library name="Custom">
<packages>
<package name="MIDLED">
</package>
<package name="20MM_COINCELL">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-SWITCH-SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="adafruit" package="C0805" value="0.1uF"/>
<element name="C2" library="adafruit" package="C0805" value="100uF"/>
<element name="R5" library="adafruit" package="R0805" value="100">
<attribute name="VALUE"/>
</element>
<element name="Q1" library="transistor" package="SOT23" value="2N3904">
<attribute name="VALUE"/>
</element>
<element name="Q2" library="transistor" package="SOT23" value="2N3904">
<attribute name="VALUE"/>
</element>
<element name="Q4" library="transistor" package="SOT23" value="2N3904">
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R0805" value="1.0 K">
<attribute name="VALUE"/>
</element>
<element name="U1" library="Atmel_By_element14_Batch_1-00" package="SOIC127P798X216-8N" value="ATTINY85V-10SU">
<attribute name="MPN" value="ATTINY85V-10SU"/>
<attribute name="OC_FARNELL" value="1455166"/>
<attribute name="OC_NEWARK" value="58M3799"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Atmel"/>
</element>
<element name="LED1" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="T1" library="transistor" package="SOT23-BEC" value="MMBT2907"/>
<element name="U$2" library="Custom" package="MIDLED" value="SFH4646-ZSFH4646"/>
<element name="U$3" library="Custom" package="MIDLED" value="SFH4646-ZSFH4646"/>
<element name="U$4" library="Custom" package="MIDLED" value="SFH4646-ZSFH4646"/>
<element name="Q3" library="transistor" package="SOT23" value="2N3904"/>
<element name="Q5" library="transistor" package="SOT23" value="2N3904"/>
<element name="Q6" library="transistor" package="SOT23" value="2N3904"/>
<element name="T2" library="transistor" package="SOT23-BEC" value="MMBT2907"/>
<element name="U$6" library="Custom" package="MIDLED" value="SFH4646-ZSFH4646"/>
<element name="U$7" library="Custom" package="MIDLED" value="SFH4646-ZSFH4646"/>
<element name="U$8" library="Custom" package="MIDLED" value="SFH4646-ZSFH4646"/>
<element name="S2" library="SparkFun-Electromechanical" package="TACTILE-SWITCH-SMD" value="SWITCH-MOMENTARY-2SMD">
<attribute name="PROD_ID" value="SWCH-08247"/>
</element>
<element name="U$1" library="Custom" package="20MM_COINCELL" value="712-BAT-HLD-001"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="T1" pad="E"/>
<contactref element="U$3" pad="VCC"/>
<contactref element="U$2" pad="VCC"/>
<contactref element="U$4" pad="VCC"/>
<contactref element="T2" pad="E"/>
<contactref element="U$7" pad="VCC"/>
<contactref element="U$6" pad="VCC"/>
<contactref element="U$8" pad="VCC"/>
<contactref element="U$1" pad="POS"/>
<contactref element="U$1" pad="POS_2"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="Q4" pad="2"/>
<contactref element="Q5" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q6" pad="2"/>
<contactref element="S2" pad="1"/>
<contactref element="U$1" pad="NEG"/>
</signal>
<signal name="MOSI">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="SCK">
<contactref element="R5" pad="1"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="RST">
<contactref element="U1" pad="1"/>
<contactref element="S2" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="Q1" pad="3"/>
<contactref element="U$3" pad="GND"/>
</signal>
<signal name="N$10">
<contactref element="Q1" pad="1"/>
<contactref element="Q2" pad="1"/>
<contactref element="Q4" pad="1"/>
<contactref element="T1" pad="C"/>
</signal>
<signal name="N$4">
<contactref element="Q2" pad="3"/>
<contactref element="U$2" pad="GND"/>
</signal>
<signal name="N$6">
<contactref element="Q4" pad="3"/>
<contactref element="U$4" pad="GND"/>
</signal>
<signal name="N$7">
<contactref element="Q3" pad="3"/>
<contactref element="U$7" pad="GND"/>
</signal>
<signal name="N$8">
<contactref element="Q3" pad="1"/>
<contactref element="Q5" pad="1"/>
<contactref element="Q6" pad="1"/>
<contactref element="T2" pad="C"/>
</signal>
<signal name="N$9">
<contactref element="Q5" pad="3"/>
<contactref element="U$6" pad="GND"/>
</signal>
<signal name="N$12">
<contactref element="T2" pad="B"/>
<contactref element="R1" pad="1"/>
<contactref element="T1" pad="B"/>
</signal>
<signal name="N$13">
<contactref element="Q6" pad="3"/>
<contactref element="U$8" pad="GND"/>
</signal>
<signal name="N$1">
<contactref element="R5" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
