<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="63.48" y2="0" width="0" layer="20"/>
<wire x1="63.48" y1="0" x2="63.5" y2="54.61" width="0" layer="20"/>
<wire x1="63.5" y1="54.61" x2="0" y2="54.61" width="0" layer="20"/>
<wire x1="0" y1="54.61" x2="0" y2="0" width="0" layer="20"/>
<text>IN</text>
<text>N</text>
<text>H</text>
<text>H</text>
<text>N</text>
<text>OUT</text>
<text>Geppetto Electronics
AC Safety Switch
v1.4.3</text>
<text>DANGER
High Voltage</text>
<text>+</text>
<text>G</text>
<text>G</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="PANASONIC_E">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="1210">
</package>
</packages>
</library>
<library name="SparkFun-Connectors-new">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-5MM-3">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="AXIAL-0.6">
<description>1W Resistor, 0.6" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STANDOFF-ELECTRICAL">
</package>
</packages>
</library>
<library name="triac">
<description>&lt;b&gt;Thyristors, Triacs, Trigger Diodes&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220BV">
<description>&lt;b&gt;Molded Package&lt;/b&gt;&lt;p&gt;
grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="optocoupler">
<description>&lt;b&gt;Opto Couplers&lt;/b&gt;&lt;p&gt;
Siemens, Hewlett-Packard, Texas Instuments, Sharp, Motorola&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL6-SMD">
<description>&lt;b&gt;DIL 6 SMD&lt;/b&gt;&lt;p&gt;
Source: http://www.fairchildsemi.com/pf/4N/4N35-M.html</description>
</package>
</packages>
</library>
<library name="CUI-VSK-S10">
<packages>
<package name="HP01SXX00WI">
</package>
</packages>
</library>
<library name="fuse">
<description>&lt;b&gt;Fuses and Fuse Holders&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TR5">
<description>&lt;b&gt;FUSE&lt;/b&gt;&lt;p&gt;
Wickmann</description>
</package>
</packages>
</library>
<library name="avr-7">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Version 7 - August 1, 2011.&lt;br&gt;&lt;br&gt;
Added ATmega164P/324P/644P devices for DIP and TQFP.
&lt;p&gt;
Version 4 - March 11, 2008.&lt;br&gt;&lt;br&gt;
This library now includes ONLY ATMEL AVR microcontrollers.  It is the result of merging all other available device libraries available at http://www.cadsoft.de/download as of the time it was made.  In addition to the legacy AT90* devices, it includes most ATMEGA devices including the new 48/88/168, most ATTiny devices and a set of ISP and JTAG pin headers.&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt; file at90smcu_v400.zip
&lt;li&gt;avr.lbr and atmel.lbr as provided by CadSoft
&lt;li&gt;avr-1.lbr by David Blundell
&lt;li&gt;avr-2.lbr by Boris Zalokar
&lt;li&gt;avr-3.lbr by Carson Reynolds
&lt;li&gt;attiny24_44_84.lbr by Pawel Szramowski (ATTiny24/44/84 devices)
&lt;li&gt;atmel.lbr by Bob Starr (ISP headers)
&lt;li&gt;moates_custom_parts.lbr (edge ISP)
&lt;li&gt;other misc sources
&lt;/ul&gt;
&lt;author&gt;Revised by David Blundell (blundar at gmail dot com) and others.&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added Mega162, Tiny2313 John Lussmyer (cougar at casadelgato.com)&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added XMega A1,A3,A4,D3,D4 John Lussmyer Aug 1, 2011(cougar at casadelgato.com)&lt;/author&gt;</description>
<packages>
<package name="AVR-ISP-6">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;&lt;p&gt; JTAG 6 Pin, 0.1" Straight</description>
</package>
<package name="SOT23/6">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;, 5 lead</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="1210" value=".01uF 500V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="PANASONIC_E" value="100µF">
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun-Connectors-new" package="SCREWTERMINAL-5MM-3" value="IN">
<attribute name="NAME"/>
</element>
<element name="JP2" library="SparkFun-Connectors-new" package="SCREWTERMINAL-5MM-3" value="OUT">
<attribute name="NAME"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X02" value="BUTTON">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="330Ω">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="360Ω">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="39Ω">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="150Ω">
<attribute name="NAME"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="10kΩ">
<attribute name="NAME"/>
</element>
<element name="S4" library="SparkFun-Electromechanical" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S5" library="SparkFun-Electromechanical" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S6" library="SparkFun-Electromechanical" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S7" library="SparkFun-Electromechanical" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="Q1" library="triac" package="TO220BV" value="BTA20">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="2"/>
</element>
<element name="OK1" library="optocoupler" package="DIL6-SMD" value="MOC3031S">
<attribute name="MF" value="FAIRCHILD SEMICONDUCTOR"/>
<attribute name="MPN" value="MOC3031SM"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="34C1335"/>
<attribute name="POPULARITY" value="0"/>
</element>
<element name="U1" library="CUI-VSK-S10" package="HP01SXX00WI" value="HP01SXX00WI"/>
<element name="R6" library="SparkFun-Resistors" package="AXIAL-0.6" value="91kΩ 1W">
<attribute name="NAME"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X02" value="WARN">
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="330Ω">
<attribute name="NAME"/>
</element>
<element name="F1" library="fuse" package="TR5" value="8A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="3"/>
</element>
<element name="JP5" library="avr-7" package="AVR-ISP-6" value="AVR-TPIVERT"/>
<element name="IC1" library="avr-7" package="SOT23/6" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="HOT">
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="Q1" pad="T2"/>
<contactref element="F1" pad="1"/>
<contactref element="U1" pad="AC1"/>
</signal>
<signal name="OUT">
<contactref element="R1" pad="1"/>
<contactref element="Q1" pad="T1"/>
<contactref element="C1" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="OK1" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="Q1" pad="G"/>
</signal>
<signal name="NEUT">
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="R6" pad="P$2"/>
<contactref element="U1" pad="AC2"/>
</signal>
<signal name="GND">
<contactref element="C3" pad="-"/>
<contactref element="C2" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="S4" pad="P1"/>
<contactref element="S7" pad="P1"/>
<contactref element="OK1" pad="2"/>
<contactref element="U1" pad="DC-"/>
<contactref element="JP4" pad="2"/>
<contactref element="JP5" pad="6"/>
<contactref element="IC1" pad="2"/>
<contactref element="S5" pad="P1"/>
<contactref element="S6" pad="P1"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="+5V">
<contactref element="C3" pad="+"/>
<contactref element="C2" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="U1" pad="DC+"/>
<contactref element="JP5" pad="2"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="R4" pad="2"/>
<contactref element="OK1" pad="1"/>
</signal>
<signal name="!RESET">
<contactref element="R5" pad="1"/>
<contactref element="JP5" pad="5"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="1"/>
<contactref element="OK1" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="JP4" pad="1"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="JP1" pad="1"/>
<contactref element="F1" pad="2"/>
</signal>
<signal name="B0/TPID">
<contactref element="JP5" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="B1/TPIC">
<contactref element="JP5" pad="3"/>
<contactref element="IC1" pad="3"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="B2">
<contactref element="IC1" pad="4"/>
<contactref element="R4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
