<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100.33" y2="0" width="0" layer="20"/>
<wire x1="100.33" y1="0" x2="100.33" y2="57.15" width="0" layer="20"/>
<wire x1="100.33" y1="57.15" x2="0" y2="57.15" width="0" layer="20"/>
<wire x1="0" y1="57.15" x2="0" y2="0" width="0" layer="20"/>
<text>DANGER
HIGH VOLTAGE</text>
<text>DANGER
HIGH VOLTAGE</text>
<text>Hydra HV board
v6.0.2</text>
<text>Geppetto
Electronics</text>
<text>AC IN</text>
<text>GROUND
</text>
<text>RELAY TEST</text>
<text>CONTACTOR</text>
<text>A</text>
<text>A</text>
<text>B</text>
<text>B</text>
<text>DANGER
HIGH VOLTAGE</text>
<text>H</text>
<text>N</text>
<text>GCM
OK</text>
</plain>
<libraries>
<library name="optocoupler">
<description>&lt;b&gt;Opto Couplers&lt;/b&gt;&lt;p&gt;
Siemens, Hewlett-Packard, Texas Instuments, Sharp, Motorola&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL4-SMD">
<description>&lt;b&gt;Dual  In Line SMD&lt;/b&gt; 4 pol.&lt;p&gt;
Source: LITE-ON ELECTRONICS, LTV816.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="AXIAL-0.6">
<description>1W Resistor, 0.6" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="PANASONIC_E">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="CAP-PTH-5MM">
</package>
<package name="1210">
</package>
</packages>
</library>
<library name="fuse">
<description>&lt;b&gt;Fuses and Fuse Holders&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TR5">
<description>&lt;b&gt;FUSE&lt;/b&gt;&lt;p&gt;
Wickmann</description>
</package>
</packages>
</library>
<library name="CUI-VSK-S10">
<packages>
<package name="PSK-3D">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
<package name="STANDOFF-ELECTRICAL">
</package>
</packages>
</library>
<library name="con-hirose">
<description>&lt;b&gt;Hirose Connectors&lt;/b&gt;&lt;p&gt;
www.hirose.co.jp&lt;p&gt;
Include : &lt;br&gt;
con-hirose-df12d(3.0)60dp0.5v80.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;
con-hirose.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;</description>
<packages>
<package name="FH21-10S-1DS">
<description>&lt;b&gt;FPC Connector&lt;/b&gt;&lt;p&gt;
1 MM, right angle</description>
</package>
</packages>
</library>
<library name="QD_PCB">
<packages>
<package name="QD_200">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-5MM-2">
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
</packages>
</library>
<library name="relay">
<description>&lt;b&gt;Relays&lt;/b&gt;&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;Eichhoff
&lt;li&gt;Finder
&lt;li&gt;Fujitsu
&lt;li&gt;HAMLIN
&lt;li&gt;OMRON
&lt;li&gt;Matsushita
&lt;li&gt;NAiS
&lt;li&gt;Siemens
&lt;li&gt;Schrack
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL07SMD">
<description>&lt;b&gt;DIL07&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61613_0000.pdf</description>
</package>
</packages>
</library>
<library name="74xx-little-de">
<description>&lt;b&gt;Single and Dual Gates Family, US symbols&lt;/b&gt;&lt;p&gt;
Little logic devices from Texas Instruments&lt;br&gt;
TinyLogic(R) from FAIRCHILD Semiconductor TM
&lt;p&gt;
&lt;author&gt;Created by evgeni@eniks.com&lt;/author&gt;&lt;br&gt;
&lt;author&gt;Extended by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
SOT753 - Philips Semiconductors&lt;br&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/datasheets/74HC_HCT1G66_3.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R2" library="SparkFun-Resistors" package="0805" value="220Ω">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="220Ω">
<attribute name="NAME"/>
</element>
<element name="PWR$1" library="CUI-VSK-S10" package="PSK-3D" value="PSK-S5B-5"/>
<element name="R1" library="SparkFun-Resistors" package="0805" value="330Ω">
<attribute name="NAME"/>
</element>
<element name="LED1" library="adafruit" package="CHIP-LED0805" value="PWR">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="PANASONIC_E" value="120µF">
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="1µF">
<attribute name="NAME"/>
</element>
<element name="D3" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value="P6KE6.8A">
<attribute name="NAME"/>
</element>
<element name="U$3" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value=""/>
<element name="U$6" library="SparkFun-Electromechanical" package="STAND-OFF" value=""/>
<element name="U$7" library="SparkFun-Electromechanical" package="STAND-OFF" value=""/>
<element name="F2" library="fuse" package="TR5" value="1A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="3"/>
</element>
<element name="S1" library="SparkFun-Electromechanical" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S2" library="SparkFun-Electromechanical" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="F1" library="fuse" package="TR5" value="1A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="3"/>
</element>
<element name="JP6" library="con-hirose" package="FH21-10S-1DS" value="FH21-10S-1DS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
</element>
<element name="U$14" library="QD_PCB" package="QD_200" value="QD_200"/>
<element name="JP1" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="AC IN">
<attribute name="NAME"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="CONTACTOR A">
<attribute name="NAME"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="CONTACTOR B">
<attribute name="NAME"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="RELAY TEST A">
<attribute name="NAME"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="RELAY TEST B">
<attribute name="NAME"/>
</element>
<element name="MV2" library="SparkFun-Capacitors" package="CAP-PTH-5MM" value="MOV-07D431K">
<attribute name="NAME"/>
</element>
<element name="MV1" library="SparkFun-Capacitors" package="CAP-PTH-5MM" value="MOV-07D431K">
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="10µF">
<attribute name="NAME"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="10µF">
<attribute name="NAME"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0805" value="39Ω">
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="1210" value=".01µF">
<attribute name="NAME"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0805" value="39Ω">
<attribute name="NAME"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="1210" value=".01µF">
<attribute name="NAME"/>
</element>
<element name="K1" library="relay" package="DIL07SMD" value="AQH0223A">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQH2223A"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="26K3060"/>
<attribute name="POPULARITY" value="0"/>
</element>
<element name="K2" library="relay" package="DIL07SMD" value="AQH0223A">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQH2223A"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="26K3060"/>
<attribute name="POPULARITY" value="0"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0805" value="10kΩ">
<attribute name="NAME"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0805" value="10kΩ">
<attribute name="NAME"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value="S1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value="S1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="AXIAL-0.6" value="68kΩ">
<attribute name="NAME"/>
</element>
<element name="IC4" library="linear" package="SO08" value="LM334M">
<attribute name="NAME"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0805" value="22Ω">
<attribute name="NAME"/>
</element>
<element name="OK1" library="optocoupler" package="DIL4-SMD" value="SFH6206-3">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="SSM3J332R">
<attribute name="NAME"/>
</element>
<element name="OK2" library="optocoupler" package="DIL4-SMD" value="SFH6206-3">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
</element>
<element name="OK3" library="optocoupler" package="DIL4-SMD" value="SFH6206-3">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.6" value="100kΩ">
<attribute name="NAME"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.6" value="100kΩ">
<attribute name="NAME"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="4.7kΩ">
<attribute name="NAME"/>
</element>
<element name="LED2" library="adafruit" package="CHIP-LED0805" value="GCM OK"/>
<element name="R7" library="SparkFun-Resistors" package="0805" value="330Ω">
<attribute name="NAME"/>
</element>
<element name="IC1" library="74xx-little-de" package="SOT23-5" value="SN74LVC1G17">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="1210" value="10µF">
<attribute name="NAME"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="RELAY_A">
<contactref element="R2" pad="1"/>
<contactref element="JP6" pad="9"/>
</signal>
<signal name="N$8">
<contactref element="MV1" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="K1" pad="8"/>
</signal>
<signal name="RELAY_B">
<contactref element="R3" pad="1"/>
<contactref element="JP6" pad="8"/>
</signal>
<signal name="N$12">
<contactref element="R3" pad="2"/>
<contactref element="K2" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="JP3" pad="2"/>
<contactref element="MV2" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="K2" pad="8"/>
</signal>
<signal name="N$21">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="GND">
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="-"/>
<contactref element="D3" pad="A"/>
<contactref element="PWR$1" pad="P$4"/>
<contactref element="LED1" pad="C"/>
<contactref element="S1" pad="P1"/>
<contactref element="S2" pad="P1"/>
<contactref element="JP6" pad="1"/>
<contactref element="U$14" pad="P$1"/>
<contactref element="U$14" pad="P$2"/>
<contactref element="JP6" pad="10"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="K1" pad="3"/>
<contactref element="K2" pad="3"/>
<contactref element="OK1" pad="2"/>
<contactref element="OK2" pad="3"/>
<contactref element="OK3" pad="3"/>
<contactref element="OK1" pad="3"/>
<contactref element="R7" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$20">
<contactref element="JP3" pad="1"/>
<contactref element="MV2" pad="2"/>
<contactref element="MV1" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="F1" pad="2"/>
<contactref element="PWR$1" pad="P$1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="+5V">
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="+"/>
<contactref element="D3" pad="C"/>
<contactref element="R1" pad="1"/>
<contactref element="PWR$1" pad="P$5"/>
<contactref element="R12" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="+12V">
<contactref element="JP6" pad="2"/>
</signal>
<signal name="!RL_TEST_A">
<contactref element="JP6" pad="5"/>
<contactref element="C4" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="OK2" pad="4"/>
</signal>
<signal name="!RL_TEST_B">
<contactref element="JP6" pad="4"/>
<contactref element="C5" pad="1"/>
<contactref element="R13" pad="2"/>
<contactref element="OK3" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="C6" pad="2"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="C7" pad="2"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="K1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="F2" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="K1" pad="6"/>
<contactref element="K2" pad="6"/>
<contactref element="R11" pad="1"/>
<contactref element="PWR$1" pad="P$2"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$7">
<contactref element="JP1" pad="1"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="JP1" pad="2"/>
<contactref element="F2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="R8" pad="P$2"/>
</signal>
<signal name="N$5">
<contactref element="R8" pad="P$1"/>
<contactref element="IC4" pad="4"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="IC4" pad="7"/>
<contactref element="IC4" pad="3"/>
<contactref element="IC4" pad="2"/>
<contactref element="IC4" pad="6"/>
<contactref element="R9" pad="2"/>
<contactref element="OK1" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="IC4" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="JP6" pad="3"/>
<contactref element="Q1" pad="3"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$15">
<contactref element="OK1" pad="4"/>
<contactref element="IC1" pad="2"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="JP4" pad="2"/>
<contactref element="OK2" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="JP4" pad="1"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="N$18">
<contactref element="OK2" pad="1"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="N$19">
<contactref element="JP5" pad="2"/>
<contactref element="OK3" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="JP5" pad="1"/>
<contactref element="R5" pad="P$2"/>
</signal>
<signal name="N$23">
<contactref element="OK3" pad="1"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="N$24">
<contactref element="R7" pad="2"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="N$25">
<contactref element="Q1" pad="1"/>
<contactref element="IC1" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
