<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100.33" y2="0" width="0.2032" layer="20"/>
<wire x1="100.33" y1="0" x2="100.33" y2="57.15" width="0.2032" layer="20"/>
<wire x1="100.33" y1="57.15" x2="0" y2="57.14" width="0.2032" layer="20"/>
<wire x1="0" y1="57.14" x2="0" y2="0" width="0.2032" layer="20"/>
<text>BLK</text>
<text>SW</text>
<text>GND</text>
<text>LCD
CONT</text>
<text>J1772 Hydra
EVSE v4.4.2</text>
<text>CAR B
PILOT</text>
<text>GND</text>
<text>GND</text>
<text>CAR A
PILOT</text>
<text>GF_TEST</text>
<text>1</text>
<text>i2c</text>
<text>CAR A
CT</text>
<text>CAR B
CT</text>
<text>GND</text>
<text>GFI</text>
<text>CLK_TST</text>
</plain>
<libraries>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="1210">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-5MM-2">
</package>
<package name="SCREWTERMINAL-3.5MM-3">
</package>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
<package name="1X06">
</package>
<package name="1X02">
</package>
<package name="1X03">
</package>
<package name="1X01">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STANDOFF-ELECTRICAL">
</package>
<package name="TRIM_POT_PTH">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
<package name="SJ_3_PASTE1&amp;2">
</package>
</packages>
</library>
<library name="microchip">
<description>&lt;b&gt;Microchip PIC Microcontrollers and other Devices&lt;/b&gt;&lt;p&gt;
Based on the following sources :
&lt;ul&gt;
&lt;li&gt;Microchip Data Book, 1993
&lt;li&gt;THE EMERGING WORLD STANDARD, 1995/1996
&lt;li&gt;Microchip, Technical Library CD-ROM, June 1998
&lt;li&gt;www.microchip.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SSOP28">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS</description>
</package>
</packages>
</library>
<library name="SparkFun-Displays">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of display devices- LED displays, LCD displays, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LCD-16X2">
</package>
</packages>
</library>
<library name="avr-7">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Version 7 - August 1, 2011.&lt;br&gt;&lt;br&gt;
Added ATmega164P/324P/644P devices for DIP and TQFP.
&lt;p&gt;
Version 4 - March 11, 2008.&lt;br&gt;&lt;br&gt;
This library now includes ONLY ATMEL AVR microcontrollers.  It is the result of merging all other available device libraries available at http://www.cadsoft.de/download as of the time it was made.  In addition to the legacy AT90* devices, it includes most ATMEGA devices including the new 48/88/168, most ATTiny devices and a set of ISP and JTAG pin headers.&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt; file at90smcu_v400.zip
&lt;li&gt;avr.lbr and atmel.lbr as provided by CadSoft
&lt;li&gt;avr-1.lbr by David Blundell
&lt;li&gt;avr-2.lbr by Boris Zalokar
&lt;li&gt;avr-3.lbr by Carson Reynolds
&lt;li&gt;attiny24_44_84.lbr by Pawel Szramowski (ATTiny24/44/84 devices)
&lt;li&gt;atmel.lbr by Bob Starr (ISP headers)
&lt;li&gt;moates_custom_parts.lbr (edge ISP)
&lt;li&gt;other misc sources
&lt;/ul&gt;
&lt;author&gt;Revised by David Blundell (blundar at gmail dot com) and others.&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added Mega162, Tiny2313 John Lussmyer (cougar at casadelgato.com)&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added XMega A1,A3,A4,D3,D4 John Lussmyer Aug 1, 2011(cougar at casadelgato.com)&lt;/author&gt;</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="AVR-ISP-6">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;&lt;p&gt; JTAG 6 Pin, 0.1" Straight</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-L">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOD-323">
</package>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOD123">
<description>&lt;b&gt;Diode&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="NX3225">
</package>
<package name="FIDUCIAL_1MM">
</package>
<package name="XTAL3215">
</package>
</packages>
</library>
<library name="con-hirose">
<description>&lt;b&gt;Hirose Connectors&lt;/b&gt;&lt;p&gt;
www.hirose.co.jp&lt;p&gt;
Include : &lt;br&gt;
con-hirose-df12d(3.0)60dp0.5v80.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;
con-hirose.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;</description>
<packages>
<package name="FH21-10S-1DS">
<description>&lt;b&gt;FPC Connector&lt;/b&gt;&lt;p&gt;
1 MM, right angle</description>
</package>
</packages>
</library>
<library name="inductor-bournes">
<description>&lt;b&gt;Bourns Inductors  - v1.01, 03/01/2010&lt;/b&gt;&lt;p&gt;
&lt;p&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;
USE AT YOUR OWN RISK!&lt;p&gt;
&lt;author&gt;Copyright (C) 2008, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;&lt;/author&gt;</description>
<packages>
<package name="SRR6038">
<description>&lt;B&gt;POWER INDUCTOR&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="CR1220">
<packages>
<package name="CR1220-SMD">
</package>
</packages>
</library>
<library name="microbuilder">
<description>&lt;h2&gt;&lt;b&gt;microBuilder.eu&lt;/b&gt; Eagle Footprint Library&lt;/h2&gt;

&lt;p&gt;Footprints for common components used in our projects and products.  This is the same library that we use internally, and it is regularly updated.  The newest version can always be found at &lt;b&gt;www.microBuilder.eu&lt;/b&gt;.  If you find this library useful, please feel free to purchase something from our online store. Please also note that all holes are optimised for metric drill bits!&lt;/p&gt;

&lt;h3&gt;Obligatory Warning&lt;/h3&gt;
&lt;p&gt;While it probably goes without saying, there are no guarantees that the footprints or schematic symbols in this library are flawless, and we make no promises of fitness for production, prototyping or any other purpose. These libraries are provided for information puposes only, and are used at your own discretion.  While we make every effort to produce accurate footprints, and many of the items found in this library have be proven in production, we can't make any promises of suitability for a specific purpose. If you do find any errors, though, please feel free to contact us at www.microbuilder.eu to let us know about it so that we can update the library accordingly!&lt;/p&gt;

&lt;h3&gt;License&lt;/h3&gt;
&lt;p&gt;This work is placed in the public domain, and may be freely used for commercial and non-commercial work with the following conditions:&lt;/p&gt;
&lt;p&gt;THIS SOFTWARE IS PROVIDED ''AS IS'' AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED.  IN NO EVENT SHALL THE INSTITUTE OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING,  BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
&lt;/p&gt;</description>
<packages>
<package name="PANASONIC_D">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package D&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="dcx(xxxx)u">
<packages>
<package name="SOT23-6">
</package>
</packages>
</library>
<library name="SparkFun-Connectors-new">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
</packages>
</library>
<library name="ck_custom">
<packages>
<package name="SOIC8">
<description>SOIC8 package type.</description>
</package>
</packages>
</library>
<library name="TC1044S">
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC2" library="avr-7" package="TQFP32-08" value="MEGA328PBAU">
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="22 pF">
<attribute name="NAME"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="22 pF">
<attribute name="NAME"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="JP4" library="avr-7" package="AVR-ISP-6" value="AVR_SPI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="R26" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="R33" library="SparkFun-Resistors" package="AXIAL-0.3" value="Rb">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="R30" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="R36" library="SparkFun-Resistors" package="AXIAL-0.3" value="Rb">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="1k 1%">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="1k 1%">
<attribute name="NAME"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="200k">
<attribute name="NAME"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="200k">
<attribute name="NAME"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0805" value="100k">
<attribute name="NAME"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0805" value="56k">
<attribute name="NAME"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0805" value="100k">
<attribute name="NAME"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="56k">
<attribute name="NAME"/>
</element>
<element name="D8" library="diode" package="SOD123" value="MMSZ5222B">
<attribute name="NAME"/>
</element>
<element name="D9" library="diode" package="SOD123" value="MMSZ5222B">
<attribute name="NAME"/>
</element>
<element name="D7" library="diode" package="SOD123" value="MMSZ5222B">
<attribute name="NAME"/>
</element>
<element name="D6" library="diode" package="SOD123" value="MMSZ5222B">
<attribute name="NAME"/>
</element>
<element name="JP7" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="CAR_B">
<attribute name="NAME"/>
</element>
<element name="JP8" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="CURRENT_B">
<attribute name="NAME"/>
</element>
<element name="JP6" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="CURRENT_A">
<attribute name="NAME"/>
</element>
<element name="S1" library="SparkFun-Electromechanical" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S2" library="SparkFun-Electromechanical" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S3" library="SparkFun-Electromechanical" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S4" library="SparkFun-Electromechanical" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="C14" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C15" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R31" library="SparkFun-Resistors" package="0805" value="560">
<attribute name="NAME"/>
</element>
<element name="R34" library="SparkFun-Resistors" package="0805" value="560">
<attribute name="NAME"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X06" value="FTDI">
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="CAR_A">
<attribute name="NAME"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="SJ2" library="SparkFun-Passives" package="SJ_2S-NO" value="DTR_RESET">
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value="P6KE16CA">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-08053"/>
</element>
<element name="D2" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value="P6KE16CA">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-08053"/>
</element>
<element name="C13" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C12" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="microchip" package="SSOP28" value="MCP23017SS">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="MCP23017-E/SS"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1467674"/>
<attribute name="OC_NEWARK" value="31K2960"/>
</element>
<element name="U1" library="SparkFun-Displays" package="LCD-16X2" value="LCD-16X2SILK"/>
<element name="R35" library="SparkFun-Resistors" package="0805" value="4.7k">
<attribute name="NAME"/>
</element>
<element name="R32" library="SparkFun-Resistors" package="0805" value="4.7k">
<attribute name="NAME"/>
</element>
<element name="SJ1" library="SparkFun-Passives" package="SJ_3_PASTE1&amp;2" value="BL_COM_SEL">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="U1A" library="SparkFun-Connectors" package="1X02" value="LCD_GB"/>
<element name="R38" library="SparkFun-Resistors" package="0805" value="220">
<attribute name="NAME"/>
</element>
<element name="R39" library="SparkFun-Resistors" package="0805" value="330">
<attribute name="NAME"/>
</element>
<element name="R40" library="SparkFun-Resistors" package="0805" value="220">
<attribute name="NAME"/>
</element>
<element name="R42" library="SparkFun-Electromechanical" package="TRIM_POT_PTH" value="20k">
<attribute name="NAME"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X03" value="SELECT">
<attribute name="VALUE"/>
</element>
<element name="C9" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="U$1" library="SparkFun-Aesthetics" package="OSHW-LOGO-L" value=""/>
<element name="IC1" library="linear" package="SO08" value="LM358D">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="20k">
<attribute name="NAME"/>
</element>
<element name="R22" library="SparkFun-Resistors" package="0805" value="100k">
<attribute name="NAME"/>
</element>
<element name="R23" library="SparkFun-Resistors" package="0805" value="150">
<attribute name="NAME"/>
</element>
<element name="D5" library="SparkFun-DiscreteSemi" package="SOD-323" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="R43" library="SparkFun-Resistors" package="0805" value="100k">
<attribute name="NAME"/>
</element>
<element name="C21" library="SparkFun-Capacitors" package="0805" value="0.022uF">
<attribute name="NAME"/>
</element>
<element name="R44" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="R41" library="SparkFun-Resistors" package="0805" value="330">
<attribute name="NAME"/>
</element>
<element name="D10" library="diode" package="SOD123" value="MMSZ5222B">
<attribute name="NAME"/>
</element>
<element name="D11" library="diode" package="SOD123" value="MMSZ5222B">
<attribute name="NAME"/>
</element>
<element name="JP9" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-3" value="GFI">
<attribute name="NAME"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="0805" value="330">
<attribute name="NAME"/>
</element>
<element name="IC6" library="SparkFun-FreqCtrl" package="SO08" value="PT7C4311WEX">
<attribute name="NAME"/>
</element>
<element name="C20" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="X1" library="adafruit" package="NX3225" value="16 MHz">
<attribute name="NAME"/>
</element>
<element name="D3" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value="MBRA140">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-08053"/>
</element>
<element name="C18" library="microbuilder" package="PANASONIC_D" value="47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0805" value="3k">
<attribute name="NAME"/>
</element>
<element name="L1" library="inductor-bournes" package="SRR6038" value="56uH">
<attribute name="NAME"/>
</element>
<element name="C1" library="microbuilder" package="PANASONIC_D" value="47uF">
<attribute name="NAME"/>
</element>
<element name="D4" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value="S1M">
<attribute name="NAME"/>
</element>
<element name="U$2" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="U$3" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="JP1" library="con-hirose" package="FH21-10S-1DS" value="FH21-10S-1DS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="B1" library="CR1220" package="CR1220-SMD" value="CR1220-SMD"/>
<element name="R28" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="X2" library="adafruit" package="XTAL3215" value="32.768 kHz">
<attribute name="NAME"/>
</element>
<element name="C17" library="SparkFun-Capacitors" package="0805" value="8pF">
<attribute name="NAME"/>
</element>
<element name="C19" library="SparkFun-Capacitors" package="0805" value="8pF">
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="R16" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="R17" library="SparkFun-Resistors" package="0805" value="3k">
<attribute name="NAME"/>
</element>
<element name="R18" library="SparkFun-Resistors" package="0805" value="3k">
<attribute name="NAME"/>
</element>
<element name="R19" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="R20" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="R21" library="SparkFun-Resistors" package="0805" value="3k">
<attribute name="NAME"/>
</element>
<element name="R24" library="SparkFun-Resistors" package="0805" value="3k">
<attribute name="NAME"/>
</element>
<element name="R27" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="JP10" library="SparkFun-Connectors" package="1X01" value="M01PTH"/>
<element name="R37" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="Q1" library="dcx(xxxx)u" package="SOT23-6" value="SI3552DV">
<attribute name="NAME"/>
</element>
<element name="Q2" library="dcx(xxxx)u" package="SOT23-6" value="SI3552DV">
<attribute name="NAME"/>
</element>
<element name="Q3" library="dcx(xxxx)u" package="SOT23-6" value="SI3552DV">
<attribute name="NAME"/>
</element>
<element name="Q4" library="dcx(xxxx)u" package="SOT23-6" value="SI3552DV">
<attribute name="NAME"/>
</element>
<element name="JP11" library="SparkFun-Connectors-new" package="1X04" value="i2c"/>
<element name="IC3" library="ck_custom" package="SOIC8" value="AP1509">
<attribute name="NAME"/>
</element>
<element name="C11" library="SparkFun-Capacitors" package="1210" value="10µF">
<attribute name="NAME"/>
</element>
<element name="IC5" library="TC1044S" package="SO08" value="TC1044S_OA">
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="1210" value="10µF">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="1210" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="SparkFun-Capacitors" package="0805" value="10uF">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="RELAY_A">
<contactref element="IC2" pad="12"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="RELAY_B">
<contactref element="IC2" pad="11"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="+12V">
<contactref element="C1" pad="+"/>
<contactref element="D4" pad="C"/>
<contactref element="JP1" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="Q4" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="IC3" pad="1"/>
<contactref element="IC5" pad="8"/>
<contactref element="IC5" pad="1"/>
</signal>
<signal name="GND">
<contactref element="R26" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="R30" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="JP4" pad="6"/>
<contactref element="S1" pad="P1"/>
<contactref element="S2" pad="P1"/>
<contactref element="S3" pad="P1"/>
<contactref element="S4" pad="P1"/>
<contactref element="C15" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="JP2" pad="6"/>
<contactref element="IC2" pad="5"/>
<contactref element="D2" pad="A"/>
<contactref element="D1" pad="A"/>
<contactref element="C13" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="IC4" pad="15"/>
<contactref element="IC4" pad="10"/>
<contactref element="IC4" pad="17"/>
<contactref element="IC4" pad="16"/>
<contactref element="SJ1" pad="3"/>
<contactref element="U1" pad="1"/>
<contactref element="R42" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="C9" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="R41" pad="2"/>
<contactref element="D11" pad="C"/>
<contactref element="C20" pad="2"/>
<contactref element="IC6" pad="4"/>
<contactref element="X1" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="X1" pad="4"/>
<contactref element="IC2" pad="21"/>
<contactref element="C4" pad="2"/>
<contactref element="C1" pad="-"/>
<contactref element="D4" pad="A"/>
<contactref element="D3" pad="A"/>
<contactref element="R11" pad="1"/>
<contactref element="C18" pad="-"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP1" pad="10"/>
<contactref element="B1" pad="CENTER"/>
<contactref element="C17" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="R27" pad="2"/>
<contactref element="Q3" pad="5"/>
<contactref element="Q1" pad="5"/>
<contactref element="JP11" pad="1"/>
<contactref element="IC3" pad="7"/>
<contactref element="IC3" pad="6"/>
<contactref element="IC3" pad="5"/>
<contactref element="IC3" pad="8"/>
<contactref element="IC3" pad="4"/>
<contactref element="C11" pad="2"/>
<contactref element="IC5" pad="3"/>
<contactref element="C3" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="JP5" pad="2"/>
<contactref element="JP9" pad="1"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="R13" pad="1"/>
<contactref element="JP4" pad="2"/>
<contactref element="R25" pad="1"/>
<contactref element="R29" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="IC2" pad="18"/>
<contactref element="IC2" pad="4"/>
<contactref element="JP2" pad="4"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="IC4" pad="18"/>
<contactref element="IC4" pad="9"/>
<contactref element="R35" pad="1"/>
<contactref element="R32" pad="1"/>
<contactref element="SJ1" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="R42" pad="3"/>
<contactref element="JP3" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="IC1" pad="8"/>
<contactref element="R22" pad="2"/>
<contactref element="C20" pad="1"/>
<contactref element="IC6" pad="8"/>
<contactref element="C18" pad="+"/>
<contactref element="R12" pad="1"/>
<contactref element="L1" pad="2"/>
<contactref element="JP1" pad="3"/>
<contactref element="R28" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="R37" pad="1"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="JP11" pad="2"/>
</signal>
<signal name="XTAL2">
<contactref element="IC2" pad="8"/>
<contactref element="C6" pad="1"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="XTAL1">
<contactref element="IC2" pad="7"/>
<contactref element="C5" pad="1"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="PILOT_RD_B">
<contactref element="IC2" pad="23"/>
<contactref element="R5" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="CURRENT_RD_B">
<contactref element="D6" pad="C"/>
<contactref element="R31" pad="1"/>
<contactref element="IC2" pad="19"/>
</signal>
<signal name="PILOT_RD_A">
<contactref element="R6" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="IC2" pad="24"/>
</signal>
<signal name="CURRENT_RD_A">
<contactref element="D8" pad="C"/>
<contactref element="R34" pad="1"/>
<contactref element="IC2" pad="22"/>
</signal>
<signal name="SDA">
<contactref element="IC2" pad="27"/>
<contactref element="IC4" pad="13"/>
<contactref element="R35" pad="2"/>
<contactref element="IC6" pad="5"/>
<contactref element="JP11" pad="4"/>
</signal>
<signal name="SCL">
<contactref element="IC2" pad="28"/>
<contactref element="IC4" pad="12"/>
<contactref element="R32" pad="2"/>
<contactref element="IC6" pad="6"/>
<contactref element="JP11" pad="3"/>
</signal>
<signal name="MOSI">
<contactref element="IC2" pad="15"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="IC2" pad="16"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="IC2" pad="17"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="!RESET">
<contactref element="IC2" pad="29"/>
<contactref element="R13" pad="2"/>
<contactref element="JP4" pad="5"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="PILOT_OUT_B">
<contactref element="IC2" pad="13"/>
<contactref element="R15" pad="1"/>
<contactref element="Q3" pad="1"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="PILOT_OUT_A">
<contactref element="IC2" pad="14"/>
<contactref element="R28" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="R25" pad="2"/>
<contactref element="R26" pad="2"/>
<contactref element="R33" pad="P$1"/>
<contactref element="D7" pad="C"/>
<contactref element="C8" pad="2"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="R29" pad="2"/>
<contactref element="R30" pad="2"/>
<contactref element="R36" pad="P$2"/>
<contactref element="D9" pad="C"/>
<contactref element="C10" pad="2"/>
<contactref element="JP6" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="IC2" pad="20"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="PILOT_A">
<contactref element="R4" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="PILOT_B">
<contactref element="R3" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="JP7" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="D7" pad="A"/>
<contactref element="D6" pad="A"/>
</signal>
<signal name="N$22">
<contactref element="D8" pad="A"/>
<contactref element="D9" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="R31" pad="2"/>
<contactref element="R33" pad="P$2"/>
<contactref element="JP8" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="R34" pad="2"/>
<contactref element="R36" pad="P$1"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="RXD">
<contactref element="IC2" pad="30"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="TXD">
<contactref element="IC2" pad="31"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="C7" pad="2"/>
<contactref element="SJ2" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="JP2" pad="1"/>
<contactref element="SJ2" pad="2"/>
</signal>
<signal name="SELECT">
<contactref element="IC4" pad="21"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="LCD_D7">
<contactref element="IC4" pad="2"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="LCD_D6">
<contactref element="IC4" pad="3"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="LCD_D5">
<contactref element="IC4" pad="4"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="LCD_D4">
<contactref element="IC4" pad="5"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="LCD_E">
<contactref element="IC4" pad="6"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="LCD_RW">
<contactref element="IC4" pad="7"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="LCD_RS">
<contactref element="IC4" pad="8"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="N$53">
<contactref element="U1" pad="15"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="N$56">
<contactref element="U1" pad="16"/>
<contactref element="R38" pad="1"/>
</signal>
<signal name="N$57">
<contactref element="U1A" pad="1"/>
<contactref element="R39" pad="1"/>
</signal>
<signal name="N$58">
<contactref element="U1A" pad="2"/>
<contactref element="R40" pad="1"/>
</signal>
<signal name="BLUE">
<contactref element="R40" pad="2"/>
<contactref element="IC4" pad="1"/>
</signal>
<signal name="GREEN">
<contactref element="R39" pad="2"/>
<contactref element="IC4" pad="28"/>
</signal>
<signal name="RED">
<contactref element="R38" pad="2"/>
<contactref element="IC4" pad="27"/>
</signal>
<signal name="N$32">
<contactref element="U1" pad="3"/>
<contactref element="R42" pad="2"/>
</signal>
<signal name="GROUND_FAULT">
<contactref element="IC2" pad="32"/>
<contactref element="IC1" pad="7"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="R2" pad="2"/>
<contactref element="R22" pad="1"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$35">
<contactref element="IC1" pad="1"/>
<contactref element="D5" pad="2"/>
</signal>
<signal name="N$37">
<contactref element="D5" pad="1"/>
<contactref element="R23" pad="2"/>
<contactref element="R43" pad="1"/>
<contactref element="C21" pad="2"/>
<contactref element="C16" pad="2"/>
</signal>
<signal name="N$38">
<contactref element="R23" pad="1"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$39">
<contactref element="C21" pad="1"/>
<contactref element="R43" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="R44" pad="1"/>
</signal>
<signal name="N$42">
<contactref element="D11" pad="A"/>
<contactref element="D10" pad="A"/>
</signal>
<signal name="N$7">
<contactref element="R14" pad="2"/>
<contactref element="JP9" pad="3"/>
</signal>
<signal name="GFI_TEST">
<contactref element="R14" pad="1"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="JP9" pad="2"/>
<contactref element="R44" pad="2"/>
<contactref element="R41" pad="1"/>
<contactref element="D10" pad="C"/>
</signal>
<signal name="N$9">
<contactref element="IC6" pad="2"/>
<contactref element="X2" pad="P$1"/>
<contactref element="C19" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="IC6" pad="1"/>
<contactref element="X2" pad="P$2"/>
<contactref element="C17" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="IC6" pad="3"/>
<contactref element="B1" pad="LEFT"/>
<contactref element="B1" pad="RIGHT"/>
</signal>
<signal name="N$44">
<contactref element="D3" pad="C"/>
<contactref element="L1" pad="1"/>
<contactref element="IC3" pad="2"/>
</signal>
<signal name="N$46">
<contactref element="R12" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="IC3" pad="3"/>
</signal>
<signal name="-12V">
<contactref element="R1" pad="2"/>
<contactref element="R20" pad="2"/>
<contactref element="Q4" pad="5"/>
<contactref element="Q2" pad="5"/>
<contactref element="IC5" pad="5"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="RL_TEST_A">
<contactref element="JP1" pad="5"/>
<contactref element="IC2" pad="26"/>
</signal>
<signal name="RL_TEST_B">
<contactref element="JP1" pad="4"/>
<contactref element="IC2" pad="25"/>
</signal>
<signal name="AUX_2">
<contactref element="JP1" pad="7"/>
<contactref element="IC2" pad="10"/>
</signal>
<signal name="AUX_1">
<contactref element="JP1" pad="6"/>
<contactref element="IC2" pad="9"/>
</signal>
<signal name="N$2">
<contactref element="R17" pad="1"/>
<contactref element="Q3" pad="6"/>
</signal>
<signal name="N$20">
<contactref element="R16" pad="1"/>
<contactref element="R17" pad="2"/>
<contactref element="Q4" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="R1" pad="1"/>
<contactref element="R18" pad="2"/>
<contactref element="Q4" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="R19" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="R20" pad="1"/>
<contactref element="R24" pad="1"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="IC6" pad="7"/>
<contactref element="JP10" pad="1"/>
<contactref element="R37" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="R18" pad="1"/>
<contactref element="Q3" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="Q4" pad="6"/>
<contactref element="R3" pad="1"/>
<contactref element="Q4" pad="4"/>
</signal>
<signal name="N$17">
<contactref element="Q2" pad="6"/>
<contactref element="Q2" pad="4"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R21" pad="2"/>
<contactref element="Q1" pad="6"/>
</signal>
<signal name="N$19">
<contactref element="R24" pad="2"/>
<contactref element="Q1" pad="4"/>
</signal>
<signal name="N$11">
<contactref element="C2" pad="2"/>
<contactref element="IC5" pad="4"/>
</signal>
<signal name="N$30">
<contactref element="C2" pad="1"/>
<contactref element="IC5" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
