<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="3.81" x2="0" y2="19.05" width="0.4064" layer="20"/>
<wire x1="3.81" y1="22.86" x2="49.53" y2="22.86" width="0.4064" layer="20"/>
<wire x1="53.34" y1="19.05" x2="53.34" y2="3.81" width="0.4064" layer="20"/>
<wire x1="49.53" y1="0" x2="3.81" y2="0" width="0.4064" layer="20"/>
<hole x="2.54" y="11.43" drill="3.556"/>
<hole x="50.8" y="11.43" drill="3.556"/>
<wire x1="3.81" y1="0" x2="0" y2="3.81" width="0.4064" layer="20" curve="-100"/>
<wire x1="53.34" y1="3.81" x2="49.53" y2="0" width="0.4064" layer="20" curve="-100"/>
<wire x1="49.53" y1="22.86" x2="53.34" y2="19.05" width="0.4064" layer="20" curve="-100"/>
<wire x1="0" y1="19.05" x2="3.81" y2="22.86" width="0.4064" layer="20" curve="-100"/>
<text>GPS
Antenna</text>
<text>Power</text>
<circle x="13.97" y="12.7" radius="6.096" width="0.000025" layer="20"/>
<text>Diagnostic
Port</text>
<circle x="26.67" y="6.096" radius="3.81" width="0.000025" layer="20"/>
<wire x1="37.592" y1="6.35" x2="44.958" y2="6.35" width="0.000025" layer="20"/>
<wire x1="37.592" y1="6.35" x2="37.592" y2="9.779" width="0.000025" layer="20" curve="-180"/>
<wire x1="44.958" y1="9.779" x2="44.958" y2="6.35" width="0.000025" layer="20" curve="-180"/>
<wire x1="37.592" y1="9.779" x2="44.958" y2="9.779" width="0.000025" layer="20"/>
</plain>
<libraries>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
</elements>
<signals>
<signal name="S$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
