<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="-1.27" y1="-0.635" x2="32.385" y2="-0.635" width="0" layer="20"/>
<wire x1="32.385" y1="-0.635" x2="32.385" y2="15.875" width="0" layer="20"/>
<wire x1="32.385" y1="15.875" x2="-1.27" y2="15.875" width="0" layer="20"/>
<wire x1="-1.27" y1="15.875" x2="-1.27" y2="-0.635" width="0" layer="20"/>
<text>Geppetto
Electronics</text>
<text>FTDI-be-gone
RS-C v1.0</text>
</plain>
<libraries>
<library name="maxim">
<description>&lt;b&gt;Maxim Components&lt;/b&gt;&lt;p&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="QFN32">
<description>&lt;b&gt;QFN 32&lt;/b&gt; 5 x 5 mm&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX7042.pdf</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
<library name="con-subd">
<description>&lt;b&gt;SUB-D Connectors&lt;/b&gt;&lt;p&gt;
Harting&lt;br&gt;
NorComp&lt;br&gt;
&lt;p&gt;
PREFIX :&lt;br&gt;
H = High density&lt;br&gt;
F = Female&lt;br&gt;
M = Male&lt;p&gt;
NUMBER: Number of pins&lt;p&gt;
SUFFIX :&lt;br&gt;
H = Horizontal&lt;br&gt;
V = Vertical &lt;br&gt;
P = Shield pin on housing&lt;br&gt;
B = No mounting holes&lt;br&gt;
S = Pins individually placeable (Single)&lt;br&gt;
D = Direct mounting &lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="M09D">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ftdichip">
<description>&lt;b&gt;FTDI (TM) CHIP&lt;/b&gt; Future Technology Devices International Ltd.&lt;p&gt;
http://www.ftdichip.com</description>
<packages>
<package name="QFN32">
<description>&lt;b&gt;QFN 32&lt;/b&gt;&lt;p&gt;
Source: http://www.ftdichip.com/Documents/DataSheets/DS_FT232R_v104.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="USBC">
<packages>
<package name="USB4110-GF-A">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X1" library="con-subd" package="M09D" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="CHIP-LED0805" value="TX">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="CHIP-LED0805" value="RX">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="150">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="0.33uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="0.33uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="0.33uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="0.33uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value=""/>
<element name="C9" library="SparkFun-Capacitors" package="0805" value=".01uF">
<attribute name="NAME"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="maxim" package="QFN32" value="MAX3243ECRHBR">
<attribute name="NAME"/>
</element>
<element name="IC1" library="ftdichip" package="QFN32" value="CY7C65213-32LTXI">
<attribute name="NAME"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="0805" value="4700pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="SparkFun-Passives" package="0805" value="400Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="USBC" package="USB4110-GF-A" value="USB4110-GF-A">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="5.1kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="5.1kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="X1" pad="5"/>
<contactref element="C9" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="IC2" pad="24"/>
<contactref element="C3" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="24"/>
<contactref element="IC1" pad="17"/>
<contactref element="IC1" pad="20"/>
<contactref element="R3" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="J1" pad="B1A12"/>
<contactref element="J1" pad="A1B12"/>
<contactref element="R5" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="TXD">
<contactref element="IC2" pad="12"/>
<contactref element="IC1" pad="30"/>
</signal>
<signal name="!RTS">
<contactref element="IC2" pad="11"/>
<contactref element="IC1" pad="32"/>
</signal>
<signal name="!CTS">
<contactref element="IC1" pad="8"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="!DTR">
<contactref element="IC2" pad="10"/>
<contactref element="IC1" pad="31"/>
</signal>
<signal name="!DSR">
<contactref element="IC2" pad="15"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="!DCD">
<contactref element="IC2" pad="14"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="!RI">
<contactref element="IC1" pad="3"/>
<contactref element="IC2" pad="19"/>
</signal>
<signal name="RXD">
<contactref element="IC2" pad="18"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="RS_RXD">
<contactref element="X1" pad="2"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="RS_CTS">
<contactref element="X1" pad="8"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="RS_DSR">
<contactref element="X1" pad="6"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="RS_DCD">
<contactref element="X1" pad="1"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="RS_RI">
<contactref element="X1" pad="9"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="RS_TXD">
<contactref element="X1" pad="3"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="RS_RTS">
<contactref element="X1" pad="7"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="RS_DTR">
<contactref element="X1" pad="4"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="!SLEEP">
<contactref element="IC2" pad="21"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="!TXLED">
<contactref element="LED1" pad="C"/>
<contactref element="IC1" pad="22"/>
</signal>
<signal name="!RXLED">
<contactref element="LED2" pad="C"/>
<contactref element="IC1" pad="21"/>
</signal>
<signal name="N$3">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="LED2" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="IC2" pad="26"/>
<contactref element="IC2" pad="22"/>
<contactref element="IC1" pad="19"/>
<contactref element="IC1" pad="1"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="C2" pad="1"/>
<contactref element="IC2" pad="29"/>
</signal>
<signal name="N$12">
<contactref element="C2" pad="2"/>
<contactref element="IC2" pad="30"/>
</signal>
<signal name="N$13">
<contactref element="C1" pad="1"/>
<contactref element="IC2" pad="28"/>
</signal>
<signal name="N$14">
<contactref element="C1" pad="2"/>
<contactref element="IC2" pad="23"/>
</signal>
<signal name="N$15">
<contactref element="C3" pad="2"/>
<contactref element="IC2" pad="27"/>
</signal>
<signal name="N$16">
<contactref element="C4" pad="1"/>
<contactref element="IC2" pad="31"/>
</signal>
<signal name="N$17">
<contactref element="C7" pad="2"/>
<contactref element="IC1" pad="16"/>
</signal>
<signal name="N$7">
<contactref element="R3" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="J1" pad="TAB1"/>
<contactref element="J1" pad="TAB3"/>
<contactref element="J1" pad="TAB4"/>
<contactref element="J1" pad="TAB2"/>
</signal>
<signal name="N$8">
<contactref element="J1" pad="B4A9"/>
<contactref element="J1" pad="A4B9"/>
<contactref element="C9" pad="1"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="J1" pad="A6"/>
<contactref element="J1" pad="B6"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="N$5">
<contactref element="J1" pad="B7"/>
<contactref element="J1" pad="A7"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="N$6">
<contactref element="J1" pad="A5"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="J1" pad="B5"/>
<contactref element="R4" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
